<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<hole x="56.5" y="11" drill="2"/>
<hole x="56.5" y="32" drill="2"/>
<hole x="53.5" y="24.5" drill="2"/>
<hole x="59.5" y="24.5" drill="2"/>
<text>dream | make | share | give</text>
<wire x1="67" y1="37" x2="67" y2="6" width="0.001" layer="20"/>
<wire x1="51" y1="6" x2="51" y2="37" width="0.001" layer="20"/>
<hole x="56.5" y="37.5" drill="3.2"/>
<hole x="56.5" y="6" drill="3.2"/>
<wire x1="51" y1="37" x2="54" y2="40" width="0.001" layer="20" curve="-90"/>
<wire x1="54" y1="40" x2="64" y2="40" width="0.001" layer="20"/>
<wire x1="64" y1="40" x2="67" y2="37" width="0.001" layer="20" curve="-90"/>
<wire x1="51" y1="6" x2="54" y2="3" width="0.001" layer="20" curve="90"/>
<wire x1="54" y1="3" x2="64" y2="3" width="0.001" layer="20"/>
<wire x1="64" y1="3" x2="67" y2="6" width="0.001" layer="20" curve="90"/>
<text>VCC</text>
<text>GND</text>
<text>CS</text>
<text>SCLK</text>
<text>MISO</text>
<text>SI</text>
<text>CCLK</text>
<text>designed by</text>
<text>peter jansen</text>
<text>open</text>
<text>mini</text>
<text>spectrometer</text>
<text>sept 1 2013</text>
<text>rev1</text>
</plain>
<libraries>
<library name="notes_mark5">
<packages>
<package name="TSL1401CL">
</package>
<package name="SOT-23-6L">
</package>
<package name="0603">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X07">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="notes_mark5" package="TSL1401CL" value="TSL1401CL"/>
<element name="U2" library="notes_mark5" package="SOT-23-6L" value="AD7940"/>
<element name="C1" library="notes_mark5" package="0603" value="0.022uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="notes_mark5" package="0603" value="0.022uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun-Passives" package="0805" value="100uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X07" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="SJ_2S-NO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="7"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="AOUT">
<contactref element="U1" pad="3"/>
<contactref element="U2" pad="3"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="SPI_CS_SPEC">
<contactref element="U2" pad="6"/>
<contactref element="JP1" pad="3"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="SPI_MISO">
<contactref element="U2" pad="5"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="SPI_CLK">
<contactref element="U2" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="SPEC_SI">
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="SPEC_CLK">
<contactref element="U1" pad="2"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="V_SPEC">
<contactref element="C2" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="V_SPEC1">
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="U2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
