<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<board>
<plain>
<wire x1="31.42" y1="41.9" x2="3.5850375" y2="41.9" width="0" layer="20"/>
<wire x1="3.5850375" y1="41.9" x2="0" y2="38.3149625" width="0" layer="20" curve="90"/>
<wire x1="0" y1="38.3149625" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="27.715503125" y2="1.27" width="0" layer="20"/>
<wire x1="27.715503125" y1="1.27" x2="31.42" y2="4.974496875" width="0" layer="20" curve="90"/>
<wire x1="31.42" y1="4.974496875" x2="31.42" y2="41.9" width="0" layer="20"/>
<text>gnd</text>
<text>gnd</text>
<text>gnd</text>
<text>gnd</text>
<text>gnd</text>
<text>tx</text>
<text>rx</text>
<text>CH1</text>
<text>chorus VTX timing</text>
<text>gnd</text>
<text>gnd</text>
<text>joner'17</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_PRO_MINI">
</package>
</packages>
</library>
<library name="jounin_omat">
<packages>
<package name="RX5808">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S-TRACE-PTH">
</package>
</packages>
</library>
<library name="TD-MySensors">
<packages>
<package name="HOLE_M3PAN_LOOSE">
<description>M3 Screw, Pan Head, Loose mount,
3.4 mm hole,
6 mm head,
6.9 mm keep out</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1/6W-RES">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Boards" package="ARDUINO_PRO_MINI" value="ARDUINO_PRO_MINI"/>
<element name="U$2" library="jounin_omat" package="RX5808" value="RX5808"/>
<element name="JP3" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="R1" library="SparkFun-Retired" package="SJ_2S-TRACE-PTH" value="SOLDERJUMPERTRACE-PTH"/>
<element name="R2" library="SparkFun-Retired" package="SJ_2S-TRACE-PTH" value="SOLDERJUMPERTRACE-PTH"/>
<element name="R3" library="SparkFun-Retired" package="SJ_2S-TRACE-PTH" value="SOLDERJUMPERTRACE-PTH"/>
<element name="U$3" library="TD-MySensors" package="HOLE_M3PAN_LOOSE" value=""/>
<element name="U$4" library="TD-MySensors" package="HOLE_M3PAN_LOOSE" value=""/>
<element name="R4" library="SparkFun-Passives" package="1/6W-RES" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="1/6W-RES" value="1k">
<attribute name="VALUE"/>
</element>
<element name="LIPO" library="SparkFun-Connectors" package="1X02" value="M02PTH">
<attribute name="NAME"/>
</element>
<element name="5VC" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
</elements>
<signals>
<signal name="CH1">
<contactref element="U$1" pad="13"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="CH2">
<contactref element="U$1" pad="14"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="CH3">
<contactref element="U$1" pad="15"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="BUZZ">
<contactref element="U$1" pad="12"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="RSSI">
<contactref element="U$2" pad="P4"/>
<contactref element="U$1" pad="20"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="P1"/>
<contactref element="U$2" pad="P6"/>
<contactref element="U$1" pad="23"/>
<contactref element="U$1" pad="4"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="LIPO" pad="1"/>
<contactref element="5VC" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="P5"/>
<contactref element="U$1" pad="21"/>
<contactref element="5VC" pad="2"/>
</signal>
<signal name="RAW">
<contactref element="U$1" pad="24"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="TX">
<contactref element="U$1" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="RX">
<contactref element="U$1" pad="2"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="THRU">
<contactref element="JP2" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="CH1R">
<contactref element="U$2" pad="P9"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="P8"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="P7"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
</signal>
<signal name="BATT">
<contactref element="U$1" pad="17"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="LIPO">
<contactref element="R4" pad="2"/>
<contactref element="LIPO" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
