<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="29.21" y2="0" width="0" layer="20"/>
<wire x1="29.21" y1="0" x2="29.21" y2="20.32" width="0" layer="20"/>
<wire x1="29.21" y1="20.32" x2="0" y2="20.32" width="0" layer="20"/>
<wire x1="0" y1="20.32" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>!CS</text>
<text>SO</text>
<text>!INT</text>
<text>SI</text>
<text>SCK</text>
<text>ON</text>
<text>3.3V</text>
<text>GND</text>
<text>!CS</text>
<text>SO</text>
<text>!INT</text>
<text>SI</text>
<text>SCK</text>
<text>ON</text>
<text>3.3V</text>
<text>CC3000 WiFi</text>
</plain>
<libraries>
<library name="Outbreak">
<packages>
<package name="TI-CC3000-WIFI-MODULE">
</package>
<package name="0805">
</package>
<package name="0402-MIN">
</package>
<package name="HEADER-1X08-NO-SILK">
</package>
<package name="ANTENNA-2.450GHZ-TI-AN043">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="M1" library="Outbreak" package="TI-CC3000-WIFI-MODULE" value="CC3000">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="Outbreak" package="0402-MIN" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="Outbreak" package="0402-MIN" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ANT1" library="Outbreak" package="ANTENNA-2.450GHZ-TI-AN043" value="ANTENNA-TRACE-WITH-GND-2.450GHZ-TI-AN043"/>
<element name="C2" library="Outbreak" package="0805" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Outbreak" package="HEADER-1X08-NO-SILK" value="HEADER-1X08-NO-SILK"/>
<element name="C3" library="Outbreak" package="0805" value="100nF"/>
<element name="C1" library="Outbreak" package="0805" value="2.2pF"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="M1" pad="28"/>
<contactref element="M1" pad="27"/>
</signal>
<signal name="N$2">
<contactref element="M1" pad="30"/>
<contactref element="M1" pad="29"/>
</signal>
<signal name="N$3">
<contactref element="M1" pad="5"/>
<contactref element="M1" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="M1" pad="35"/>
<contactref element="L1" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="L2" pad="1"/>
<contactref element="ANT1" pad="ANT"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="ANT1" pad="RFGND"/>
<contactref element="L1" pad="2"/>
<contactref element="L2" pad="2"/>
<contactref element="M1" pad="42"/>
<contactref element="M1" pad="41"/>
<contactref element="M1" pad="40"/>
<contactref element="M1" pad="39"/>
<contactref element="M1" pad="38"/>
<contactref element="M1" pad="37"/>
<contactref element="M1" pad="36"/>
<contactref element="M1" pad="34"/>
<contactref element="M1" pad="33"/>
<contactref element="M1" pad="32"/>
<contactref element="M1" pad="31"/>
<contactref element="M1" pad="25"/>
<contactref element="M1" pad="1"/>
<contactref element="M1" pad="43"/>
<contactref element="M1" pad="44"/>
<contactref element="M1" pad="45"/>
<contactref element="M1" pad="9"/>
<contactref element="M1" pad="10"/>
<contactref element="M1" pad="11"/>
<contactref element="M1" pad="16"/>
<contactref element="M1" pad="18"/>
<contactref element="M1" pad="20"/>
<contactref element="M1" pad="22"/>
<contactref element="M1" pad="46"/>
<contactref element="M1" pad="21"/>
<contactref element="C2" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="!SPI_CS">
<contactref element="M1" pad="12"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="!SPI_INT">
<contactref element="M1" pad="14"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="SCK">
<contactref element="M1" pad="17"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="MOSI">
<contactref element="M1" pad="15"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="MISO">
<contactref element="M1" pad="13"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="VDD">
<contactref element="M1" pad="23"/>
<contactref element="M1" pad="19"/>
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="8"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="VBAT_SW">
<contactref element="M1" pad="26"/>
<contactref element="U$1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
