<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="36.8175" y2="0" width="0" layer="20"/>
<wire x1="36.8175" y1="0" x2="36.8175" y2="54.6" width="0" layer="20"/>
<wire x1="36.8175" y1="54.6" x2="0" y2="54.6" width="0" layer="20"/>
<wire x1="0" y1="54.6" x2="0" y2="0" width="0" layer="20"/>
<text>by Mowee</text>
<text>Compact MarcDuino </text>
<text>S</text>
<text>S</text>
<text>S</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>S</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>S</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>RX</text>
<text>TX</text>
<text>5V IN</text>
<text>POWER</text>
<text>SLC</text>
<text>SDA</text>
<text>ISP</text>
<text>-</text>
<text>+</text>
<text>S</text>
<text>MASTER</text>
<text>SLAVE</text>
<text>This board runs the MarcDuino v2 firmware only. </text>
<text>Compact MarcDuino by Mowee</text>
<text>REV 1.5.2  4-5-2016</text>
<text>H</text>
<text>H</text>
<text>H</text>
<text>V</text>
<text>V</text>
<text>V</text>
<text>L</text>
<text>L</text>
<text>L</text>
<text>L</text>
<text>-</text>
<text>+</text>
<text>5V IN</text>
<text>+</text>
<text>-</text>
<text>Front</text>
<text>Rear</text>
<text>Top</text>
<text>Pwr</text>
<text>Pwr</text>
<text>Pwr</text>
<text>Pwr</text>
<text>Pwr</text>
<text>F</text>
<text>R</text>
<text>T</text>
<text>M</text>
<text>SkyJetty</text>
<text>LED2</text>
<text>LED1</text>
</plain>
<libraries>
<library name="  SparkFun">
<packages>
<package name="STAND-OFF-TIGHT">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="CAP-PTH-SMALL">
</package>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
<library name="  SkyJetty Parts">
<packages>
<package name="DIP-28">
<description>28 PIN DIP</description>
</package>
<package name="2X03-NS">
<description>6 Pin header  2x3 pins  NO SILK SCREEN</description>
</package>
<package name="RES-TH-V">
</package>
<package name="1X03">
</package>
<package name="1X02-NS">
<description>NO SILK SCREEN</description>
</package>
<package name="3MM_R">
<description>LED 3 mm, round</description>
</package>
<package name="1X04">
</package>
<package name="CPOL-RADIAL-.25&quot;">
<description>&lt;b&gt;Radial Aluminum Electrolytic&lt;/b&gt;&lt;p&gt;
.25" dia - Radial Electrolytic&lt;p&gt;
100uF 25v</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C4" library="  SparkFun" package="CAP-PTH-SMALL" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="54W8092"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="FK18X7R1H104K"/>
</element>
<element name="R2" library="  SkyJetty Parts" package="RES-TH-V" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="38K0327"/>
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="MCF 0.25W 1K"/>
</element>
<element name="R1" library="  SkyJetty Parts" package="RES-TH-V" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="38K0328"/>
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="MCF 0.25W 10K"/>
</element>
<element name="ST3" library="  SparkFun" package="STAND-OFF-TIGHT" value="STAND-OFFTIGHT">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="ST4" library="  SparkFun" package="STAND-OFF-TIGHT" value="STAND-OFFTIGHT">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q1" library="  SparkFun" package="HC49US" value="16MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="84R5809"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="9B-16.000MAAJ-B"/>
</element>
<element name="C1" library="  SparkFun" package="CAP-PTH-SMALL" value="20pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="27T6051"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="SR151A200JAR"/>
</element>
<element name="C2" library="  SparkFun" package="CAP-PTH-SMALL" value="20pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="27T6051"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="SR151A200JAR"/>
</element>
<element name="PROG1" library="  SkyJetty Parts" package="2X03-NS" value="AVR-SPI-6NS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="IC1" library="  SkyJetty Parts" package="DIP-28" value="AVR-MEGA328P-DIPDIP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="ST2" library="  SparkFun" package="STAND-OFF-TIGHT" value="STAND-OFFTIGHT">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="ST1" library="  SparkFun" package="STAND-OFF-TIGHT" value="STAND-OFFTIGHT">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="C3" library="  SparkFun" package="CAP-PTH-SMALL" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="54W8092"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="FK18X7R1H104K"/>
</element>
<element name="JP1" library="  SkyJetty Parts" package="1X02-NS" value="Power IN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP3" library="  SkyJetty Parts" package="1X03" value="1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="LED1" library="  SkyJetty Parts" package="3MM_R" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="33C1331"/>
<attribute name="MF" value="VISHAY/TELEFUNKEN"/>
<attribute name="MPN" value="TLHR5400"/>
</element>
<element name="JP2" library="  SkyJetty Parts" package="1X03" value="To Slave">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP4" library="  SkyJetty Parts" package="1X03" value="2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP5" library="  SkyJetty Parts" package="1X03" value="3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP6" library="  SkyJetty Parts" package="1X03" value="4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP7" library="  SkyJetty Parts" package="1X03" value="5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP8" library="  SkyJetty Parts" package="1X03" value="6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP9" library="  SkyJetty Parts" package="1X03" value="7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP10" library="  SkyJetty Parts" package="1X03" value="8">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP11" library="  SkyJetty Parts" package="1X03" value="9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP12" library="  SkyJetty Parts" package="1X03" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP13" library="  SkyJetty Parts" package="1X04" value="INTERCONNECT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP14" library="  SkyJetty Parts" package="1X03" value="MP3/Teeces">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP15" library="  SkyJetty Parts" package="1X03" value="RC IN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R3" library="  SkyJetty Parts" package="RES-TH-V" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="38K0363"/>
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="MCF 0.25W 330R"/>
</element>
<element name="LED2" library="  SkyJetty Parts" package="3MM_R" value="YELLOW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP16" library="  SkyJetty Parts" package="1X04" value="I2C">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP17" library="  SkyJetty Parts" package="1X04" value="I2C">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP18" library="  SkyJetty Parts" package="1X04" value="I2C">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP22" library="  SkyJetty Parts" package="1X03" value="AUX 1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP23" library="  SkyJetty Parts" package="1X03" value="AUX 2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="C5" library="  SkyJetty Parts" package="CPOL-RADIAL-.25&quot;" value="CAP_POL_100uF-16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP19" library="  SparkFun" package="SJ_2S-NO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP20" library="  SparkFun" package="SJ_2S-NO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP21" library="  SparkFun" package="SJ_2S-NO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP24" library="  SparkFun" package="SJ_2S-NO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP25" library="  SparkFun" package="SJ_2S-NO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="PROG1" pad="6"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="22"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP7" pad="1"/>
<contactref element="JP8" pad="1"/>
<contactref element="JP9" pad="1"/>
<contactref element="JP10" pad="1"/>
<contactref element="JP11" pad="1"/>
<contactref element="JP12" pad="1"/>
<contactref element="JP14" pad="1"/>
<contactref element="JP15" pad="1"/>
<contactref element="JP13" pad="1"/>
<contactref element="JP22" pad="1"/>
<contactref element="JP23" pad="1"/>
<contactref element="C5" pad="-"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="JP18" pad="2"/>
<contactref element="JP17" pad="2"/>
<contactref element="JP16" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="PROG1" pad="5"/>
</signal>
<signal name="TX">
<contactref element="IC1" pad="3"/>
<contactref element="JP13" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="PROG1" pad="2"/>
<contactref element="IC1" pad="21"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="20"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP6" pad="2"/>
<contactref element="JP7" pad="2"/>
<contactref element="JP8" pad="2"/>
<contactref element="JP9" pad="2"/>
<contactref element="JP10" pad="2"/>
<contactref element="JP11" pad="2"/>
<contactref element="JP12" pad="2"/>
<contactref element="JP13" pad="2"/>
<contactref element="C5" pad="+"/>
<contactref element="JP16" pad="1"/>
<contactref element="JP17" pad="1"/>
<contactref element="JP18" pad="1"/>
<contactref element="JP19" pad="1"/>
<contactref element="JP20" pad="1"/>
<contactref element="JP21" pad="1"/>
<contactref element="JP24" pad="1"/>
<contactref element="JP25" pad="1"/>
</signal>
<signal name="RX">
<contactref element="IC1" pad="2"/>
<contactref element="JP13" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="PC2_AUX1">
<contactref element="IC1" pad="25"/>
<contactref element="JP22" pad="3"/>
</signal>
<signal name="PC4_SDA">
<contactref element="IC1" pad="27"/>
<contactref element="JP18" pad="4"/>
<contactref element="JP16" pad="4"/>
<contactref element="JP17" pad="4"/>
</signal>
<signal name="PC5_SCL">
<contactref element="IC1" pad="28"/>
<contactref element="JP18" pad="3"/>
<contactref element="JP16" pad="3"/>
<contactref element="JP17" pad="3"/>
</signal>
<signal name="SRV2">
<contactref element="IC1" pad="5"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="SRV3">
<contactref element="IC1" pad="6"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="SRV4">
<contactref element="IC1" pad="11"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="PD7_AUX2">
<contactref element="IC1" pad="13"/>
<contactref element="JP23" pad="3"/>
</signal>
<signal name="SRV5">
<contactref element="IC1" pad="12"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="RC_IN">
<contactref element="IC1" pad="14"/>
<contactref element="JP15" pad="3"/>
</signal>
<signal name="SRV6">
<contactref element="IC1" pad="15"/>
<contactref element="JP8" pad="3"/>
</signal>
<signal name="SRV7">
<contactref element="IC1" pad="16"/>
<contactref element="JP9" pad="3"/>
</signal>
<signal name="PC0_SLVOUT">
<contactref element="IC1" pad="23"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="SRV1">
<contactref element="IC1" pad="4"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="SRV10_SCK">
<contactref element="IC1" pad="19"/>
<contactref element="PROG1" pad="3"/>
<contactref element="JP12" pad="3"/>
</signal>
<signal name="SRV8_MOSI">
<contactref element="IC1" pad="17"/>
<contactref element="PROG1" pad="4"/>
<contactref element="JP10" pad="3"/>
</signal>
<signal name="PC1_MP3">
<contactref element="IC1" pad="24"/>
<contactref element="JP14" pad="3"/>
</signal>
<signal name="SRV9_MISO">
<contactref element="IC1" pad="18"/>
<contactref element="PROG1" pad="1"/>
<contactref element="JP11" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="JP2" pad="2"/>
<contactref element="JP19" pad="2"/>
</signal>
<signal name="PC3_LED">
<contactref element="IC1" pad="26"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="JP14" pad="2"/>
<contactref element="JP20" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="JP15" pad="2"/>
<contactref element="JP21" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="JP22" pad="2"/>
<contactref element="JP24" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="JP23" pad="2"/>
<contactref element="JP25" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="LED1" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="LED2" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
