<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.0">
<drawing>
<board>
<plain>
<wire x1="36.83" y1="66.04" x2="36.83" y2="6.35" width="0" layer="20"/>
<wire x1="36.83" y1="6.35" x2="34.29" y2="3.81" width="0" layer="20" curve="-90"/>
<wire x1="34.29" y1="3.81" x2="3.81" y2="3.81" width="0" layer="20"/>
<wire x1="3.81" y1="3.81" x2="1.27" y2="6.35" width="0" layer="20" curve="-90"/>
<wire x1="1.27" y1="6.35" x2="1.27" y2="66.04" width="0" layer="20"/>
<wire x1="1.27" y1="66.04" x2="3.81" y2="68.58" width="0" layer="20" curve="-90"/>
<wire x1="3.81" y1="68.58" x2="34.29" y2="68.58" width="0" layer="20"/>
<wire x1="34.29" y1="68.58" x2="36.83" y2="66.04" width="0" layer="20" curve="-90"/>
<text>RevA</text>
<text>Berkeley 17</text>
<text>A</text>
<text>x</text>
<text>o</text>
<text>n</text>
<text>TOM:</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
<package name="MOLEX-1X3">
</package>
<package name="MOLEX-1X4">
</package>
</packages>
</library>
<library name="myParts">
<packages>
<package name="BLUEFRUIT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JOY1" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="JOY2" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="MCU" library="myParts" package="BLUEFRUIT" value="BLUEFRUIT"/>
<element name="EMG1" library="SparkFun-Connectors" package="MOLEX-1X3" value=""/>
<element name="EMG2" library="SparkFun-Connectors" package="MOLEX-1X3" value=""/>
<element name="EMG3" library="SparkFun-Connectors" package="MOLEX-1X3" value=""/>
<element name="ACCEL" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="JOY1" pad="1"/>
<contactref element="JOY2" pad="3"/>
<contactref element="MCU" pad="GND"/>
<contactref element="EMG3" pad="3"/>
<contactref element="EMG2" pad="3"/>
<contactref element="EMG1" pad="3"/>
<contactref element="ACCEL" pad="4"/>
</signal>
<signal name="X">
<contactref element="JOY1" pad="2"/>
<contactref element="MCU" pad="A3"/>
</signal>
<signal name="Y">
<contactref element="JOY2" pad="2"/>
<contactref element="MCU" pad="A5"/>
</signal>
<signal name="3V">
<contactref element="JOY2" pad="1"/>
<contactref element="JOY1" pad="3"/>
<contactref element="MCU" pad="3V"/>
<contactref element="EMG3" pad="2"/>
<contactref element="EMG2" pad="2"/>
<contactref element="EMG1" pad="2"/>
<contactref element="ACCEL" pad="3"/>
</signal>
<signal name="EMG1">
<contactref element="MCU" pad="A0"/>
<contactref element="EMG1" pad="1"/>
</signal>
<signal name="EMG2">
<contactref element="MCU" pad="A2"/>
<contactref element="EMG2" pad="1"/>
</signal>
<signal name="EMG3">
<contactref element="MCU" pad="A4"/>
<contactref element="EMG3" pad="1"/>
</signal>
<signal name="NC">
<contactref element="MCU" pad="A1"/>
</signal>
<signal name="SCL">
<contactref element="MCU" pad="SCL"/>
<contactref element="ACCEL" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="MCU" pad="SDA"/>
<contactref element="ACCEL" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
