<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="9.525" y1="38.735" x2="19.05" y2="38.735" width="0" layer="20"/>
<wire x1="19.05" y1="38.735" x2="20.32" y2="37.465" width="0" layer="20" curve="-90"/>
<wire x1="20.32" y1="37.465" x2="20.32" y2="22.225" width="0" layer="20"/>
<wire x1="20.32" y1="22.225" x2="19.05" y2="20.955" width="0" layer="20" curve="-90"/>
<wire x1="19.05" y1="20.955" x2="0" y2="20.955" width="0" layer="20"/>
<wire x1="0" y1="20.955" x2="0" y2="6.35" width="0" layer="20"/>
<wire x1="0" y1="6.35" x2="6.35" y2="0" width="0" layer="20" curve="90"/>
<wire x1="6.35" y1="0" x2="73.66" y2="0" width="0" layer="20"/>
<wire x1="73.66" y1="0" x2="86.36" y2="12.3825" width="0" layer="20" curve="90"/>
<wire x1="86.36" y1="41.91" x2="73.66" y2="54.61" width="0" layer="20" curve="90"/>
<wire x1="73.66" y1="54.61" x2="12.065" y2="54.61" width="0" layer="20"/>
<wire x1="12.065" y1="54.61" x2="9.525" y2="51.7525" width="0" layer="20" curve="90"/>
<wire x1="9.525" y1="51.7525" x2="9.525" y2="38.735" width="0" layer="20"/>
<text>uBlox Cape</text>
<text>TX/RX - UART4
PPS - P8.8
Active Antenna 3.3v
DS18B20</text>
<text>William Rea</text>
<wire x1="86.36" y1="12.3825" x2="86.36" y2="42.2275" width="0" layer="20"/>
<text>WP</text>
<text>A1</text>
<text>A0</text>
<text>www.wacan.asn.au</text>
<text>www.hewball.com.au</text>
<text>Hewball</text>
<text>P9</text>
<text>P8</text>
<text>7V-32V DC</text>
<text>+ -</text>
<text>Version 0.4</text>
</plain>
<libraries>
<library name="logic-supply">
<packages>
<package name="BB_CAPE_TOP">
<description>Use this footprint for proper assembly file generation</description>
</package>
<package name="HEADER_1X3">
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; SOIC 150 mil</description>
</package>
</packages>
</library>
<library name="ava">
<packages>
<package name="UBLOX_MAX">
<description>uBlox MAX</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_12MM_PTH">
</package>
</packages>
</library>
<library name="wrea">
<packages>
<package name="IND_BLM18_0603">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SMA_EDGELAUNCH_UFL">
</package>
<package name="1X2-3.5MM">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="PANASONIC_H13">
</package>
</packages>
</library>
<library name="1wire">
<description>&lt;h1&gt;Dallas/Maxim 1-Wire/iButton devices&lt;/h1&gt;
&lt;p&gt;Onewire is a simple, low-cost bus system working with hundreds of devices on an up to 300m long one-wire (plus GND) bus system. It is relative slow (~16kBaud) but electrically undemanding, too. The onewire is hotplug-capable, if the host software supports it. The bus can be controlled by a single &amp;mu;C port pin or by special host adapter chips, which are available for RS232, Parallel, I&lt;sup&gt;2&lt;/sup&gt;C, and USB to onewire conversion. They are available as ready-to-run host adapter devices, too.&lt;/p&gt;
&lt;p&gt;The chips on the bus can be powered through the bus line, this is called "parasite power". All neccesary circuit and capacities for parasite power are on chip. Some chips need an additional power source to provide all features.&lt;/p&gt;
&lt;p&gt;iButton is an application for onewire devices, using special packaged onewire devices as keys or for data storage. All onewire chips have a unique serial number for technical reasons, and together with the hot-plug capability this makes them useable as unique keys. In addition, many onewire chips have additional memory (EPROM, EEPROM, RAM) on the chip, which can be used to store cryptographic keys. iButtons come in various packages which are protected against corrosive agents and weather influences.&lt;/p&gt;
&lt;p&gt;Get more info at &lt;tt&gt;http://www.maxim-ic.com/1-Wire.cfm&lt;/tt&gt;&lt;/p&gt;
&lt;p&gt;Linux driver at &lt;tt&gt;http://owfs.sf.net&lt;/tt&gt;&lt;/p&gt;
&lt;h3&gt;Copyright notice:&lt;/h3&gt;
&lt;p&gt;The devices in this library are copyrighted by various authors &amp;mdash; permission to use, distribute and modify this library is given to you at the terms of the LGPL. Copyright holders are&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Jan Kandziora &amp;lt;jjj@gmx.de&amp;gt;&lt;/li&gt;
&lt;li&gt;Giovanni Varasano &amp;lt;giovanni.varasano@fastwebnet.it&amp;gt;&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;The authorship for each device is given in the device notes.&lt;/p&gt;</description>
<packages>
<package name="TO92-">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="national-semiconductor">
<description>&lt;b&gt;National Semiconductor&lt;/b&gt;&lt;p&gt;
http://www.national.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO263-5">
<description>&lt;b&gt;TO-263&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMC">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="inductor-coilcraft">
<description>&lt;b&gt;Coilcraft SMD Inductors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;br&gt;
Modified: by Eugene Sadovoi evgeni@eniks.com&lt;/author&gt;</description>
<packages>
<package name="MSS1260">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="153CLV-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
</packages>
</library>
<library name="_hhn_PtcFuses_Siba_r500">
<description>&lt;h2&gt;&lt;b&gt;SIBA PTC-Fuses Series 194600, 194700&lt;/h2&gt;
&lt;h3&gt;Packages: SMD 1812 (4.5 x 3.2)mm; 2920 (7.5 x 5.5)mm&lt;/h3&gt;

&lt;p&gt;&lt;pre&gt;

&lt;b&gt;Rev. 5.0.0&lt;/b&gt;
as of 2013-05-17, Eagle 5+&lt;/pre&gt;&lt;/p&gt;


&lt;p&gt;&lt;pre&gt;&lt;b&gt;Changelog&lt;/b&gt;
5.0.0              (initial)&lt;/pre&gt;&lt;/p&gt;

&lt;hr /&gt;

&lt;pre&gt;Author: &lt;author&gt;Dipl.-Ing. FH Rainer Bayer&lt;/author&lt;/b&gt;
Heilbronn University  HHN         &lt;a href="http://www.hs-heilbronn.de/rainer.bayer" target="_blank"&gt;http://www.hs-heilbronn.de/rainer.bayer&lt;/a&gt; &amp;middot; &lt;a href="mailto:rainer.bayer@hs-heilbronn.de" target="_blank"&gt;rainer.bayer@hs-heilbronn.de&lt;/a&gt;
Engineering office    ing-rb:     &lt;a href="http://www.ing-rb.de/" target="_blank"&gt;http://www.ing-rb.de/&lt;/a&gt;                   &amp;middot; &lt;a href="mailto:eagle@ing-rb.de" target="_blank"&gt;eagle@ing-rb.de&lt;/a&gt;
Lectureship           dozent-rb:  &lt;a href="http://www.dozent-rb.de/" target="_blank"&gt;http://www.dozent-rb.de/&lt;/a&gt;                &amp;middot; &lt;a href="mailto:eagle@dozent-rb.de" target="_blank"&gt;eagle@dozent-rb.de&lt;/a&gt;&lt;/pre&gt;&lt;/author&gt;&lt;/pre&gt;</description>
<packages>
<package name="2920">
<description>&lt;p&gt;SIBA &lt;b&gt;2920&lt;/b&gt; (7.5 x 5.5)mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Jumper Solder">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BB1" library="logic-supply" package="BB_CAPE_TOP" value="BBH2"/>
<element name="IC1" library="logic-supply" package="SO08" value="24LC256">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun" package="0603-RES" value="5.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun" package="0603-RES" value="5.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun" package="0603-RES" value="5.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="0603-RES" value="5.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="0603-RES" value="5.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="0603-RES" value="5.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="WP" library="Jumper Solder" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="U$1" library="ava" package="UBLOX_MAX" value="UBLOX_MAX">
<attribute name="MPN" value="MAX-7Q"/>
</element>
<element name="L2" library="wrea" package="IND_BLM18_0603" value="">
<attribute name="MPN" value="BLM18HG102SN1D"/>
<attribute name="VENDOR" value="MURATA"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="BLM18HG102SN1D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="wrea" package="IND_BLM18_0603" value="">
<attribute name="MPN" value="BLM18HG102SN1D"/>
<attribute name="VENDOR" value="MURATA"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="BLM18HG102SN1D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="adafruit" package="SMA_EDGELAUNCH_UFL" value=""/>
<element name="R7" library="SparkFun-Resistors" package="0603-RES" value="22">
<attribute name="MPN" value="RMCF0805JT22R0"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun-Passives" package="0603" value="">
<attribute name="MPN" value="LBR2012T220K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BAT1" library="SparkFun-Electromechanical" package="BATTCON_12MM_PTH" value="">
<attribute name="MPN" value="BK-890"/>
</element>
<element name="DS18B20" library="1wire" package="TO92-" value="DS18B20">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J13" library="logic-supply" package="HEADER_1X3" value=""/>
<element name="WP1" library="Jumper Solder" package="SJ" value=""/>
<element name="WP2" library="Jumper Solder" package="SJ" value=""/>
<element name="FIXED5V" library="national-semiconductor" package="TO263-5" value="LM2596SX-5.0">
<attribute name="OC_NEWARK" value="41K3842"/>
<attribute name="MPN" value="LM2596S-ADJ/NOPB"/>
<attribute name="MF" value="NATIONAL SEMICONDUCTOR"/>
<attribute name="OC_FARNELL" value="9494367"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D13" library="diode" package="SMC" value="SS34">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="inductor-coilcraft" package="MSS1260" value="33uH">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="PANASONIC_H13" value="680uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="153CLV-0810" value="220uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F2" library="_hhn_PtcFuses_Siba_r500" package="2920" value="PTC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM"/>
<element name="D1" library="diode" package="SMC" value="SS34">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="SCL">
<contactref element="IC1" pad="6"/>
<contactref element="R5" pad="1"/>
<contactref element="BB1" pad="P9.19"/>
</signal>
<signal name="N$63">
<contactref element="L2" pad="1"/>
<contactref element="BB1" pad="P9.13"/>
</signal>
<signal name="N$64">
<contactref element="L4" pad="1"/>
<contactref element="BB1" pad="P9.11"/>
</signal>
<signal name="3.3V">
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U$1" pad="9_V_RESET"/>
<contactref element="U$1" pad="8_VCC"/>
<contactref element="U$1" pad="7_VCC_IO"/>
<contactref element="DS18B20" pad="3"/>
<contactref element="R8" pad="2"/>
<contactref element="J13" pad="3"/>
<contactref element="BB1" pad="P9.3"/>
<contactref element="BB1" pad="P9.4"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="WP" pad="2"/>
<contactref element="U$1" pad="1_GND"/>
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="10_GND"/>
<contactref element="U$1" pad="12_GND"/>
<contactref element="X1" pad="GND@2"/>
<contactref element="X1" pad="GND@1"/>
<contactref element="X1" pad="GND@4"/>
<contactref element="X1" pad="GND@3"/>
<contactref element="BAT1" pad="GND"/>
<contactref element="DS18B20" pad="1"/>
<contactref element="J13" pad="1"/>
<contactref element="WP1" pad="1"/>
<contactref element="WP2" pad="1"/>
<contactref element="BB1" pad="P9.1"/>
<contactref element="BB1" pad="P9.2"/>
<contactref element="BB1" pad="P8.2"/>
<contactref element="BB1" pad="P8.1"/>
<contactref element="FIXED5V" pad="3"/>
<contactref element="FIXED5V" pad="5"/>
<contactref element="D13" pad="A"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="-"/>
<contactref element="C5" pad="-"/>
<contactref element="J1" pad="2"/>
<contactref element="BB1" pad="P9.45"/>
<contactref element="BB1" pad="P9.43"/>
<contactref element="BB1" pad="P9.46"/>
<contactref element="BB1" pad="P9.44"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="5"/>
<contactref element="R6" pad="1"/>
<contactref element="BB1" pad="P9.20"/>
</signal>
<signal name="N$80">
<contactref element="DS18B20" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="J13" pad="2"/>
<contactref element="BB1" pad="P9.22"/>
</signal>
<signal name="N$68">
</signal>
<signal name="N$69">
</signal>
<signal name="N$70">
</signal>
<signal name="N$136">
</signal>
<signal name="N$137">
</signal>
<signal name="N$138">
</signal>
<signal name="N$139">
</signal>
<signal name="N$140">
</signal>
<signal name="N$262">
</signal>
<signal name="N$263">
</signal>
<signal name="N$264">
</signal>
<signal name="N$265">
</signal>
<signal name="N$266">
</signal>
<signal name="N$269">
</signal>
<signal name="N$270">
</signal>
<signal name="N$271">
</signal>
<signal name="N$272">
</signal>
<signal name="N$273">
</signal>
<signal name="N$274">
</signal>
<signal name="N$275">
</signal>
<signal name="N$276">
</signal>
<signal name="N$277">
</signal>
<signal name="N$281">
</signal>
<signal name="N$282">
</signal>
<signal name="N$283">
</signal>
<signal name="N$284">
</signal>
<signal name="N$285">
</signal>
<signal name="N$286">
</signal>
<signal name="N$287">
</signal>
<signal name="N$288">
</signal>
<signal name="N$289">
</signal>
<signal name="N$290">
</signal>
<signal name="N$291">
</signal>
<signal name="N$293">
</signal>
<signal name="N$294">
</signal>
<signal name="N$295">
</signal>
<signal name="N$296">
</signal>
<signal name="N$297">
</signal>
<signal name="N$298">
</signal>
<signal name="N$299">
</signal>
<signal name="N$300">
</signal>
<signal name="N$301">
</signal>
<signal name="N$302">
</signal>
<signal name="N$303">
</signal>
<signal name="N$304">
</signal>
<signal name="N$305">
</signal>
<signal name="N$306">
</signal>
<signal name="N$307">
</signal>
<signal name="N$308">
</signal>
<signal name="N$309">
</signal>
<signal name="N$310">
</signal>
<signal name="N$311">
</signal>
<signal name="N$312">
</signal>
<signal name="N$313">
</signal>
<signal name="N$314">
</signal>
<signal name="N$315">
</signal>
<signal name="N$316">
</signal>
<signal name="N$317">
</signal>
<signal name="N$318">
</signal>
<signal name="N$319">
</signal>
<signal name="N$320">
</signal>
<signal name="N$321">
</signal>
<signal name="N$322">
</signal>
<signal name="N$323">
</signal>
<signal name="N$324">
</signal>
<signal name="N$325">
</signal>
<signal name="N$326">
</signal>
<signal name="N$327">
</signal>
<signal name="N$328">
</signal>
<signal name="N$329">
</signal>
<signal name="N$330">
</signal>
<signal name="N$331">
</signal>
<signal name="N$332">
</signal>
<signal name="N$333">
</signal>
<signal name="N$334">
</signal>
<signal name="N$335">
</signal>
<signal name="N$336">
</signal>
<signal name="N$337">
</signal>
<signal name="N$338">
</signal>
<signal name="N$339">
</signal>
<signal name="N$340">
</signal>
<signal name="N$341">
</signal>
<signal name="N$342">
</signal>
<signal name="N$343">
</signal>
<signal name="N$344">
</signal>
<signal name="N$345">
</signal>
<signal name="N$346">
</signal>
<signal name="N$347">
</signal>
<signal name="N$348">
</signal>
<signal name="N$349">
</signal>
<signal name="N$350">
</signal>
<signal name="N$351">
</signal>
<signal name="N$352">
</signal>
<signal name="N$353">
</signal>
<signal name="N$354">
</signal>
<signal name="N$355">
</signal>
<signal name="N$356">
</signal>
<signal name="N$357">
</signal>
<signal name="N$358">
</signal>
<signal name="N$360">
</signal>
<signal name="N$361">
</signal>
<signal name="N$362">
</signal>
<signal name="N$363">
</signal>
<signal name="N$364">
</signal>
<signal name="N$365">
</signal>
<signal name="N$366">
</signal>
<signal name="N$367">
</signal>
<signal name="N$368">
</signal>
<signal name="N$369">
</signal>
<signal name="N$370">
</signal>
<signal name="N$371">
</signal>
<signal name="N$372">
</signal>
<signal name="N$374">
</signal>
<signal name="N$378">
</signal>
<signal name="N$379">
</signal>
<signal name="N$380">
</signal>
<signal name="N$383">
</signal>
<signal name="N$384">
</signal>
<signal name="N$385">
</signal>
<signal name="N$388">
</signal>
<signal name="N$389">
</signal>
<signal name="N$390">
</signal>
<signal name="N$395">
</signal>
<signal name="N$396">
</signal>
<signal name="N$184">
</signal>
<signal name="N$201">
</signal>
<signal name="N$230">
</signal>
<signal name="N$231">
</signal>
<signal name="WP">
<contactref element="IC1" pad="7"/>
<contactref element="R4" pad="1"/>
<contactref element="WP" pad="1"/>
</signal>
<signal name="N$232">
<contactref element="IC1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="WP1" pad="2"/>
</signal>
<signal name="N$233">
<contactref element="IC1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="WP2" pad="2"/>
</signal>
<signal name="N$234">
<contactref element="IC1" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$79">
</signal>
<signal name="N$143">
</signal>
<signal name="N$145">
</signal>
<signal name="N$377">
<contactref element="U$1" pad="6_V_BCKP"/>
<contactref element="BAT1" pad="VCC@1"/>
</signal>
<signal name="N$382">
<contactref element="U$1" pad="3_RXD1"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="N$386">
<contactref element="U$1" pad="2_TXD1"/>
<contactref element="L4" pad="2"/>
</signal>
<signal name="N$235">
<contactref element="U$1" pad="14_VCC_RF"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="RF">
<contactref element="L1" pad="1"/>
<contactref element="U$1" pad="11_RF_IN"/>
<contactref element="X1" pad="P"/>
</signal>
<signal name="N$375">
<contactref element="L1" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="TIMEPULSE">
<contactref element="BB1" pad="P8.8"/>
<contactref element="U$1" pad="4_TIMEPULSE"/>
</signal>
<signal name="VCC">
<contactref element="FIXED5V" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="+"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$96">
<contactref element="FIXED5V" pad="2"/>
<contactref element="D13" pad="C"/>
<contactref element="U$2" pad="P$2"/>
</signal>
<signal name="N$97">
<contactref element="F2" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="DCIN">
<contactref element="F2" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="5V">
<contactref element="BB1" pad="P9.7"/>
<contactref element="BB1" pad="P9.8"/>
</signal>
<signal name="N$49">
<contactref element="BB1" pad="P9.41"/>
</signal>
<signal name="N$50">
<contactref element="BB1" pad="P9.39"/>
</signal>
<signal name="N$51">
<contactref element="BB1" pad="P9.37"/>
</signal>
<signal name="N$52">
<contactref element="BB1" pad="P9.35"/>
</signal>
<signal name="N$53">
<contactref element="BB1" pad="P9.33"/>
</signal>
<signal name="N$54">
<contactref element="BB1" pad="P9.31"/>
</signal>
<signal name="N$55">
<contactref element="BB1" pad="P9.29"/>
</signal>
<signal name="N$56">
<contactref element="BB1" pad="P9.27"/>
</signal>
<signal name="N$57">
<contactref element="BB1" pad="P9.25"/>
</signal>
<signal name="N$58">
<contactref element="BB1" pad="P9.23"/>
</signal>
<signal name="N$59">
<contactref element="BB1" pad="P9.21"/>
</signal>
<signal name="N$61">
<contactref element="BB1" pad="P9.17"/>
</signal>
<signal name="N$62">
<contactref element="BB1" pad="P9.15"/>
</signal>
<signal name="N$65">
<contactref element="BB1" pad="P9.9"/>
</signal>
<signal name="VRAW">
<contactref element="BB1" pad="P9.5"/>
<contactref element="BB1" pad="P9.6"/>
<contactref element="C5" pad="+"/>
<contactref element="FIXED5V" pad="4"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="N$74">
<contactref element="BB1" pad="P9.10"/>
</signal>
<signal name="N$75">
<contactref element="BB1" pad="P9.12"/>
</signal>
<signal name="N$76">
<contactref element="BB1" pad="P9.14"/>
</signal>
<signal name="N$77">
<contactref element="BB1" pad="P9.16"/>
</signal>
<signal name="N$78">
<contactref element="BB1" pad="P9.18"/>
</signal>
<signal name="N$81">
<contactref element="BB1" pad="P9.24"/>
</signal>
<signal name="N$82">
<contactref element="BB1" pad="P9.26"/>
</signal>
<signal name="N$83">
<contactref element="BB1" pad="P9.28"/>
</signal>
<signal name="N$84">
<contactref element="BB1" pad="P9.30"/>
</signal>
<signal name="N$85">
<contactref element="BB1" pad="P9.32"/>
</signal>
<signal name="N$86">
<contactref element="BB1" pad="P9.34"/>
</signal>
<signal name="N$87">
<contactref element="BB1" pad="P9.36"/>
</signal>
<signal name="N$88">
<contactref element="BB1" pad="P9.38"/>
</signal>
<signal name="N$89">
<contactref element="BB1" pad="P9.40"/>
</signal>
<signal name="N$90">
<contactref element="BB1" pad="P9.42"/>
</signal>
<signal name="N$24">
<contactref element="BB1" pad="P8.45"/>
</signal>
<signal name="N$25">
<contactref element="BB1" pad="P8.43"/>
</signal>
<signal name="N$26">
<contactref element="BB1" pad="P8.41"/>
</signal>
<signal name="N$27">
<contactref element="BB1" pad="P8.39"/>
</signal>
<signal name="N$28">
<contactref element="BB1" pad="P8.37"/>
</signal>
<signal name="N$29">
<contactref element="BB1" pad="P8.35"/>
</signal>
<signal name="N$30">
<contactref element="BB1" pad="P8.33"/>
</signal>
<signal name="N$31">
<contactref element="BB1" pad="P8.31"/>
</signal>
<signal name="N$32">
<contactref element="BB1" pad="P8.29"/>
</signal>
<signal name="N$33">
<contactref element="BB1" pad="P8.27"/>
</signal>
<signal name="N$34">
<contactref element="BB1" pad="P8.25"/>
</signal>
<signal name="N$35">
<contactref element="BB1" pad="P8.23"/>
</signal>
<signal name="N$36">
<contactref element="BB1" pad="P8.21"/>
</signal>
<signal name="N$37">
<contactref element="BB1" pad="P8.19"/>
</signal>
<signal name="N$38">
<contactref element="BB1" pad="P8.17"/>
</signal>
<signal name="N$39">
<contactref element="BB1" pad="P8.15"/>
</signal>
<signal name="N$40">
<contactref element="BB1" pad="P8.13"/>
</signal>
<signal name="N$41">
<contactref element="BB1" pad="P8.11"/>
</signal>
<signal name="N$42">
<contactref element="BB1" pad="P8.9"/>
</signal>
<signal name="N$43">
<contactref element="BB1" pad="P8.7"/>
</signal>
<signal name="N$44">
<contactref element="BB1" pad="P8.5"/>
</signal>
<signal name="N$45">
<contactref element="BB1" pad="P8.3"/>
</signal>
<signal name="N$3">
<contactref element="BB1" pad="P8.4"/>
</signal>
<signal name="N$4">
<contactref element="BB1" pad="P8.6"/>
</signal>
<signal name="N$6">
<contactref element="BB1" pad="P8.10"/>
</signal>
<signal name="N$7">
<contactref element="BB1" pad="P8.12"/>
</signal>
<signal name="N$8">
<contactref element="BB1" pad="P8.14"/>
</signal>
<signal name="N$9">
<contactref element="BB1" pad="P8.16"/>
</signal>
<signal name="N$10">
<contactref element="BB1" pad="P8.18"/>
</signal>
<signal name="N$11">
<contactref element="BB1" pad="P8.20"/>
</signal>
<signal name="N$12">
<contactref element="BB1" pad="P8.22"/>
</signal>
<signal name="N$13">
<contactref element="BB1" pad="P8.24"/>
</signal>
<signal name="N$14">
<contactref element="BB1" pad="P8.26"/>
</signal>
<signal name="N$15">
<contactref element="BB1" pad="P8.28"/>
</signal>
<signal name="N$16">
<contactref element="BB1" pad="P8.30"/>
</signal>
<signal name="N$17">
<contactref element="BB1" pad="P8.32"/>
</signal>
<signal name="N$18">
<contactref element="BB1" pad="P8.34"/>
</signal>
<signal name="N$19">
<contactref element="BB1" pad="P8.36"/>
</signal>
<signal name="N$20">
<contactref element="BB1" pad="P8.38"/>
</signal>
<signal name="N$21">
<contactref element="BB1" pad="P8.40"/>
</signal>
<signal name="N$22">
<contactref element="BB1" pad="P8.42"/>
</signal>
<signal name="N$23">
<contactref element="BB1" pad="P8.44"/>
</signal>
<signal name="N$46">
<contactref element="BB1" pad="P8.46"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
