<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="20.066" y1="1.524" x2="38.024" y2="1.524" width="0" layer="20"/>
<wire x1="38.024" y1="1.524" x2="38.024" y2="27.168" width="0" layer="20"/>
<wire x1="38.024" y1="27.168" x2="20.066" y2="27.168" width="0" layer="20"/>
<wire x1="20.066" y1="27.168" x2="20.066" y2="1.524" width="0" layer="20"/>
<text>SFS</text>
<text>SCLK</text>
<text>PG7</text>
<text>PG6</text>
<text>STD</text>
<text>SRD</text>
<text>/CTS</text>
<text>/RTS</text>
<text>TX</text>
<text>RX</text>
<text>OP5</text>
<text>OP4</text>
<text>OP3</text>
<text>/RST</text>
<text>GND</text>
<text>3V3</text>
<text>+</text>
</plain>
<libraries>
<library name="ns_lmx9838">
<packages>
<package name="LTCC70">
<description>LTCC SB70A 70 pins, 10mm x 17mm x 2.0mm</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TC26HEZ">
<description>32kHz crystal package&lt;br&gt;
This is the "EZ" version, which has limited top masking for improved ease of assembly.</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="ns_lmx9838" package="LTCC70" value=""/>
<element name="Y1" library="SparkFun-FreqCtrl" package="TC26HEZ" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value=""/>
<element name="C2" library="SparkFun-Capacitors" package="0805" value=""/>
<element name="C3" library="SparkFun-Capacitors" package="0805" value=""/>
<element name="C4" library="SparkFun-Capacitors" package="0805" value=""/>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="JP4" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="JP5" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="JP6" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="SparkFun-PowerIC" package="SOT223" value=""/>
<element name="JP7" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="C6" library="SparkFun-Capacitors" package="0805" value=""/>
<element name="C7" library="SparkFun-Capacitors" package="0805" value=""/>
<element name="PG7" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PG6" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value=""/>
<element name="R2" library="SparkFun-Resistors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC_CORE">
<contactref element="U$1" pad="P$9"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="P$32"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="U$1" pad="P$17"/>
<contactref element="U$1" pad="P$18"/>
<contactref element="U$1" pad="P$29"/>
<contactref element="U$1" pad="P$24"/>
<contactref element="U$1" pad="P$30"/>
<contactref element="U$1" pad="P$31"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="JP7" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="P$28"/>
<contactref element="Y1" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="Y1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="P$27"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="P$15"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="P$14"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="P$13"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="P$12"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="P$7"/>
<contactref element="JP3" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="P$19"/>
<contactref element="JP3" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P$23"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="P$22"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="P$21"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="P$20"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="P$25"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="P$26"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="P$16"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="P$2"/>
<contactref element="JP6" pad="4"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="3"/>
<contactref element="JP7" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="P$10"/>
<contactref element="C4" pad="2"/>
<contactref element="U$1" pad="P$6"/>
<contactref element="C5" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="U$1" pad="P$11"/>
<contactref element="C3" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="C6" pad="1"/>
<contactref element="PG7" pad="A"/>
<contactref element="PG6" pad="A"/>
</signal>
<signal name="N$20">
<contactref element="PG7" pad="K"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="PG6" pad="K"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
