<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="31.75" y2="0" width="0" layer="20"/>
<wire x1="31.75" y1="0" x2="31.75" y2="27.94" width="0" layer="20"/>
<wire x1="31.75" y1="27.94" x2="0" y2="27.94" width="0" layer="20"/>
<wire x1="0" y1="27.94" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.54" y="3.556" drill="2.8"/>
<hole x="2.54" y="24.384" drill="2.8"/>
<hole x="29.21" y="24.892" drill="2.8"/>
<hole x="29.21" y="3.556" drill="2.8"/>
<text>PROGRAMMED</text>
<text>www.TelescopeLab.com</text>
<text>SPAC OPTICAL LAB</text>
<text>12v LED Dimmer
v1.0-9/2015</text>
<text>10K POT</text>
</plain>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,81/1,1">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="2,54/1,1">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 220 Vertical&lt;/b&gt; Package works with various parts including N-Channel MOSFET SparkFun SKU: COM-10213</description>
</package>
</packages>
</library>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL8">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="CAP-PTH-SMALL">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="9-12VIN" library="wirepad" package="3,81/1,1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5VLED" library="wirepad" package="3,81/1,1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="wirepad" package="3,81/1,1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GNDLED" library="wirepad" package="3,81/1,1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="12F683" library="microchip" package="DIL8" value="PIC12F683P">
<attribute name="OC_FARNELL" value="9759034"/>
<attribute name="MPN" value="PIC12F683-I/P"/>
<attribute name="MF" value="MICROCHIP"/>
<attribute name="OC_NEWARK" value="89H0442"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.4" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POTGND" library="wirepad" package="2,54/1,1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POTWIPE" library="wirepad" package="2,54/1,1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POT5V" library="wirepad" package="2,54/1,1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FQP30N06L" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET">
<attribute name="PROD_ID" value="TRANS-10060"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="linear" package="TO220V" value="7805">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HVLED" library="wirepad" package="3,81/1,1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="adafruit" package="DO41-10" value="1N4001">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="GND" pad="1"/>
<contactref element="12F683" pad="8"/>
<contactref element="POTGND" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="FQP30N06L" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="12F683" pad="5"/>
<contactref element="FQP30N06L" pad="1"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="5V">
<contactref element="R1" pad="P$1"/>
<contactref element="12F683" pad="1"/>
<contactref element="5VLED" pad="1"/>
<contactref element="POT5V" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="POTWIPE" pad="1"/>
<contactref element="12F683" pad="7"/>
</signal>
<signal name="N$2">
<contactref element="12F683" pad="4"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="GNDLED">
<contactref element="GNDLED" pad="1"/>
<contactref element="FQP30N06L" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="C1" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="HVLED" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="9-12VIN" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
