<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="-0.115734375" y1="53.2287" x2="-0.01081875" y2="3.824490625" width="0" layer="20"/>
<wire x1="-0.01081875" y1="3.824490625" x2="5.095028125" y2="-1.28926875" width="0" layer="20" curve="85"/>
<wire x1="5.095028125" y1="-1.28926875" x2="27.83035" y2="-1.37525625" width="0" layer="20"/>
<wire x1="27.83035" y1="-1.37525625" x2="33.56679375" y2="4.3513875" width="0" layer="20" curve="85"/>
<wire x1="33.56679375" y1="4.3513875" x2="33.463721875" y2="52.891859375" width="0" layer="20"/>
<wire x1="33.463721875" y1="52.891859375" x2="28.060503125" y2="58.303390625" width="0" layer="20" curve="85"/>
<wire x1="28.060503125" y1="58.303390625" x2="5.05444375" y2="58.390403125" width="0" layer="20"/>
<wire x1="5.05444375" y1="58.390403125" x2="-0.115734375" y2="53.2287" width="0" layer="20" curve="85"/>
<hole x="4.318" y="54.356" drill="3.175"/>
<hole x="29.083" y="54.356" drill="3.175"/>
<hole x="29.083" y="3.302" drill="3.175"/>
<hole x="4.318" y="3.302" drill="3.175"/>
<text>IR BLASTER 0.42</text>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_5MM">
<description>&lt;B&gt;LED 5mm PTH&lt;/B&gt;&lt;p&gt;
5 mm, round
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED-IR-THRU&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AUDIO-JACK">
<description>&lt;h3&gt;3.5mm Stereo Audio Jack&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Audio-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="nodemcu">
<description>NODEMCU</description>
<packages>
<package name="NODEMCU">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Sensors&lt;/h3&gt;
This library contains sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application.
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TSOP382">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="SparkFun-LED" package="LED_5MM" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-12058"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED_5MM" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-12058"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="AUDIO-JACK" value="AUDIO_JACK_3.5MM_PTH">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08447"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08447"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08447"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.3" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="nodemcu" package="NODEMCU" value="NODEMCU"/>
<element name="U1" library="SparkFun-Sensors" package="TSOP382" value="38kHz">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SEN-10266"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="3V">
<contactref element="U$1" pad="11"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="28"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="17"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="14"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="P$1"/>
<contactref element="U$1" pad="29"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="15"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R4" pad="P$1"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="3"/>
<contactref element="D1" pad="K"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="A"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="Q2" pad="3"/>
<contactref element="D2" pad="K"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="P$2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="P$2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="P$2"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="24"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="25"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="23"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R2" pad="P$2"/>
<contactref element="J1" pad="TIP"/>
<contactref element="J1" pad="RING"/>
</signal>
<signal name="N$13">
<contactref element="J1" pad="SLEEVE"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="20"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$15">
<contactref element="R6" pad="P$2"/>
<contactref element="Q3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
