<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="-20.5" y1="0" x2="20.5" y2="0" width="0" layer="20"/>
<wire x1="20.5" y1="0" x2="20.5" y2="31.5" width="0" layer="20"/>
<wire x1="20.5" y1="31.5" x2="-20.5" y2="31.5" width="0" layer="20"/>
<wire x1="-20.5" y1="31.5" x2="-20.5" y2="0" width="0" layer="20"/>
<text>Rev 1</text>
<text>Designed by:</text>
<text>MrSwirlyEyes</text>
<text>AmbiLamp</text>
<text>NEED TO CONNECT RED GREEN AND BLUE</text>
</plain>
<libraries>
<library name="PiB_logo">
<packages>
<package name="MRSWIRLYEYES-LOGO">
</package>
</packages>
</library>
<library name="_resistors">
<packages>
<package name="RESC1005X35_SMD-0402">
<description>CHIP, 1 X 0.5 X 0.35 mm body
&lt;p&gt;CHIP package with body size 1 X 0.5 X 0.35 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_switches">
<packages>
<package name="BTN_MOMENTARY_SPST-NO_L3-W2.5">
</package>
</packages>
</library>
<library name="_capacitors">
<packages>
<package name="CAPC1005X55_SMD-0402">
<description>CHIP, 1 X 0.5 X 0.55 mm body
&lt;p&gt;CHIP package with body size 1 X 0.5 X 0.55 mm&lt;/p&gt;</description>
</package>
<package name="CAPCP3216X160">
<description>Chip, 3.20 X 1.60 X 1.60 mm body
&lt;p&gt;Chip package with body size 3.20 X 1.60 X 1.60 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_radio_frequency">
<packages>
<package name="ESP8266-12E">
</package>
</packages>
</library>
<library name="_connectors">
<packages>
<package name="USB_MICRO-B_1050170001">
</package>
</packages>
</library>
<library name="_ic_power">
<packages>
<package name="SOT95P280X145-5">
<description>5-SOT23, 0.95 mm pitch, 2.8 mm span, 2.9 X 1.6 X 1.45 mm body
&lt;p&gt;5-pin SOT23 package with 0.95 mm pitch, 2.8 mm span with body size 2.9 X 1.6 X 1.45 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_ic_bridge">
<packages>
<package name="QFN50P500X500X75-28">
<description>28-QFN, 0.50 mm pitch, 5.00 X 5.00 X 0.75 mm body
&lt;p&gt;28-pin QFN package with 0.50 mm pitch with body size 5.00 X 5.00 X 0.75 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_leds">
<packages>
<package name="LEDC1005X40_LED-0402">
<description>CHIP, 1 X 0.5 X 0.4 mm body
&lt;p&gt;CHIP package with body size 1 X 0.5 X 0.4 mm&lt;/p&gt;</description>
</package>
<package name="HDRVR4W75P254_1X4_1066X254X850B">
<description>Single-row, 4-pin Receptacle Header (Female) Straight, 2.54 mm (0.10 in) col pitch, 8.50 mm insulator length, 10.66 X 2.54 X 8.50 mm body
&lt;p&gt;Single-row (1X4), 4-pin Receptacle Header (Female) Straight package with 2.54 mm (0.10 in) col pitch, 0.75 mm lead width, 3.20 mm tail length and 8.50 mm insulator length with overall size 10.66 X 2.54 X 8.50 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_transistors">
<packages>
<package name="SOT65P210X90-3">
<description>3-SOT23, 0.65 mm pitch, 2.10 mm span, 2.10 X 1.24 X 0.90 mm body
&lt;p&gt;3-pin SOT23 package with 0.65 mm pitch, 2.10 mm span with body size 2.10 X 1.24 X 0.90 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_sensors">
<packages>
<package name="TEMPERATURE-SENSOR_DHT22">
</package>
<package name="PHOTORESISTOR_TALL">
</package>
</packages>
</library>
<library name="_displays">
<packages>
<package name="HDRV4W64P254_1X4_1016X254X838B">
<description>Single-row, 4-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 10.16 X 2.54 X 8.38 mm body
&lt;p&gt;Single-row (1X4), 4-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.05 mm tail length and 5.84 mm mating length with overall size 10.16 X 2.54 X 8.38 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_sound">
<packages>
<package name="MICROPHONE_D9.7">
</package>
</packages>
</library>
<library name="_op_amps">
<packages>
<package name="SOIC127P600X175-14">
<description>14-SOIC, 1.27 mm pitch, 6.00 mm span, 8.65 X 3.90 X 1.75 mm body
&lt;p&gt;14-pin SOIC package with 1.27 mm pitch, 6.00 mm span with body size 8.65 X 3.90 X 1.75 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_discrete_semiconductors">
<packages>
<package name="SODFL1608X70">
<description>SODFL, 1.60 mm span, 1.20 X 0.80 X 0.70 mm body
&lt;p&gt;SODFL package with 1.60 mm span with body size 1.20 X 0.80 X 0.70 mm&lt;/p&gt;</description>
</package>
<package name="SODFL3616X98">
<description>SODFL, 3.60 mm span, 2.70 X 1.65 X 0.98 mm body
&lt;p&gt;SODFL package with 3.60 mm span with body size 2.70 X 1.65 X 0.98 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BJT1" library="_transistors" package="SOT65P210X90-3" value="MMBT2222 0.6A/40V">
<attribute name="DATASHEET" value="http://www.onsemi.com/pub/Collateral/MMBT2222AWT1-D.PDF"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/product-detail/en/on-semiconductor/MMBT2222AWT1G/MMBT2222AWT1GOSCT-ND/1139807"/>
<attribute name="DISTPN" value="MMBT2222AWT1GOSCT-ND"/>
<attribute name="MFR" value="ON Semiconductor"/>
<attribute name="MPN" value="MMBT2222AWT1G"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BJT2" library="_transistors" package="SOT65P210X90-3" value="MMBT2222 0.6A/40V">
<attribute name="DATASHEET" value="http://www.onsemi.com/pub/Collateral/MMBT2222AWT1-D.PDF"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/product-detail/en/on-semiconductor/MMBT2222AWT1G/MMBT2222AWT1GOSCT-ND/1139807"/>
<attribute name="DISTPN" value="MMBT2222AWT1GOSCT-ND"/>
<attribute name="MFR" value="ON Semiconductor"/>
<attribute name="MPN" value="MMBT2222AWT1G"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ESP1" library="_radio_frequency" package="ESP8266-12E" value="ESP8266-12E">
<attribute name="DATASHEET" value="https://www.kloppenborg.net/images/blog/esp8266/esp8266-esp12e-specs.pdf"/>
<attribute name="DIST" value="Amazon"/>
<attribute name="DISTLINK" value="https://www.amazon.com/Gowoops-ESP8266-Wireless-Transceiver-Development/dp/B01M4IOFIT/ref=sr_1_7?ie=UTF8&amp;qid=1537090267&amp;sr=8-7&amp;keywords=esp8266+12e"/>
<attribute name="DISTPN" value="B01M4IOFIT"/>
<attribute name="MFR" value="Espressif Systems"/>
<attribute name="MPN" value="ESP8266-12E"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="_ic_bridge" package="QFN50P500X500X75-28" value="CP2102N">
<attribute name="DATASHEET" value="https://www.silabs.com/documents/public/data-sheets/cp2102n-datasheet.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=336-3694-ND"/>
<attribute name="DISTPN" value="336-3694-ND"/>
<attribute name="MFR" value="Silicon Labs"/>
<attribute name="MPN" value="CP2102N-A01-GQFN28"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="CP2102N"/>
</element>
<element name="R8" library="_resistors" package="RESC1005X35_SMD-0402" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_51_RoHS_P_0.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG1281CT-ND"/>
<attribute name="DISTPN" value="YAG1281CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0710KP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="_resistors" package="RESC1005X35_SMD-0402" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_51_RoHS_P_0.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG1281CT-ND"/>
<attribute name="DISTPN" value="YAG1281CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0710KP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="_resistors" package="RESC1005X35_SMD-0402" value="220K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-220KLRCT-ND"/>
<attribute name="DISTPN" value="311-220KLRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402FR-07220KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="_resistors" package="RESC1005X35_SMD-0402" value="100K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-100KJRCT-ND"/>
<attribute name="DISTPN" value="311-100KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB1" library="_connectors" package="USB_MICRO-B_1050170001" value="USB2.0 MICRO-B">
<attribute name="DATASHEET" value="https://www.molex.com/pdm_docs/sd/1050170001_sd.pdf"/>
<attribute name="DATASHEET_CABLE" value="http://www.qualtekusa.com/images/Cable%20Assemblies/PDF_2/3025031-06.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=WM1399CT-ND"/>
<attribute name="DISTLINK_CABLE" value="https://www.digikey.com/products/en?keywords=Q967-ND"/>
<attribute name="DISTPN" value="WM1399CT-ND"/>
<attribute name="DISTPN_CABLE" value="Q967-ND"/>
<attribute name="DIST_CABLE" value="Digikey"/>
<attribute name="MFR" value="Molex, LLC"/>
<attribute name="MFR_CABLE" value="Qualtek"/>
<attribute name="MPN" value="1050170001"/>
<attribute name="MPN_CABLE" value="3025031-06"/>
<attribute name="VALUE" value="USB2.0 MICRO-B"/>
</element>
<element name="D1" library="_discrete_semiconductors" package="SODFL3616X98" value="1A / 20V / 0.34V">
<attribute name="DATASHEET" value="http://www.onsemi.com/pub/Collateral/MBR120VLSFT1-D.PDF"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=MBR120VLSFT3GOSCT-ND"/>
<attribute name="DISTPN" value="MBR120VLSFT3GOSCT-ND"/>
<attribute name="MFR" value="ON Semiconductor"/>
<attribute name="MPN" value="MBR120VLSFT3G"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="_capacitors" package="CAPC1005X55_SMD-0402" value="0.1uF/50V">
<attribute name="DATASHEET" value="https://product.tdk.com/info/en/catalog/datasheets/mlcc_commercial_soft_en.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=445-173610-1-ND"/>
<attribute name="DISTPN" value="445-173610-1-ND"/>
<attribute name="MFR" value="TDK Corporation"/>
<attribute name="MPN" value="C1005X7R1H104K050BE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="_capacitors" package="CAPC1005X55_SMD-0402" value="0.1uF/50V">
<attribute name="DATASHEET" value="https://product.tdk.com/info/en/catalog/datasheets/mlcc_commercial_soft_en.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=445-173610-1-ND"/>
<attribute name="DISTPN" value="445-173610-1-ND"/>
<attribute name="MFR" value="TDK Corporation"/>
<attribute name="MPN" value="C1005X7R1H104K050BE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="_capacitors" package="CAPC1005X55_SMD-0402" value="10uF/6.3V">
<attribute name="DATASHEET" value="https://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/mlcc/c02e.ashx"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=490-13233-1-ND"/>
<attribute name="DISTPN" value="490-13233-1-ND"/>
<attribute name="MFR" value="Murata Electronics North America"/>
<attribute name="MPN" value="GRM155C80J106ME11D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="_capacitors" package="CAPC1005X55_SMD-0402" value="10uF/6.3V">
<attribute name="DATASHEET" value="https://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/mlcc/c02e.ashx"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=490-13233-1-ND"/>
<attribute name="DISTPN" value="490-13233-1-ND"/>
<attribute name="MFR" value="Murata Electronics North America"/>
<attribute name="MPN" value="GRM155C80J106ME11D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VREG1" library="_ic_power" package="SOT95P280X145-5" value="AP2112K-3.3TRG1 600mA / 3.3V">
<attribute name="DATASHEET" value="https://www.diodes.com/assets/Datasheets/AP2112.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=AP2112K-3.3TRG1DICT-ND"/>
<attribute name="DISTPN" value="AP2112K-3.3TRG1DICT-ND"/>
<attribute name="MFR" value="Diodes Incorporated"/>
<attribute name="MPN" value="AP2112K-3.3TRG1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="_capacitors" package="CAPC1005X55_SMD-0402" value="1uF/25V">
<attribute name="DATASHEET" value="https://product.tdk.com/info/en/catalog/datasheets/mlcc_commercial_lowprofile_en.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=445-13185-1-ND"/>
<attribute name="DISTPN" value="445-13185-1-ND"/>
<attribute name="MFR" value="TDK Corporation"/>
<attribute name="MPN" value="CGB2A1X5R1E105K033BC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="_capacitors" package="CAPC1005X55_SMD-0402" value="1uF/25V">
<attribute name="DATASHEET" value="https://product.tdk.com/info/en/catalog/datasheets/mlcc_commercial_lowprofile_en.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=445-13185-1-ND"/>
<attribute name="DISTPN" value="445-13185-1-ND"/>
<attribute name="MFR" value="TDK Corporation"/>
<attribute name="MPN" value="CGB2A1X5R1E105K033BC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="_resistors" package="RESC1005X35_SMD-0402" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_51_RoHS_P_0.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG1281CT-ND"/>
<attribute name="DISTPN" value="YAG1281CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0710KP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="_resistors" package="RESC1005X35_SMD-0402" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_51_RoHS_P_0.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG1281CT-ND"/>
<attribute name="DISTPN" value="YAG1281CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0710KP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="_resistors" package="RESC1005X35_SMD-0402" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_51_RoHS_P_0.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG1281CT-ND"/>
<attribute name="DISTPN" value="YAG1281CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0710KP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="_resistors" package="RESC1005X35_SMD-0402" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_51_RoHS_P_0.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG1281CT-ND"/>
<attribute name="DISTPN" value="YAG1281CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0710KP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="_resistors" package="RESC1005X35_SMD-0402" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_51_RoHS_P_0.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG1281CT-ND"/>
<attribute name="DISTPN" value="YAG1281CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0710KP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="_capacitors" package="CAPC1005X55_SMD-0402" value="0.1uF/50V">
<attribute name="DATASHEET" value="https://product.tdk.com/info/en/catalog/datasheets/mlcc_commercial_soft_en.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=445-173610-1-ND"/>
<attribute name="DISTPN" value="445-173610-1-ND"/>
<attribute name="MFR" value="TDK Corporation"/>
<attribute name="MPN" value="C1005X7R1H104K050BE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="C8" library="_capacitors" package="CAPCP3216X160" value="100uF/10V">
<attribute name="DATASHEET" value="http://datasheets.avx.com/TLJ.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=478-5651-1-ND"/>
<attribute name="DISTPN" value="478-5651-1-ND"/>
<attribute name="MFR" value="AVX Corporation"/>
<attribute name="MPN" value="TLJA107M010R1400"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="_switches" package="BTN_MOMENTARY_SPST-NO_L3-W2.5" value="50mA/12V">
<attribute name="DATASHEET" value="http://omronfs.omron.com/en_US/ecb/products/pdf/en-b3u.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=SW1020CT-ND"/>
<attribute name="DISTPN" value="SW1020CT-ND"/>
<attribute name="MFR" value="Omron Electronics Inc-EMC Div"/>
<attribute name="MPN" value="B3U-1000P"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="_leds" package="LEDC1005X40_LED-0402" value="BLUE">
<attribute name="DATASHEET" value="https://www.bivar.com/portals/0/products/SM0402BWC.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=492-2203-1-ND"/>
<attribute name="DISTPN" value="492-2203-1-ND"/>
<attribute name="MFR" value="Bivar Inc."/>
<attribute name="MPN" value="SM0402BWC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="_capacitors" package="CAPC1005X55_SMD-0402" value="0.1uF/50V">
<attribute name="DATASHEET" value="https://product.tdk.com/info/en/catalog/datasheets/mlcc_commercial_soft_en.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=445-173610-1-ND"/>
<attribute name="DISTPN" value="445-173610-1-ND"/>
<attribute name="MFR" value="TDK Corporation"/>
<attribute name="MPN" value="C1005X7R1H104K050BE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="_capacitors" package="CAPC1005X55_SMD-0402" value="1uF/25V">
<attribute name="DATASHEET" value="https://product.tdk.com/info/en/catalog/datasheets/mlcc_commercial_lowprofile_en.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=445-13185-1-ND"/>
<attribute name="DISTPN" value="445-13185-1-ND"/>
<attribute name="MFR" value="TDK Corporation"/>
<attribute name="MPN" value="CGB2A1X5R1E105K033BC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="PiB_logo" package="MRSWIRLYEYES-LOGO" value=""/>
<element name="OPAMP1" library="_op_amps" package="SOIC127P600X175-14" value="LMV324">
<attribute name="DATASHEET" value="http://www.ti.com/lit/ds/symlink/lmv324.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=296-9569-1-ND"/>
<attribute name="DISTPN" value="296-9569-1-ND"/>
<attribute name="MFR" value="Texas Instruments"/>
<attribute name="MPN" value="LMV324IDR"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="LMV324"/>
</element>
<element name="MIC1" library="_sound" package="MICROPHONE_D9.7" value="20Hz-20kHz">
<attribute name="DATASHEET" value="https://www.cui.com/product/resource/cma-4544pf-w.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=102-1721-ND"/>
<attribute name="DISTPN" value="102-1721-ND"/>
<attribute name="MFR" value="CUI Inc."/>
<attribute name="MPN" value="CMA-4544PF-W"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="_resistors" package="RESC1005X35_SMD-0402" value="2.2K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-2.2KJRCT-ND"/>
<attribute name="DISTPN" value="311-2.2KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-072K2L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="_capacitors" package="CAPC1005X55_SMD-0402" value="10uF/6.3V">
<attribute name="DATASHEET" value="https://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/mlcc/c02e.ashx"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=490-13233-1-ND"/>
<attribute name="DISTPN" value="490-13233-1-ND"/>
<attribute name="MFR" value="Murata Electronics North America"/>
<attribute name="MPN" value="GRM155C80J106ME11D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="_resistors" package="RESC1005X35_SMD-0402" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_51_RoHS_P_0.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG1281CT-ND"/>
<attribute name="DISTPN" value="YAG1281CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0710KP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="_resistors" package="RESC1005X35_SMD-0402" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_51_RoHS_P_0.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG1281CT-ND"/>
<attribute name="DISTPN" value="YAG1281CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0710KP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="_resistors" package="RESC1005X35_SMD-0402" value="100K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-100KLRCT-ND"/>
<attribute name="DISTPN" value="311-100KLRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="_resistors" package="RESC1005X35_SMD-0402" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_51_RoHS_P_0.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG1281CT-ND"/>
<attribute name="DISTPN" value="YAG1281CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0710KP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="_capacitors" package="CAPC1005X55_SMD-0402" value="1uF/25V">
<attribute name="DATASHEET" value="https://product.tdk.com/info/en/catalog/datasheets/mlcc_commercial_lowprofile_en.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=445-13185-1-ND"/>
<attribute name="DISTPN" value="445-13185-1-ND"/>
<attribute name="MFR" value="TDK Corporation"/>
<attribute name="MPN" value="CGB2A1X5R1E105K033BC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="_resistors" package="RESC1005X35_SMD-0402" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_51_RoHS_P_0.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG1281CT-ND"/>
<attribute name="DISTPN" value="YAG1281CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0710KP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="_discrete_semiconductors" package="SODFL1608X70" value="RB751">
<attribute name="DATASHEET" value="https://www.onsemi.com/pub/Collateral/RB751S40T1-D.PDF"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=RB751S40T5GOSCT-ND"/>
<attribute name="DISTPN" value="RB751S40T5GOSCT-ND"/>
<attribute name="MFR" value="ON Semiconductor"/>
<attribute name="MPN" value="RB751S40T5G"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="_discrete_semiconductors" package="SODFL1608X70" value="RB751">
<attribute name="DATASHEET" value="https://www.onsemi.com/pub/Collateral/RB751S40T1-D.PDF"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=RB751S40T5GOSCT-ND"/>
<attribute name="DISTPN" value="RB751S40T5GOSCT-ND"/>
<attribute name="MFR" value="ON Semiconductor"/>
<attribute name="MPN" value="RB751S40T5G"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="_resistors" package="RESC1005X35_SMD-0402" value="22K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-3.30KLRCT-ND"/>
<attribute name="DISTPN" value="311-22KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0722KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="_resistors" package="RESC1005X35_SMD-0402" value="100">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-AC_51_RoHS_L_6.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG3516CT-ND"/>
<attribute name="DISTPN" value="YAG3516CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="AC0402JR-07100RL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="_capacitors" package="CAPC1005X55_SMD-0402" value="10uF/6.3V">
<attribute name="DATASHEET" value="https://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/mlcc/c02e.ashx"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=490-13233-1-ND"/>
<attribute name="DISTPN" value="490-13233-1-ND"/>
<attribute name="MFR" value="Murata Electronics North America"/>
<attribute name="MPN" value="GRM155C80J106ME11D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="_resistors" package="RESC1005X35_SMD-0402" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_51_RoHS_P_0.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG1281CT-ND"/>
<attribute name="DISTPN" value="YAG1281CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0710KP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="_resistors" package="RESC1005X35_SMD-0402" value="100K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-100KLRCT-ND"/>
<attribute name="DISTPN" value="311-100KLRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="_resistors" package="RESC1005X35_SMD-0402" value="3.3K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-3.30KLRCT-ND"/>
<attribute name="DISTPN" value="311-3.30KLRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402FR-073K3L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="_resistors" package="RESC1005X35_SMD-0402" value="100K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-100KLRCT-ND"/>
<attribute name="DISTPN" value="311-100KLRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="_resistors" package="RESC1005X35_SMD-0402" value="100">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-AC_51_RoHS_L_6.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG3516CT-ND"/>
<attribute name="DISTPN" value="YAG3516CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="AC0402JR-07100RL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="_capacitors" package="CAPC1005X55_SMD-0402" value="10uF/6.3V">
<attribute name="DATASHEET" value="https://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/mlcc/c02e.ashx"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=490-13233-1-ND"/>
<attribute name="DISTPN" value="490-13233-1-ND"/>
<attribute name="MFR" value="Murata Electronics North America"/>
<attribute name="MPN" value="GRM155C80J106ME11D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TEMP1" library="_sensors" package="TEMPERATURE-SENSOR_DHT22" value="DHT22">
<attribute name="DATASHEET" value="https://cdn-learn.adafruit.com/downloads/pdf/dht.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=1528-1504-ND"/>
<attribute name="DISTPN" value="1528-1504-ND"/>
<attribute name="MFR" value="Adafruit Industries LLC"/>
<attribute name="MPN" value="385"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="_resistors" package="RESC1005X35_SMD-0402" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_51_RoHS_P_0.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG1281CT-ND"/>
<attribute name="DISTPN" value="YAG1281CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0710KP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="_capacitors" package="CAPC1005X55_SMD-0402" value="0.1uF/50V">
<attribute name="DATASHEET" value="https://product.tdk.com/info/en/catalog/datasheets/mlcc_commercial_soft_en.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=445-173610-1-ND"/>
<attribute name="DISTPN" value="445-173610-1-ND"/>
<attribute name="MFR" value="TDK Corporation"/>
<attribute name="MPN" value="C1005X7R1H104K050BE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OLED_SCREEN1" library="_displays" package="HDRV4W64P254_1X4_1016X254X838B" value="SSD1306">
<attribute name="DATASHEET" value="https://cdn-shop.adafruit.com/datasheets/SSD1306.pdf"/>
<attribute name="DATASHEET_CONNECTOR" value="https://drawings-pdf.s3.amazonaws.com/C10436.pdf"/>
<attribute name="DIST" value="Amazon"/>
<attribute name="DISTLINK" value="https://www.amazon.com/Serial-Display-Module-Arduino-MakerFocus/dp/B076WXR8N9/ref=sr_1_4?s=electronics&amp;ie=UTF8&amp;qid=1522732901&amp;sr=1-4&amp;keywords=0.96+inch+OLED+Display+Module"/>
<attribute name="DISTLINK_CONNECTOR" value="https://www.digikey.com/products/en?keywords=PEC04SAAN"/>
<attribute name="DISTPN" value="B076WXR8N9"/>
<attribute name="DISTPN_CONNECTOR" value="S1012E-04-ND"/>
<attribute name="DIST_CONNECTOR" value="Digikey"/>
<attribute name="MFR" value="Makerfocus"/>
<attribute name="MFR_CONNECTOR" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="SSD1306"/>
<attribute name="MPN_CONNECTOR" value="PEC04SAAN"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="_capacitors" package="CAPC1005X55_SMD-0402" value="10uF/6.3V">
<attribute name="DATASHEET" value="https://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/mlcc/c02e.ashx"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=490-13233-1-ND"/>
<attribute name="DISTPN" value="490-13233-1-ND"/>
<attribute name="MFR" value="Murata Electronics North America"/>
<attribute name="MPN" value="GRM155C80J106ME11D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LDR1" library="_sensors" package="PHOTORESISTOR_TALL" value="LDR">
<attribute name="DATASHEET" value="https://cdn-learn.adafruit.com/downloads/pdf/photocells.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=1528-2141-ND"/>
<attribute name="DISTPN" value="1528-2141-ND"/>
<attribute name="MFR" value="Adafruit Industries LLC"/>
<attribute name="MPN" value="161"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="_resistors" package="RESC1005X35_SMD-0402" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-RC_51_RoHS_P_0.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG1281CT-ND"/>
<attribute name="DISTPN" value="YAG1281CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0710KP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="_leds" package="HDRVR4W75P254_1X4_1066X254X850B" value="RGB">
<attribute name="DATASHEET" value="N/A"/>
<attribute name="DATASHEET_CONNECTOR" value="https://drawings-pdf.s3.amazonaws.com/10492.pdf"/>
<attribute name="DIST" value="Amazon"/>
<attribute name="DISTLINK" value="https://www.amazon.com/Tricolor-Multicolor-Lighting-Electronics-Components/dp/B01C19ENFK/ref=sr_1_1?ie=UTF8&amp;qid=1504314575&amp;sr=8-1&amp;keywords=RGB+Clear+Common+Anode"/>
<attribute name="DISTLINK_CONNECTOR" value="https://www.digikey.com/products/en?mpart=PPPC041LFBN-RC&amp;v=35"/>
<attribute name="DISTPN" value="B01C19ENFK"/>
<attribute name="DISTPN_CONNECTOR" value="S7037-ND"/>
<attribute name="DIST_CONNECTOR" value="Digikey"/>
<attribute name="MFR" value="Chanzon"/>
<attribute name="MFR_CONNECTOR" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="100F5T-YT-RGB-CA"/>
<attribute name="MPN_CONNECTOR" value="PPPC041LFBN-RC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GPIO0">
<contactref element="BJT1" pad="3"/>
<contactref element="R5" pad="1"/>
<contactref element="ESP1" pad="18"/>
</signal>
<signal name="DTR">
<contactref element="BJT1" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="N$6">
<contactref element="R8" pad="2"/>
<contactref element="BJT1" pad="1"/>
</signal>
<signal name="RTS">
<contactref element="R8" pad="1"/>
<contactref element="IC1" pad="24"/>
<contactref element="BJT2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="EP"/>
<contactref element="R2" pad="1"/>
<contactref element="USB1" pad="5"/>
<contactref element="ESP1" pad="15"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="VREG1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C8" pad="K"/>
<contactref element="SW1" pad="P$1"/>
<contactref element="R11" pad="1"/>
<contactref element="USB1" pad="GND@0"/>
<contactref element="USB1" pad="GND@1"/>
<contactref element="USB1" pad="GND@2"/>
<contactref element="USB1" pad="GND@3"/>
<contactref element="USB1" pad="GND@4"/>
<contactref element="USB1" pad="GND@5"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="IC1" pad="P$1"/>
<contactref element="IC1" pad="P$3"/>
<contactref element="IC1" pad="P$4"/>
<contactref element="IC1" pad="P$5"/>
<contactref element="USB1" pad="P$1"/>
<contactref element="USB1" pad="P$2"/>
<contactref element="R15" pad="1"/>
<contactref element="MIC1" pad="2"/>
<contactref element="OPAMP1" pad="11"/>
<contactref element="OPAMP1" pad="5"/>
<contactref element="C13" pad="2"/>
<contactref element="R21" pad="1"/>
<contactref element="R27" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="TEMP1" pad="GND"/>
<contactref element="C15" pad="2"/>
<contactref element="OLED_SCREEN1" pad="GND"/>
<contactref element="C16" pad="2"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="ADC">
<contactref element="ESP1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VBUS">
<contactref element="USB1" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="D1" pad="K"/>
</signal>
<signal name="D+">
<contactref element="IC1" pad="4"/>
<contactref element="USB1" pad="3"/>
</signal>
<signal name="D-">
<contactref element="IC1" pad="5"/>
<contactref element="USB1" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="ESP1" pad="8"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="6"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="VREG1" pad="5"/>
<contactref element="C2" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C8" pad="A"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="R31" pad="2"/>
<contactref element="TEMP1" pad="VCC"/>
<contactref element="C15" pad="1"/>
<contactref element="OLED_SCREEN1" pad="VCC"/>
<contactref element="C16" pad="1"/>
<contactref element="LDR1" pad="P$2"/>
<contactref element="R26" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="OPAMP1" pad="4"/>
<contactref element="R12" pad="2"/>
<contactref element="LED3" pad="VCC"/>
</signal>
<signal name="GPIO15">
<contactref element="R7" pad="2"/>
<contactref element="ESP1" pad="16"/>
<contactref element="LED3" pad="GREEN"/>
</signal>
<signal name="GPIO2">
<contactref element="R6" pad="1"/>
<contactref element="ESP1" pad="17"/>
<contactref element="LED3" pad="RED"/>
</signal>
<signal name="EN">
<contactref element="ESP1" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="!RESET">
<contactref element="ESP1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="SW1" pad="P$2"/>
<contactref element="BJT2" pad="3"/>
</signal>
<signal name="RX">
<contactref element="ESP1" pad="21"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="TX">
<contactref element="ESP1" pad="22"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="26"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="K"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="C11" pad="2"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R16" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="OPAMP1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="MIC1" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R16" pad="2"/>
<contactref element="OPAMP1" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R15" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="OPAMP1" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="C12" pad="2"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="OPAMP1" pad="6"/>
<contactref element="D2" pad="K"/>
<contactref element="R19" pad="1"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="D2" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="R19" pad="2"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="OPAMP1" pad="7"/>
<contactref element="D3" pad="K"/>
</signal>
<signal name="N$15">
<contactref element="R21" pad="2"/>
<contactref element="OPAMP1" pad="10"/>
<contactref element="R20" pad="2"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="OPAMP1" pad="9"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="AMP_ENVELOPE">
<contactref element="OPAMP1" pad="8"/>
<contactref element="R22" pad="2"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="OPAMP1" pad="12"/>
<contactref element="R28" pad="1"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="OPAMP1" pad="13"/>
<contactref element="R26" pad="1"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="OPAMP1" pad="14"/>
<contactref element="R28" pad="2"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="GATE">
<contactref element="R29" pad="2"/>
<contactref element="ESP1" pad="7"/>
</signal>
<signal name="DHT22">
<contactref element="TEMP1" pad="DATA"/>
<contactref element="R31" pad="1"/>
<contactref element="ESP1" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="OLED_SCREEN1" pad="SDA"/>
<contactref element="ESP1" pad="19"/>
</signal>
<signal name="SCL">
<contactref element="OLED_SCREEN1" pad="SCL"/>
<contactref element="ESP1" pad="20"/>
</signal>
<signal name="LDR">
<contactref element="LDR1" pad="P$1"/>
<contactref element="R32" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="BLUE">
<contactref element="LED3" pad="BLUE"/>
<contactref element="ESP1" pad="6"/>
</signal>
<signal name="5V">
<contactref element="C1" pad="1"/>
<contactref element="VREG1" pad="3"/>
<contactref element="D1" pad="A"/>
<contactref element="VREG1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="BJT2" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
