<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="29.21" width="0.254" layer="20"/>
<wire x1="0" y1="29.21" x2="21.59" y2="29.21" width="0.254" layer="20"/>
<wire x1="21.59" y1="29.21" x2="21.59" y2="0" width="0.254" layer="20"/>
<wire x1="21.59" y1="0" x2="0" y2="0" width="0.254" layer="20"/>
<text>VDD</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>RESET</text>
<text>SCL</text>
<text>SDA</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
</plain>
<libraries>
<library name="PCA9548A">
<packages>
<package name="TSSOP24">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AVR_ICSP">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PCA9548A" library="PCA9548A" package="TSSOP24" value="TSSOP24A"/>
<element name="JP1" library="SparkFun-Connectors" package="AVR_ICSP" value="M05X2PTH"/>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="BUS" library="SparkFun-Connectors" package="1X05" value=""/>
</elements>
<signals>
<signal name="SDA0">
<contactref element="JP1" pad="1"/>
<contactref element="PCA9548A" pad="SD0"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="SCL0">
<contactref element="JP1" pad="2"/>
<contactref element="PCA9548A" pad="SC0"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="SDA1">
<contactref element="JP1" pad="3"/>
<contactref element="PCA9548A" pad="SD1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="SCL1">
<contactref element="JP1" pad="4"/>
<contactref element="PCA9548A" pad="SC1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="SCL2">
<contactref element="JP1" pad="6"/>
<contactref element="PCA9548A" pad="SC2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="SDA4">
<contactref element="JP1" pad="9"/>
<contactref element="PCA9548A" pad="SD4"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="SDA3">
<contactref element="JP1" pad="7"/>
<contactref element="PCA9548A" pad="SD3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="SDA2">
<contactref element="JP1" pad="5"/>
<contactref element="PCA9548A" pad="SD2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="SCL3">
<contactref element="PCA9548A" pad="SC3"/>
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="SCL4">
<contactref element="PCA9548A" pad="SC4"/>
<contactref element="R10" pad="1"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="VDD">
<contactref element="BUS" pad="2"/>
<contactref element="PCA9548A" pad="VDD"/>
<contactref element="R13" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="GND">
<contactref element="BUS" pad="1"/>
<contactref element="PCA9548A" pad="VSS"/>
<contactref element="PCA9548A" pad="A1"/>
<contactref element="PCA9548A" pad="A0"/>
<contactref element="PCA9548A" pad="A2"/>
</signal>
<signal name="N$1">
<contactref element="PCA9548A" pad="RESET"/>
<contactref element="R11" pad="2"/>
<contactref element="BUS" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="BUS" pad="4"/>
<contactref element="PCA9548A" pad="SCL"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="BUS" pad="5"/>
<contactref element="R12" pad="1"/>
<contactref element="PCA9548A" pad="SDA"/>
</signal>
<signal name="N$10">
</signal>
</signals>
</board>
</drawing>
</eagle>
