<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="40.31" y2="0" width="0" layer="20"/>
<wire x1="40.31" y1="0" x2="40.31" y2="35.55" width="0" layer="20"/>
<wire x1="40.31" y1="35.55" x2="0" y2="35.55" width="0" layer="20"/>
<wire x1="0" y1="35.55" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Batteries">
<description>&lt;h3&gt;SparkFun Batteries&lt;/h3&gt;
This library contains battery clips, connectors, and appropriately sized silk outlines for LiPo batteries. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_20MM_4LEGS_OVERPASTE">
<description>&lt;h3&gt;20mm Coin Cell Battery (CR2032) Holder - SMD (Dual Pad) (Overpaste on pads)&lt;/h3&gt;
&lt;p&gt;This holder fits 20mm Lithium coin cell batteries and holds the battery in place with friction. The metal housing connects to the positive (+) side of the battery and the PCB pad underneath is connected to the negative (-) side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/BAT-BLH-001.jpg"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_TEST_POINTS">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Test Point Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="6_PIN_SERIAL_TARGET_SIDE_RA_SMT">
<description>&lt;h3&gt;6 pin Serial Target - Right Angle  SMT&lt;/h3&gt;
Package for devices meant to mate to an FTDI connector. 
&lt;p&gt; tDocu shows pin location. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;6_Pin_Serial_Target&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="lph-7366">
<description>&lt;b&gt;LPH-7366: PCD8544-based Nokia 5110 monochrome LCD display&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="LPH-7366">
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MLF32-PAD">
</package>
</packages>
</library>
<library name="ADXL345">
<packages>
<package name="LGA_CC-14-1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BT2" library="SparkFun-Batteries" package="BATTCON_20MM_4LEGS_OVERPASTE" value="">
<attribute name="PROD_ID" value="PRT-11892 "/>
<attribute name="SF_SKU" value="BATT-10373"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X3_TEST_POINTS" value="AVR_SPI_PROG_3X2TESTPOINTS"/>
<element name="J2" library="SparkFun-Connectors" package="6_PIN_SERIAL_TARGET_SIDE_RA_SMT" value="">
<attribute name="PROD_ID" value="CONN-08971"/>
</element>
<element name="LCD1" library="lph-7366" package="LPH-7366" value="LPH-7366"/>
<element name="U1" library="SparkFun-IC-Microcontroller" package="MLF32-PAD" value=""/>
<element name="U2" library="ADXL345" package="LGA_CC-14-1" value="ADXL345BCCZ">
<attribute name="MANUFACTURER_PART_NUMBER" value="ADXL345BCCZ"/>
<attribute name="VENDOR" value="Analog Devices Inc"/>
</element>
</elements>
<signals>
<signal name="VDD">
<contactref element="LCD1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="LCD1" pad="7"/>
<contactref element="U1" pad="PAD"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="BT2" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="5"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="3V">
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="20"/>
<contactref element="BT2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
