<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<text>rst</text>
<text>3vo</text>
<text>gnd</text>
<text>en</text>
<text>bat</text>
<text>usb</text>
<text>sda</text>
<text>scl</text>
<text>tx</text>
<text>rx</text>
<text>mi</text>
<text>mo</text>
<text>sck</text>
<wire x1="2.54" y1="22.86" x2="48.26" y2="22.86" width="0" layer="20"/>
<wire x1="48.26" y1="22.86" x2="50.8" y2="20.32" width="0" layer="20" curve="-90"/>
<wire x1="50.8" y1="20.32" x2="50.8" y2="2.54" width="0" layer="20"/>
<wire x1="50.8" y1="2.54" x2="48.26" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="48.26" y1="0" x2="2.54" y2="0" width="0" layer="20"/>
<wire x1="2.54" y1="0" x2="0" y2="2.54" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="2.54" x2="0" y2="20.32" width="0" layer="20"/>
<wire x1="0" y1="20.32" x2="2.54" y2="22.86" width="0" layer="20" curve="-90"/>
<text>feather</text>
<text>proto</text>
<text>wing</text>
<text>A</text>
<text>Adapter for Pervasive Displays, rev D</text>
<text>For Feather M0:</text>
<text>PANEL_ON 9, BORDER 17, DISCHARGE 10, </text>
<text>RESET 6, BUSY 18, EPD_CS 19, FLASH_CS 5 </text>
<text>+ SPI &amp; I2C</text>
<text>EmbeddedArtists</text>
</plain>
<libraries>
<library name="microbuilder">
<packages>
<package name="FEATHERWING">
</package>
<package name="1X16_ROUND_76MIL">
</package>
<package name="1X12_ROUND_76MIL">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X07_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -7 Pin  No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MS1" library="microbuilder" package="FEATHERWING" value="FEATHERWING"/>
<element name="JP3" library="microbuilder" package="1X16_ROUND_76MIL" value=""/>
<element name="JP1" library="microbuilder" package="1X12_ROUND_76MIL" value=""/>
<element name="J1" library="SparkFun-Connectors" package="1X07_NO_SILK" value=""/>
<element name="J2" library="SparkFun-Connectors" package="1X07_NO_SILK" value=""/>
</elements>
<signals>
<signal name="N$2">
<contactref element="MS1" pad="16"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="MS1" pad="15"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="MS1" pad="14"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="MS1" pad="13"/>
<contactref element="JP3" pad="4"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="MS1" pad="12"/>
<contactref element="JP3" pad="5"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="MS1" pad="11"/>
<contactref element="JP3" pad="6"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="MS1" pad="10"/>
<contactref element="JP3" pad="7"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="MS1" pad="9"/>
<contactref element="JP3" pad="8"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="MS1" pad="8"/>
<contactref element="JP3" pad="9"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="MS1" pad="7"/>
<contactref element="JP3" pad="10"/>
</signal>
<signal name="N$14">
<contactref element="MS1" pad="6"/>
<contactref element="JP3" pad="11"/>
</signal>
<signal name="N$15">
<contactref element="MS1" pad="5"/>
<contactref element="JP3" pad="12"/>
</signal>
<signal name="GND">
<contactref element="MS1" pad="4"/>
<contactref element="JP3" pad="13"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="AREF">
<contactref element="MS1" pad="3"/>
<contactref element="JP3" pad="14"/>
</signal>
<signal name="3V">
<contactref element="MS1" pad="2"/>
<contactref element="JP3" pad="15"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="MS1" pad="1"/>
<contactref element="JP3" pad="16"/>
</signal>
<signal name="VBAT">
<contactref element="MS1" pad="28"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="MS1" pad="27"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="USB">
<contactref element="MS1" pad="26"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="MS1" pad="25"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="MS1" pad="24"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$19">
<contactref element="MS1" pad="23"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$20">
<contactref element="MS1" pad="22"/>
<contactref element="JP1" pad="7"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="N$21">
<contactref element="MS1" pad="21"/>
<contactref element="JP1" pad="8"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$22">
<contactref element="MS1" pad="20"/>
<contactref element="JP1" pad="9"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$23">
<contactref element="MS1" pad="19"/>
<contactref element="JP1" pad="10"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$24">
<contactref element="MS1" pad="18"/>
<contactref element="JP1" pad="11"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$25">
<contactref element="MS1" pad="17"/>
<contactref element="JP1" pad="12"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$30">
</signal>
</signals>
</board>
</drawing>
</eagle>
