<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="50.927" x2="0" y2="3.175" width="0" layer="20"/>
<wire x1="0" y1="3.175" x2="3.175" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.175" y1="0" x2="63.5" y2="0" width="0" layer="20"/>
<wire x1="63.5" y1="0" x2="76.2" y2="12.7" width="0" layer="20" curve="90"/>
<wire x1="76.2" y1="12.7" x2="76.2" y2="41.402" width="0" layer="20"/>
<wire x1="76.2" y1="41.402" x2="63.5" y2="54.61" width="0" layer="20" curve="90"/>
<wire x1="63.5" y1="54.61" x2="3.175" y2="54.61" width="0" layer="20"/>
<wire x1="3.175" y1="54.61" x2="0" y2="50.927" width="0" layer="20" curve="90"/>
<text>CUT OUT</text>
<text>CUT OUT</text>
<text>CUT OUT</text>
<text>CUT OUT</text>
<text>CUT OUT</text>
<text>CUT OUT</text>
<hole x="70.485" y="48.26" drill="3.175"/>
<hole x="70.485" y="6.35" drill="3.175"/>
<hole x="4.445" y="51.435" drill="3.175"/>
<hole x="4.445" y="3.175" drill="3.175"/>
<text>-</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>Hexacopter
Cape Rev A</text>
<text>C</text>
<text>B</text>
<text>A</text>
<text>C</text>
<text>C</text>
<text>C</text>
<text>C</text>
<text>C</text>
<text>B</text>
<text>B</text>
<text>B</text>
<text>B</text>
<text>B</text>
<text>A</text>
<text>A</text>
<text>A</text>
<text>A</text>
<text>A</text>
<text>COM</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>A</text>
<text>B</text>
<text>C</text>
<text>-</text>
<text>+</text>
<text>A</text>
<text>B</text>
<text>C</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>C</text>
<text>B</text>
<text>B</text>
<text>A</text>
<text>A</text>
<text>+</text>
<text>COM</text>
<text>-</text>
<text>C</text>
<text>B</text>
<text>A</text>
<text>A</text>
<text>B</text>
<text>C</text>
<text>C</text>
<text>B</text>
<text>A</text>
<text>A</text>
<text>1</text>
<text>6</text>
<text>SIGNALS</text>
<text>Hexacopter
Cape Rev A</text>
</plain>
<libraries>
<library name="matts">
<packages>
<package name="DYS_BLHELI_ESC">
</package>
<package name="3_PADS">
</package>
<package name="2PADS">
</package>
<package name="MA06-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Strawson_Eagle_Lib">
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ESC_3" library="matts" package="DYS_BLHELI_ESC" value="DYS_BLHELI_ESC"/>
<element name="ESC_2" library="matts" package="DYS_BLHELI_ESC" value="DYS_BLHELI_ESC"/>
<element name="ESC_1" library="matts" package="DYS_BLHELI_ESC" value="DYS_BLHELI_ESC"/>
<element name="ESC_4" library="matts" package="DYS_BLHELI_ESC" value="DYS_BLHELI_ESC"/>
<element name="ESC_5" library="matts" package="DYS_BLHELI_ESC" value="DYS_BLHELI_ESC"/>
<element name="ESC_6" library="matts" package="DYS_BLHELI_ESC" value="DYS_BLHELI_ESC"/>
<element name="SIGNALS" library="matts" package="MA06-1" value="">
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="3" library="matts" package="3_PADS" value="3_PADS">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="2" library="matts" package="3_PADS" value="3_PADS">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="1" library="matts" package="3_PADS" value="3_PADS">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="6" library="matts" package="3_PADS" value="3_PADS">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="5" library="matts" package="3_PADS" value="3_PADS">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="4" library="matts" package="3_PADS" value="3_PADS">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="C1" library="Strawson_Eagle_Lib" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="C2" library="Strawson_Eagle_Lib" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="C3" library="Strawson_Eagle_Lib" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="C4" library="Strawson_Eagle_Lib" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="SERIES2" library="matts" package="2PADS" value="2PADS"/>
<element name="SERIES" library="matts" package="2PADS" value="2PADS"/>
<element name="PWR" library="matts" package="2PADS" value="2PADS">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="AUX2" library="matts" package="2PADS" value="2PADS">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="AUX1" library="matts" package="2PADS" value="2PADS">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="3A">
<contactref element="ESC_3" pad="7"/>
<contactref element="ESC_3" pad="8"/>
<contactref element="3" pad="A"/>
<contactref element="3" pad="P$4"/>
<contactref element="3" pad="P$7"/>
<contactref element="3" pad="P$8"/>
<contactref element="3" pad="P$9"/>
</signal>
<signal name="3B">
<contactref element="ESC_3" pad="9"/>
<contactref element="ESC_3" pad="10"/>
<contactref element="3" pad="B"/>
<contactref element="3" pad="P$5"/>
<contactref element="3" pad="P$10"/>
<contactref element="3" pad="P$11"/>
<contactref element="3" pad="P$12"/>
</signal>
<signal name="3C">
<contactref element="ESC_3" pad="11"/>
<contactref element="ESC_3" pad="12"/>
<contactref element="3" pad="C"/>
<contactref element="3" pad="P$6"/>
<contactref element="3" pad="P$13"/>
<contactref element="3" pad="P$14"/>
<contactref element="3" pad="P$15"/>
</signal>
<signal name="2A">
<contactref element="ESC_2" pad="7"/>
<contactref element="ESC_2" pad="8"/>
<contactref element="2" pad="A"/>
<contactref element="2" pad="P$4"/>
<contactref element="2" pad="P$7"/>
<contactref element="2" pad="P$8"/>
<contactref element="2" pad="P$9"/>
</signal>
<signal name="2B">
<contactref element="ESC_2" pad="9"/>
<contactref element="ESC_2" pad="10"/>
<contactref element="2" pad="B"/>
<contactref element="2" pad="P$5"/>
<contactref element="2" pad="P$10"/>
<contactref element="2" pad="P$11"/>
<contactref element="2" pad="P$12"/>
</signal>
<signal name="2C">
<contactref element="ESC_2" pad="11"/>
<contactref element="ESC_2" pad="12"/>
<contactref element="2" pad="C"/>
<contactref element="2" pad="P$6"/>
<contactref element="2" pad="P$13"/>
<contactref element="2" pad="P$14"/>
<contactref element="2" pad="P$15"/>
</signal>
<signal name="4A">
<contactref element="ESC_4" pad="7"/>
<contactref element="ESC_4" pad="8"/>
<contactref element="4" pad="A"/>
<contactref element="4" pad="P$4"/>
<contactref element="4" pad="P$7"/>
<contactref element="4" pad="P$8"/>
<contactref element="4" pad="P$9"/>
</signal>
<signal name="4B">
<contactref element="ESC_4" pad="9"/>
<contactref element="ESC_4" pad="10"/>
<contactref element="4" pad="B"/>
<contactref element="4" pad="P$5"/>
<contactref element="4" pad="P$10"/>
<contactref element="4" pad="P$11"/>
<contactref element="4" pad="P$12"/>
</signal>
<signal name="4C">
<contactref element="ESC_4" pad="11"/>
<contactref element="ESC_4" pad="12"/>
<contactref element="4" pad="C"/>
<contactref element="4" pad="P$6"/>
<contactref element="4" pad="P$13"/>
<contactref element="4" pad="P$14"/>
<contactref element="4" pad="P$15"/>
</signal>
<signal name="5A">
<contactref element="ESC_5" pad="7"/>
<contactref element="ESC_5" pad="8"/>
<contactref element="5" pad="A"/>
<contactref element="5" pad="P$4"/>
<contactref element="5" pad="P$7"/>
<contactref element="5" pad="P$8"/>
<contactref element="5" pad="P$9"/>
</signal>
<signal name="5B">
<contactref element="ESC_5" pad="9"/>
<contactref element="ESC_5" pad="10"/>
<contactref element="5" pad="B"/>
<contactref element="5" pad="P$5"/>
<contactref element="5" pad="P$10"/>
<contactref element="5" pad="P$11"/>
<contactref element="5" pad="P$12"/>
</signal>
<signal name="5C">
<contactref element="ESC_5" pad="11"/>
<contactref element="ESC_5" pad="12"/>
<contactref element="5" pad="C"/>
<contactref element="5" pad="P$6"/>
<contactref element="5" pad="P$13"/>
<contactref element="5" pad="P$14"/>
<contactref element="5" pad="P$15"/>
</signal>
<signal name="1A">
<contactref element="ESC_1" pad="7"/>
<contactref element="ESC_1" pad="8"/>
<contactref element="1" pad="A"/>
<contactref element="1" pad="P$4"/>
<contactref element="1" pad="P$7"/>
<contactref element="1" pad="P$8"/>
<contactref element="1" pad="P$9"/>
</signal>
<signal name="1B">
<contactref element="ESC_1" pad="9"/>
<contactref element="ESC_1" pad="10"/>
<contactref element="1" pad="B"/>
<contactref element="1" pad="P$5"/>
<contactref element="1" pad="P$10"/>
<contactref element="1" pad="P$11"/>
<contactref element="1" pad="P$12"/>
</signal>
<signal name="1C">
<contactref element="ESC_1" pad="11"/>
<contactref element="ESC_1" pad="12"/>
<contactref element="1" pad="C"/>
<contactref element="1" pad="P$6"/>
<contactref element="1" pad="P$13"/>
<contactref element="1" pad="P$14"/>
<contactref element="1" pad="P$15"/>
</signal>
<signal name="6A">
<contactref element="ESC_6" pad="7"/>
<contactref element="ESC_6" pad="8"/>
<contactref element="6" pad="A"/>
<contactref element="6" pad="P$4"/>
<contactref element="6" pad="P$7"/>
<contactref element="6" pad="P$8"/>
<contactref element="6" pad="P$9"/>
</signal>
<signal name="6B">
<contactref element="ESC_6" pad="9"/>
<contactref element="ESC_6" pad="10"/>
<contactref element="6" pad="B"/>
<contactref element="6" pad="P$5"/>
<contactref element="6" pad="P$10"/>
<contactref element="6" pad="P$11"/>
<contactref element="6" pad="P$12"/>
</signal>
<signal name="6C">
<contactref element="ESC_6" pad="11"/>
<contactref element="ESC_6" pad="12"/>
<contactref element="6" pad="C"/>
<contactref element="6" pad="P$6"/>
<contactref element="6" pad="P$13"/>
<contactref element="6" pad="P$14"/>
<contactref element="6" pad="P$15"/>
</signal>
<signal name="VCC">
<contactref element="ESC_2" pad="2"/>
<contactref element="ESC_2" pad="1"/>
<contactref element="ESC_1" pad="2"/>
<contactref element="ESC_1" pad="1"/>
<contactref element="ESC_5" pad="2"/>
<contactref element="ESC_5" pad="1"/>
<contactref element="ESC_6" pad="2"/>
<contactref element="ESC_6" pad="1"/>
<contactref element="ESC_3" pad="2"/>
<contactref element="ESC_3" pad="1"/>
<contactref element="ESC_4" pad="2"/>
<contactref element="ESC_4" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="SERIES2" pad="+TOP"/>
<contactref element="SERIES2" pad="+1"/>
<contactref element="SERIES2" pad="+5"/>
<contactref element="SERIES2" pad="+BOTTOM"/>
<contactref element="PWR" pad="+TOP"/>
<contactref element="PWR" pad="+1"/>
<contactref element="PWR" pad="+5"/>
<contactref element="PWR" pad="+BOTTOM"/>
<contactref element="SERIES2" pad="+2"/>
<contactref element="SERIES2" pad="+3"/>
<contactref element="SERIES2" pad="+4"/>
<contactref element="PWR" pad="+2"/>
<contactref element="PWR" pad="+3"/>
<contactref element="PWR" pad="+4"/>
<contactref element="AUX2" pad="+TOP"/>
<contactref element="AUX2" pad="+1"/>
<contactref element="AUX2" pad="+5"/>
<contactref element="AUX2" pad="+BOTTOM"/>
<contactref element="AUX2" pad="+4"/>
<contactref element="AUX2" pad="+2"/>
<contactref element="AUX2" pad="+3"/>
<contactref element="AUX1" pad="+5"/>
<contactref element="AUX1" pad="+TOP"/>
<contactref element="AUX1" pad="+BOTTOM"/>
<contactref element="AUX1" pad="+3"/>
<contactref element="AUX1" pad="+1"/>
<contactref element="AUX1" pad="+4"/>
<contactref element="AUX1" pad="+2"/>
</signal>
<signal name="GND">
<contactref element="ESC_3" pad="5"/>
<contactref element="ESC_3" pad="6"/>
<contactref element="ESC_3" pad="4"/>
<contactref element="ESC_4" pad="4"/>
<contactref element="ESC_4" pad="5"/>
<contactref element="ESC_4" pad="6"/>
<contactref element="ESC_5" pad="5"/>
<contactref element="ESC_5" pad="4"/>
<contactref element="ESC_5" pad="6"/>
<contactref element="ESC_2" pad="5"/>
<contactref element="ESC_2" pad="6"/>
<contactref element="ESC_2" pad="4"/>
<contactref element="ESC_1" pad="6"/>
<contactref element="ESC_1" pad="4"/>
<contactref element="ESC_1" pad="5"/>
<contactref element="ESC_6" pad="6"/>
<contactref element="ESC_6" pad="4"/>
<contactref element="ESC_6" pad="5"/>
<contactref element="ESC_3" pad="P$1"/>
<contactref element="ESC_2" pad="P$1"/>
<contactref element="ESC_1" pad="P$1"/>
<contactref element="ESC_6" pad="P$1"/>
<contactref element="ESC_5" pad="P$1"/>
<contactref element="ESC_4" pad="P$1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="SERIES" pad="B"/>
<contactref element="SERIES" pad="P$11"/>
<contactref element="SERIES" pad="P$5"/>
<contactref element="SERIES" pad="P$12"/>
<contactref element="SERIES" pad="P$10"/>
<contactref element="PWR" pad="B"/>
<contactref element="PWR" pad="P$11"/>
<contactref element="PWR" pad="P$5"/>
<contactref element="PWR" pad="P$12"/>
<contactref element="PWR" pad="P$10"/>
<contactref element="SERIES" pad="P$13"/>
<contactref element="SERIES" pad="P$14"/>
<contactref element="PWR" pad="P$13"/>
<contactref element="PWR" pad="P$14"/>
<contactref element="AUX2" pad="P$14"/>
<contactref element="AUX2" pad="P$10"/>
<contactref element="AUX2" pad="P$12"/>
<contactref element="AUX2" pad="P$5"/>
<contactref element="AUX2" pad="B"/>
<contactref element="AUX2" pad="P$13"/>
<contactref element="AUX2" pad="P$11"/>
<contactref element="AUX1" pad="P$5"/>
<contactref element="AUX1" pad="P$13"/>
<contactref element="AUX1" pad="B"/>
<contactref element="AUX1" pad="P$11"/>
<contactref element="AUX1" pad="P$14"/>
<contactref element="AUX1" pad="P$10"/>
<contactref element="AUX1" pad="P$12"/>
</signal>
<signal name="PWM_3">
<contactref element="ESC_3" pad="3"/>
<contactref element="SIGNALS" pad="3"/>
</signal>
<signal name="PWM_2">
<contactref element="ESC_2" pad="3"/>
<contactref element="SIGNALS" pad="2"/>
</signal>
<signal name="PWM_1">
<contactref element="ESC_1" pad="3"/>
<contactref element="SIGNALS" pad="1"/>
</signal>
<signal name="PWM_6">
<contactref element="ESC_6" pad="3"/>
<contactref element="SIGNALS" pad="6"/>
</signal>
<signal name="PWM_5">
<contactref element="ESC_5" pad="3"/>
<contactref element="SIGNALS" pad="5"/>
</signal>
<signal name="PWM_4">
<contactref element="ESC_4" pad="3"/>
<contactref element="SIGNALS" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="SERIES2" pad="B"/>
<contactref element="SERIES2" pad="P$11"/>
<contactref element="SERIES2" pad="P$5"/>
<contactref element="SERIES2" pad="P$12"/>
<contactref element="SERIES2" pad="P$10"/>
<contactref element="SERIES" pad="+TOP"/>
<contactref element="SERIES" pad="+1"/>
<contactref element="SERIES" pad="+5"/>
<contactref element="SERIES" pad="+BOTTOM"/>
<contactref element="SERIES2" pad="P$13"/>
<contactref element="SERIES2" pad="P$14"/>
<contactref element="SERIES" pad="+2"/>
<contactref element="SERIES" pad="+3"/>
<contactref element="SERIES" pad="+4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
