<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>0R
1T
2
3*
4
5*
6*
7</text>
<text>8
9*
10*
11*
12
13
GND
REF</text>
<text>A5
A4
A3
A2
A1
A0</text>
<text>A6</text>
<text>VIN
GND
GND
5V
3V3
R</text>
<text>Nano2Nove</text>
<text>N2N002</text>
<text>7-12V</text>
<text>A7</text>
<wire x1="0.635" y1="0" x2="41.91" y2="0" width="0" layer="20"/>
<wire x1="41.91" y1="0" x2="42.545" y2="0.635" width="0" layer="20" curve="90"/>
<wire x1="42.545" y1="0.635" x2="42.545" y2="53.34" width="0" layer="20"/>
<wire x1="42.545" y1="53.34" x2="41.91" y2="53.975" width="0" layer="20" curve="90"/>
<wire x1="41.91" y1="53.975" x2="0.635" y2="53.975" width="0" layer="20"/>
<wire x1="0.635" y1="53.975" x2="0" y2="53.34" width="0" layer="20" curve="90"/>
<wire x1="0" y1="53.34" x2="0" y2="0.635" width="0" layer="20"/>
<wire x1="0" y1="0.635" x2="0.635" y2="0" width="0" layer="20" curve="90"/>
</plain>
<libraries>
<library name="arno">
<packages>
<package name="ARDUINO-NANO-V3-NOHOLES-SILK">
</package>
<package name="DUEMILANOVE-VIAS">
</package>
<package name="LOGO_ARNO_SMALL_MIR">
</package>
<package name="LOGO_ARNO_SMALL">
</package>
<package name="DIODE-075">
<description>&lt;b&gt;Diode (7.5mm)&lt;/b&gt;&lt;br /&gt;
Based on &lt;em&gt;D-7.5&lt;/em&gt; from &lt;em&gt;diode.lbr&lt;/em&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH_LOCK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ARD1" library="arno" package="ARDUINO-NANO-V3-NOHOLES-SILK" value=""/>
<element name="ARD2" library="arno" package="DUEMILANOVE-VIAS" value="ARDUINO-PINSVIAS"/>
<element name="J1" library="jumper" package="JP1" value="">
<attribute name="VALUE"/>
</element>
<element name="CON" library="SparkFun-Connectors" package="POWER_JACK_PTH_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="arno" package="LOGO_ARNO_SMALL_MIR" value=""/>
<element name="U$2" library="arno" package="LOGO_ARNO_SMALL" value=""/>
<element name="ARD3" library="arno" package="DUEMILANOVE-VIAS" value="ARDUINO-PINSVIAS"/>
<element name="D1" library="arno" package="DIODE-075" value=""/>
<element name="D2" library="arno" package="DIODE-075" value=""/>
</elements>
<signals>
<signal name="D2">
<contactref element="ARD1" pad="D2"/>
<contactref element="ARD2" pad="D2"/>
<contactref element="ARD3" pad="D2"/>
</signal>
<signal name="D3">
<contactref element="ARD1" pad="D3"/>
<contactref element="ARD2" pad="D3"/>
<contactref element="ARD3" pad="D3"/>
</signal>
<signal name="D4">
<contactref element="ARD1" pad="D4"/>
<contactref element="ARD2" pad="D4"/>
<contactref element="ARD3" pad="D4"/>
</signal>
<signal name="D5">
<contactref element="ARD1" pad="D5"/>
<contactref element="ARD2" pad="D5"/>
<contactref element="ARD3" pad="D5"/>
</signal>
<signal name="D6">
<contactref element="ARD1" pad="D6"/>
<contactref element="ARD2" pad="D6"/>
<contactref element="ARD3" pad="D6"/>
</signal>
<signal name="D7">
<contactref element="ARD1" pad="D7"/>
<contactref element="ARD2" pad="D7"/>
<contactref element="ARD3" pad="D7"/>
</signal>
<signal name="D8">
<contactref element="ARD1" pad="D8"/>
<contactref element="ARD2" pad="D8"/>
<contactref element="ARD3" pad="D8"/>
</signal>
<signal name="D9">
<contactref element="ARD1" pad="D9"/>
<contactref element="ARD2" pad="D9"/>
<contactref element="ARD3" pad="D9"/>
</signal>
<signal name="D10">
<contactref element="ARD1" pad="D10"/>
<contactref element="ARD2" pad="D10"/>
<contactref element="ARD3" pad="D10"/>
</signal>
<signal name="D11">
<contactref element="ARD1" pad="D11"/>
<contactref element="ARD2" pad="D11"/>
<contactref element="ARD3" pad="D11"/>
</signal>
<signal name="D12">
<contactref element="ARD1" pad="D12"/>
<contactref element="ARD2" pad="D12"/>
<contactref element="ARD3" pad="D12"/>
</signal>
<signal name="D13">
<contactref element="ARD1" pad="D13"/>
<contactref element="ARD2" pad="D13"/>
<contactref element="ARD3" pad="D13"/>
</signal>
<signal name="A0">
<contactref element="ARD1" pad="A0"/>
<contactref element="ARD2" pad="A0"/>
<contactref element="ARD3" pad="A0"/>
</signal>
<signal name="A1">
<contactref element="ARD1" pad="A1"/>
<contactref element="ARD2" pad="A1"/>
<contactref element="ARD3" pad="A1"/>
</signal>
<signal name="A2">
<contactref element="ARD1" pad="A2"/>
<contactref element="ARD2" pad="A2"/>
<contactref element="ARD3" pad="A2"/>
</signal>
<signal name="A3">
<contactref element="ARD1" pad="A3"/>
<contactref element="ARD2" pad="A3"/>
<contactref element="ARD3" pad="A3"/>
</signal>
<signal name="A4">
<contactref element="ARD1" pad="A4"/>
<contactref element="ARD2" pad="A4"/>
<contactref element="ARD3" pad="A4"/>
</signal>
<signal name="A5">
<contactref element="ARD1" pad="A5"/>
<contactref element="ARD2" pad="A5"/>
<contactref element="ARD3" pad="A5"/>
</signal>
<signal name="5V">
<contactref element="ARD2" pad="5V"/>
<contactref element="ARD1" pad="5V"/>
<contactref element="ARD3" pad="5V"/>
</signal>
<signal name="3V3">
<contactref element="ARD1" pad="3V3"/>
<contactref element="ARD2" pad="3.3V"/>
<contactref element="ARD3" pad="3.3V"/>
</signal>
<signal name="GND">
<contactref element="ARD1" pad="GND@2"/>
<contactref element="ARD2" pad="GND@1"/>
<contactref element="ARD1" pad="GND@1"/>
<contactref element="ARD2" pad="GND@2"/>
<contactref element="ARD2" pad="GND@0"/>
<contactref element="ARD3" pad="GND@2"/>
<contactref element="ARD3" pad="GND@0"/>
<contactref element="ARD3" pad="GND@1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="AREF">
<contactref element="ARD1" pad="REF"/>
<contactref element="ARD2" pad="AREF"/>
<contactref element="ARD3" pad="AREF"/>
</signal>
<signal name="RST">
<contactref element="ARD2" pad="RES"/>
<contactref element="ARD1" pad="RST@1"/>
<contactref element="ARD1" pad="RST@2"/>
<contactref element="ARD3" pad="RES"/>
</signal>
<signal name="D0">
<contactref element="ARD1" pad="D0RX"/>
<contactref element="ARD2" pad="RX"/>
<contactref element="ARD3" pad="RX"/>
</signal>
<signal name="D1">
<contactref element="ARD1" pad="D1TX"/>
<contactref element="ARD2" pad="TX"/>
<contactref element="ARD3" pad="TX"/>
</signal>
<signal name="A7">
<contactref element="ARD1" pad="A7"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="A6">
<contactref element="ARD1" pad="A6"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="ARD2" pad="VIN"/>
<contactref element="ARD1" pad="VIN"/>
<contactref element="ARD3" pad="VIN"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$1">
<contactref element="CON" pad="PWR"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="CON" pad="GND"/>
<contactref element="D2" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
