<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="49.51" y2="0" width="0" layer="20"/>
<wire x1="49.51" y1="0" x2="49.51" y2="36.5" width="0" layer="20"/>
<wire x1="49.51" y1="36.5" x2="0" y2="36.5" width="0" layer="20"/>
<wire x1="0" y1="36.5" x2="0" y2="0" width="0" layer="20"/>
<text>IN</text>
<text>GND</text>
<text>OUT</text>
<text>GND</text>
<text>7805</text>
<text>7805</text>
<text>7812</text>
<text>ARDUINO-5V</text>
<text>24V</text>
<text>BAT</text>
<text>AB9V</text>
<text>C1-470UF</text>
<text>C2-220UF</text>
<text>C3-470UF</text>
<text>C4-220UF</text>
<text>GND</text>
<text>12V OUT</text>
<text>R1</text>
<text>100</text>
<text>R2</text>
<text>100</text>
<text>SWITCH-1</text>
<text>SWITCH-2</text>
<text>driver VS here</text>
<text>skdungu pcb designs</text>
<text>motor control circuit</text>
<text>motor control circuit</text>
<text>motor control circuit</text>
<text>motor control circuit</text>
</plain>
<libraries>
<library name="tango">
<packages>
<package name="L7805">
</package>
</packages>
</library>
<library name="78xx_with_heatsink">
<description>&lt;b&gt;78xx/79xx voltage regulator in TO-220 package in a horizontal position with the FK231-SA220/DO-2 heatsink underneath&lt;/b&gt;</description>
<packages>
<package name="78XXH">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="battery">
<description>&lt;b&gt;Lithium Batteries and NC Accus&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="AB9V">
<description>&lt;B&gt;9-V BATTERY CLIP&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C5B4.5">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 4.5 mm, grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="7805" library="tango" package="L7805" value="-L7805"/>
<element name="7812" library="78xx_with_heatsink" package="78XXH" value=""/>
<element name="ARDUINO-5V" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="BAT" library="battery" package="AB9V" value="AB9V"/>
<element name="C1-470UF" library="capacitor-wima" package="C5B4.5" value=""/>
<element name="C2-220UF" library="capacitor-wima" package="C5B4.5" value=""/>
<element name="C3-470UF" library="capacitor-wima" package="C5B4.5" value=""/>
<element name="C4-220UF" library="capacitor-wima" package="C5B4.5" value=""/>
<element name="GND" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="12VOUT" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="100">
<attribute name="PROD_ID" value="RES-12181"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="100">
<attribute name="PROD_ID" value="RES-12181"/>
</element>
<element name="SWITCH-1" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="SWITCH-2" library="SparkFun-Connectors" package="1X01" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="BAT" pad="+"/>
<contactref element="7812" pad="IN"/>
<contactref element="C1-470UF" pad="1"/>
<contactref element="7805" pad="IN"/>
<contactref element="C3-470UF" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="7812" pad="OUT"/>
<contactref element="R1" pad="P$1"/>
<contactref element="C2-220UF" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="7805" pad="OUT"/>
<contactref element="R2" pad="P$1"/>
<contactref element="C4-220UF" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C3-470UF" pad="2"/>
<contactref element="C4-220UF" pad="2"/>
<contactref element="7805" pad="GND"/>
<contactref element="C1-470UF" pad="2"/>
<contactref element="C2-220UF" pad="2"/>
<contactref element="7812" pad="GND"/>
<contactref element="BAT" pad="-"/>
<contactref element="GND" pad="1"/>
</signal>
<signal name="12VOUT">
<contactref element="12VOUT" pad="1"/>
<contactref element="SWITCH-1" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="ARDUINO-5V">
<contactref element="ARDUINO-5V" pad="1"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
