<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="15.24" width="0" layer="20"/>
<wire x1="25.4" y1="15.24" x2="25.4" y2="0" width="0" layer="20"/>
<text>C1</text>
<text>D2</text>
<text>R1</text>
<text>R2</text>
<text>D1</text>
<text>R3</text>
<text>R4</text>
<text>ATtiny85</text>
<text>POWER</text>
<text>+</text>
<text>µ-USBasp V1.2</text>
<text>cpldcpu 06/2013</text>
<text>+</text>
<text>C2</text>
<text>R5</text>
<text>PGM</text>
<text>MOSI</text>
<text>NC</text>
<text>RST</text>
<text>SCK</text>
<text>MISO</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="tb_custom">
<description>Lotverbinder für die Platinenkante. Einseitig.</description>
<packages>
<package name="ISP_EDGE2X5_LONG">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U6" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="Tiny85-20-SMT">
<attribute name="PROD_ID" value="IC-09092"/>
<attribute name="VALUE" value="Tiny85-20-SMT"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="100n">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="USB-A-H" value="USB-A-H"/>
<element name="D1" library="SparkFun-DiscreteSemi" package="SOD-323" value="3.6V">
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SOD-323" value="3.6V">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="68">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="68">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0805" value="1k5">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="tb_custom" package="ISP_EDGE2X5_LONG" value="TB_ISPEDGE_2X5_LONG"/>
<element name="LED1" library="led" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0805" value="390">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="0805" value="390">
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="100n">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U6" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="D1" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="JP2" pad="GND"/>
<contactref element="LED1" pad="C"/>
<contactref element="U$1" pad="6"/>
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="8"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="5V">
<contactref element="U6" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="JP2" pad="VBUS"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="PB1">
<contactref element="U6" pad="6"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="NRES">
<contactref element="U6" pad="1"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="PB2">
<contactref element="U6" pad="7"/>
<contactref element="U$1" pad="7"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="PB0">
<contactref element="U6" pad="5"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="JP2" pad="D-"/>
<contactref element="D1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="JP2" pad="D+"/>
<contactref element="D2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="PB3">
<contactref element="R2" pad="2"/>
<contactref element="U6" pad="2"/>
</signal>
<signal name="PB4">
<contactref element="R1" pad="2"/>
<contactref element="U6" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
