<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="72.39" y2="0" width="0" layer="20"/>
<wire x1="72.39" y1="0" x2="72.39" y2="43.942" width="0" layer="20"/>
<wire x1="72.39" y1="43.942" x2="0" y2="43.942" width="0" layer="20"/>
<wire x1="0" y1="43.942" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="MegaRAM">
<description>Generated from &lt;b&gt;MegaRAM.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="0603">
<description>IPC 1608 chip</description>
</package>
<package name="COCOON_48BIT_WINGSIDE">
</package>
<package name="TSOP48">
<description>&lt;b&gt;48-Lead Thin Small Outline Package (TSOP)&lt;/b&gt; 12mm x 20mm SST Package Code: EK&lt;p&gt;
Source: http://www.sst.com/dotAsset/40687.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="MegaRAM" package="TSOP48" value="IS61-64WV204816"/>
<element name="IC2" library="MegaRAM" package="TSOP48" value="IS61-64WV204816"/>
<element name="J1" library="MegaRAM" package="COCOON_48BIT_WINGSIDE" value="COCOON_48BIT_WINGSIDE"/>
<element name="C3" library="MegaRAM" package="0603" value="0.1uF"/>
<element name="C1" library="MegaRAM" package="0603" value="0.1uF"/>
<element name="C2" library="MegaRAM" package="0603" value="0.1uF"/>
<element name="C4" library="MegaRAM" package="0603" value="0.1uF"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="13"/>
<contactref element="IC1" pad="37"/>
<contactref element="IC2" pad="13"/>
<contactref element="IC2" pad="37"/>
<contactref element="C4" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="GNDW2@1"/>
<contactref element="J1" pad="GNDW2@2"/>
<contactref element="J1" pad="GNDW1@4"/>
<contactref element="J1" pad="GNDW1@3"/>
<contactref element="J1" pad="GNDW1@2"/>
<contactref element="J1" pad="GNDW1@1"/>
</signal>
<signal name="3V3">
<contactref element="IC1" pad="12"/>
<contactref element="IC1" pad="36"/>
<contactref element="IC2" pad="12"/>
<contactref element="IC2" pad="36"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="J1" pad="3V3W2@1"/>
<contactref element="J1" pad="3V3W2@2"/>
<contactref element="J1" pad="3V3W1@3"/>
<contactref element="J1" pad="3V3W1@2"/>
<contactref element="J1" pad="3V3W1@1"/>
<contactref element="J1" pad="3V3W1@4"/>
</signal>
<signal name="A0">
<contactref element="IC1" pad="5"/>
<contactref element="IC2" pad="5"/>
<contactref element="J1" pad="B3@1"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="4"/>
<contactref element="IC2" pad="4"/>
<contactref element="J1" pad="A15@1"/>
</signal>
<signal name="A2">
<contactref element="IC1" pad="3"/>
<contactref element="IC2" pad="3"/>
<contactref element="J1" pad="B2@1"/>
</signal>
<signal name="A3">
<contactref element="IC1" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="J1" pad="A16@1"/>
</signal>
<signal name="A4">
<contactref element="IC1" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="J1" pad="B1@1"/>
</signal>
<signal name="A5">
<contactref element="IC1" pad="48"/>
<contactref element="IC2" pad="48"/>
<contactref element="J1" pad="A1@2"/>
</signal>
<signal name="A6">
<contactref element="IC1" pad="47"/>
<contactref element="IC2" pad="47"/>
<contactref element="J1" pad="A2@2"/>
</signal>
<signal name="A7">
<contactref element="IC1" pad="46"/>
<contactref element="IC2" pad="46"/>
<contactref element="J1" pad="A3@2"/>
</signal>
<signal name="A8">
<contactref element="IC1" pad="45"/>
<contactref element="IC2" pad="45"/>
<contactref element="J1" pad="A4@2"/>
</signal>
<signal name="A9">
<contactref element="IC1" pad="30"/>
<contactref element="IC2" pad="30"/>
<contactref element="J1" pad="B11@1"/>
</signal>
<signal name="A10">
<contactref element="IC1" pad="29"/>
<contactref element="IC2" pad="29"/>
<contactref element="J1" pad="B12@1"/>
</signal>
<signal name="A11">
<contactref element="IC1" pad="28"/>
<contactref element="IC2" pad="28"/>
<contactref element="J1" pad="A5@1"/>
</signal>
<signal name="A12">
<contactref element="IC1" pad="27"/>
<contactref element="IC2" pad="27"/>
<contactref element="J1" pad="B13@1"/>
</signal>
<signal name="A13">
<contactref element="IC1" pad="26"/>
<contactref element="IC2" pad="26"/>
<contactref element="J1" pad="A4@1"/>
</signal>
<signal name="A14">
<contactref element="IC1" pad="25"/>
<contactref element="IC2" pad="25"/>
<contactref element="J1" pad="A3@1"/>
</signal>
<signal name="A15">
<contactref element="IC1" pad="24"/>
<contactref element="IC2" pad="24"/>
<contactref element="J1" pad="A7@1"/>
</signal>
<signal name="A16">
<contactref element="IC1" pad="23"/>
<contactref element="IC2" pad="23"/>
<contactref element="J1" pad="B10@1"/>
</signal>
<signal name="A17">
<contactref element="IC1" pad="22"/>
<contactref element="IC2" pad="22"/>
<contactref element="J1" pad="A8@1"/>
</signal>
<signal name="A18">
<contactref element="IC1" pad="21"/>
<contactref element="IC2" pad="21"/>
<contactref element="J1" pad="B9@1"/>
</signal>
<signal name="A19">
<contactref element="IC1" pad="20"/>
<contactref element="IC2" pad="20"/>
<contactref element="J1" pad="A9@1"/>
</signal>
<signal name="A20">
<contactref element="IC1" pad="31"/>
<contactref element="IC2" pad="31"/>
<contactref element="J1" pad="A6@1"/>
</signal>
<signal name="!LB">
<contactref element="IC1" pad="42"/>
<contactref element="IC2" pad="42"/>
<contactref element="J1" pad="A7@2"/>
</signal>
<signal name="!UB">
<contactref element="IC1" pad="43"/>
<contactref element="IC2" pad="43"/>
<contactref element="J1" pad="A6@2"/>
</signal>
<signal name="!WE">
<contactref element="IC1" pad="18"/>
<contactref element="IC2" pad="18"/>
<contactref element="J1" pad="B8@1"/>
</signal>
<signal name="!OE">
<contactref element="IC1" pad="44"/>
<contactref element="IC2" pad="44"/>
<contactref element="J1" pad="A5@2"/>
</signal>
<signal name="D15">
<contactref element="IC1" pad="41"/>
<contactref element="IC2" pad="41"/>
<contactref element="J1" pad="A8@2"/>
</signal>
<signal name="D14">
<contactref element="IC1" pad="40"/>
<contactref element="IC2" pad="40"/>
<contactref element="J1" pad="A9@2"/>
</signal>
<signal name="D13">
<contactref element="IC1" pad="39"/>
<contactref element="IC2" pad="39"/>
<contactref element="J1" pad="A10@2"/>
</signal>
<signal name="D12">
<contactref element="IC1" pad="38"/>
<contactref element="IC2" pad="38"/>
<contactref element="J1" pad="A11@2"/>
</signal>
<signal name="D11">
<contactref element="IC1" pad="35"/>
<contactref element="IC2" pad="35"/>
<contactref element="J1" pad="A12@2"/>
</signal>
<signal name="D10">
<contactref element="IC1" pad="34"/>
<contactref element="IC2" pad="34"/>
<contactref element="J1" pad="A13@2"/>
</signal>
<signal name="D9">
<contactref element="IC1" pad="33"/>
<contactref element="IC2" pad="33"/>
<contactref element="J1" pad="A14@2"/>
</signal>
<signal name="D8">
<contactref element="IC1" pad="32"/>
<contactref element="IC2" pad="32"/>
<contactref element="J1" pad="A15@2"/>
</signal>
<signal name="D7">
<contactref element="IC1" pad="17"/>
<contactref element="IC2" pad="17"/>
<contactref element="J1" pad="A10@1"/>
</signal>
<signal name="D6">
<contactref element="IC1" pad="16"/>
<contactref element="IC2" pad="16"/>
<contactref element="J1" pad="B7@1"/>
</signal>
<signal name="D5">
<contactref element="IC1" pad="15"/>
<contactref element="IC2" pad="15"/>
<contactref element="J1" pad="A11@1"/>
</signal>
<signal name="D4">
<contactref element="IC1" pad="14"/>
<contactref element="IC2" pad="14"/>
<contactref element="J1" pad="B6@1"/>
</signal>
<signal name="D3">
<contactref element="IC1" pad="11"/>
<contactref element="IC2" pad="11"/>
<contactref element="J1" pad="A12@1"/>
</signal>
<signal name="D2">
<contactref element="IC1" pad="10"/>
<contactref element="IC2" pad="10"/>
<contactref element="J1" pad="B5@1"/>
</signal>
<signal name="D1">
<contactref element="IC1" pad="9"/>
<contactref element="IC2" pad="9"/>
<contactref element="J1" pad="A13@1"/>
</signal>
<signal name="D0">
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="8"/>
<contactref element="J1" pad="B4@1"/>
</signal>
<signal name="!CS2">
<contactref element="IC2" pad="7"/>
<contactref element="J1" pad="A16@2"/>
</signal>
<signal name="N$49">
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="!CS1">
<contactref element="IC1" pad="7"/>
<contactref element="J1" pad="A14@1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
