<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.48" y2="0" width="0" layer="20"/>
<wire x1="30.48" y1="0" x2="30.48" y2="22.86" width="0" layer="20"/>
<wire x1="30.48" y1="22.86" x2="0" y2="22.86" width="0" layer="20"/>
<wire x1="0" y1="22.86" x2="0" y2="0" width="0" layer="20"/>
<text>PMOS
high side
driver v1
ki-co.uk</text>
</plain>
<libraries>
<library name="kingswood">
<description>Kingswood custom parts</description>
<packages>
<package name="SOT23">
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="PAD_R_25_12">
</package>
<package name="PAD_R_20_09">
</package>
<package name="SOIC8">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="kingswood" package="SOT23" value="FDN337N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="kingswood" package="SOT23" value="FDN337N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="kingswood" package="SOT23" value="FDN337N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="kingswood" package="SOT23" value="FDN337N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="kingswood" package="R0603" value="3k3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="kingswood" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="kingswood" package="R0603" value="3k3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="kingswood" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="kingswood" package="R0603" value="3k3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="kingswood" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="kingswood" package="R0603" value="3k3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="kingswood" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="kingswood" package="PAD_R_25_12" value="Out1">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="TP10" library="kingswood" package="PAD_R_20_09" value="GND">
<attribute name="VALUE"/>
</element>
<element name="TP11" library="kingswood" package="PAD_R_20_09" value="In3">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="TP12" library="kingswood" package="PAD_R_20_09" value="In4">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="kingswood" package="PAD_R_25_12" value="Out2">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="+V" library="kingswood" package="PAD_R_25_12" value="+V1">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="kingswood" package="PAD_R_20_09" value="GND">
<attribute name="VALUE"/>
</element>
<element name="TP5" library="kingswood" package="PAD_R_20_09" value="In1">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="TP6" library="kingswood" package="PAD_R_20_09" value="In2">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="TP7" library="kingswood" package="PAD_R_25_12" value="Out3">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="kingswood" package="PAD_R_25_12" value="Out4">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="TP9" library="kingswood" package="PAD_R_25_12" value="+V2">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="kingswood" package="SOIC8" value="IRF7316">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="kingswood" package="SOIC8" value="IRF7316">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="kingswood" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="kingswood" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="kingswood" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="kingswood" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="R13" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="RX6">
<contactref element="R23" pad="1"/>
<contactref element="R22" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="V1">
<contactref element="R13" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="+V" pad="PAD"/>
</signal>
<signal name="N$4">
<contactref element="R12" pad="1"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R22" pad="1"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="Q2" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="TP4" pad="PAD"/>
<contactref element="Q4" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="TP10" pad="PAD"/>
<contactref element="R11" pad="1"/>
<contactref element="R41" pad="1"/>
<contactref element="R31" pad="1"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="TP5" pad="PAD"/>
<contactref element="Q1" pad="3"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="TP6" pad="PAD"/>
<contactref element="Q2" pad="3"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="OUT1">
<contactref element="U1" pad="7"/>
<contactref element="TP1" pad="PAD"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="OUT2">
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="6"/>
<contactref element="TP2" pad="PAD"/>
</signal>
<signal name="N$11">
<contactref element="R33" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R43" pad="1"/>
<contactref element="R42" pad="2"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="V2">
<contactref element="R33" pad="2"/>
<contactref element="R43" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="TP9" pad="PAD"/>
</signal>
<signal name="N$14">
<contactref element="R32" pad="1"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R42" pad="1"/>
<contactref element="Q4" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="TP11" pad="PAD"/>
<contactref element="Q3" pad="3"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="TP12" pad="PAD"/>
<contactref element="Q4" pad="3"/>
<contactref element="R41" pad="2"/>
</signal>
<signal name="OUT4">
<contactref element="U2" pad="7"/>
<contactref element="TP7" pad="PAD"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="OUT3">
<contactref element="U2" pad="5"/>
<contactref element="U2" pad="6"/>
<contactref element="TP8" pad="PAD"/>
</signal>
<signal name="+V1">
</signal>
</signals>
</board>
</drawing>
</eagle>
