<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.15" y2="0" width="0" layer="20"/>
<wire x1="30.15" y1="0" x2="30.15" y2="42.154" width="0" layer="20"/>
<wire x1="30.15" y1="42.154" x2="0" y2="42.154" width="0" layer="20"/>
<wire x1="0" y1="42.154" x2="0" y2="0" width="0" layer="20"/>
<text>+</text>
<text>+5</text>
<text>GND</text>
<text>GND</text>
<text>SIG</text>
<text>NO</text>
<text>NC</text>
<text>PWR</text>
<text>SIG</text>
<hole x="27.686" y="40.005" drill="2.8"/>
<hole x="27.94" y="2.032" drill="2.8"/>
<hole x="2.286" y="2.032" drill="2.8"/>
<hole x="2.286" y="40.005" drill="2.8"/>
<text>B</text>
<text>C</text>
<text>E</text>
</plain>
<libraries>
<library name="relay">
<description>&lt;b&gt;Relays&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Eichhoff
&lt;li&gt;Finder
&lt;li&gt;Fujitsu
&lt;li&gt;HAMLIN
&lt;li&gt;OMRON
&lt;li&gt;Matsushita
&lt;li&gt;NAiS
&lt;li&gt;Siemens
&lt;li&gt;Schrack
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DS2Y">
<description>&lt;b&gt;MINIATURE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0023.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMB-DIODE">
<description>&lt;b&gt;Diode&lt;/b&gt;&lt;p&gt;
Basic small signal diode good up to 200mA. SMB footprint. Common part #: BAS16</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="LED-1206">
</package>
<package name="0805">
</package>
<package name="PTC-1206">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMB">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="02P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="04P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="03P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P1-20">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="K2" library="relay" package="DS2Y" value="DS2Y-S-DC5V">
<attribute name="OC_NEWARK" value="13P3268"/>
<attribute name="MPN" value="DS2Y-S-DC5V"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="D2" library="SparkFun" package="SMB-DIODE" value=""/>
<element name="Q1" library="SparkFun" package="SOT23" value=""/>
<element name="LED1" library="SparkFun" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="SparkFun" package="PTC-1206" value="PTCSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="diode" package="SMB" value=""/>
<element name="SL1" library="con-amp-quick" package="02P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SL2" library="con-amp-quick" package="04P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SL3" library="con-amp-quick" package="03P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER" library="testpad" package="P1-20" value="PTR1PAD1-20">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SIGNAL" library="testpad" package="P1-20" value="PTR1PAD1-20">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="testpad" package="P1-20" value="PTR1PAD1-20">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="R3" library="SparkFun" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="SL1" pad="1"/>
<contactref element="F1" pad="1"/>
<contactref element="POWER" pad="TP"/>
</signal>
<signal name="GNDA">
<contactref element="SL1" pad="2"/>
<contactref element="D3" pad="A"/>
<contactref element="Q1" pad="2"/>
<contactref element="SL3" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="GND" pad="TP"/>
</signal>
<signal name="+5V">
<contactref element="F1" pad="2"/>
<contactref element="D3" pad="C"/>
<contactref element="R1" pad="1"/>
<contactref element="K2" pad="1"/>
<contactref element="D2" pad="C"/>
<contactref element="SL3" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="K2" pad="16"/>
<contactref element="Q1" pad="3"/>
<contactref element="D2" pad="A"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="SL3" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="SIGNAL" pad="TP"/>
</signal>
<signal name="N$8">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="K2" pad="11"/>
<contactref element="SL2" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="K2" pad="13"/>
<contactref element="SL2" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="K2" pad="4"/>
<contactref element="SL2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="K2" pad="8"/>
<contactref element="SL2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="LED2" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
