<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="101.58" y2="0" width="0" layer="20"/>
<wire x1="101.58" y1="0" x2="101.58" y2="53.645" width="0" layer="20"/>
<wire x1="101.58" y1="53.645" x2="0" y2="53.645" width="0" layer="20"/>
<wire x1="0" y1="53.645" x2="0" y2="0" width="0" layer="20"/>
<hole x="10.16" y="50.8" drill="2"/>
<hole x="15.24" y="21.59" drill="2"/>
<text>MicroSD</text>
<text>XB0</text>
<text>XB1</text>
<text>L</text>
<text>FIX</text>
<text>RSSI</text>
<text>SD</text>
<text>PWR</text>
<text>TX</text>
<text>RX</text>
<text>3.3V</text>
<text>RSSI</text>
<text>GND</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>RESET</text>
<text>GPS</text>
<text>BZR</text>
<text>L</text>
<text>GPSANT</text>
<text>XB1</text>
<text>XB0</text>
<text>X</text>
<text>Y</text>
<text>Z</text>
<text>C1</text>
<text>C2</text>
<text>C3</text>
<text>C4</text>
<text>V</text>
<text>OpenSourceAerospace.com</text>
<text>RocketMega R2.1</text>
<text>Open Source Hardware</text>
<text>XBee</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="kurt">
<description>My Lib.</description>
<packages>
<package name="LGA16-4X4">
<description>16 Terminal LGA in a 4mm x 4mm package</description>
</package>
<package name="LGA14">
<description>LGA14 package 5mm x 3mm</description>
</package>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-PTH-NS">
</package>
<package name="U.FL">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AYZ0202">
<description>&lt;b&gt;DPDT Slide Switch SMD&lt;/b&gt;
www.SparkFun.com SKU : Comp-SMDS</description>
</package>
<package name="BUZZER-CCV">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO016">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE_ALT">
</package>
</packages>
</library>
<library name="zortness">
<description>Zortness' library&lt;br&gt;
&lt;a href="https://github.com/zortness/zort-eagle-library"&gt;GitHub&lt;/a&gt;</description>
<packages>
<package name="LFCSP-16">
</package>
<package name="1X6TERMINALBLOCK">
<description>&lt;b&gt;1x6 Terminal Block at 0.01" (2.54mm) pitch&lt;/b&gt;&lt;br/&gt;
&lt;a href="http://www.digikey.com/product-detail/en/282834-5/A98336-ND/1153266"&gt;DigiKey&lt;/a&gt;</description>
</package>
<package name="1206X4RESISTORARRAY">
<description>&lt;b&gt;1206 4x Resistor Array (Vishay S Series)&lt;/b&gt;&lt;br/&gt;
Used by Vishay thick film resistor arrays with 4 elements and longer end terminals.&lt;br/&gt;
&lt;a href="http://www.digikey.com/product-detail/en/CRA06S0831K00JTA/CRA6S81.0KCT-ND/1285879"&gt;DigiKey Vishay 1k x 4&lt;/a&gt;&lt;br/&gt;
&lt;a href="http://www.vishay.com/docs/31002/cra06es.pdf"&gt;Datasheet&lt;/a&gt;</description>
</package>
<package name="MICROSD">
<description>&lt;b&gt;MicroSD Connector&lt;/b&gt;&lt;br/&gt;
&lt;a href="http://www.digikey.com/product-detail/en/693071010811/732-3819-1-ND/3124603"&gt;DigiKey&lt;/a&gt;&lt;br/&gt;
&lt;a href="http://katalog.we-online.de/em/datasheet/693071010811.pdf"&gt;datasheet&lt;/a&gt;</description>
</package>
<package name="BMP180">
<description>&lt;b&gt;BMP180 Modified LGA7&lt;/b&gt;&lt;br/&gt;
&lt;a href="http://www.digikey.com/product-detail/en/BMP180/828-1027-1-ND/2688260"&gt;DigiKey&lt;/a&gt;&lt;br/&gt;
&lt;a href="http://ae-bst.resource.bosch.com/media/products/dokumente/bmp180/BST-BMP180-DS000-08.pdf"&gt;Datasheet&lt;/a&gt;</description>
</package>
<package name="TACTILE_KMR2">
<description>&lt;b&gt;KMR 2 Tactile Switch&lt;/b&gt;&lt;br/&gt;
Pad for KMR 2-Series tactile switches.&lt;br/&gt;
&lt;a href="http://www.digikey.com/product-search/en?FV=ffec3f7a"&gt;KMR 2 Series at DigiKey&lt;/a&gt;&lt;br/&gt;
&lt;a href="http://www.digikey.com/product-detail/en/KMR231NG%20LFS/CKN10246CT-ND/2176497"&gt;KMR231NGLFS&lt;/a&gt;</description>
</package>
<package name="ARDUINO_MEGA">
<description>Full Arduino MEGA footprint</description>
</package>
<package name="OSAEROSPACE_V">
</package>
<package name="XBEE">
</package>
<package name="POWERPAK1212-8">
<description>Vishay PowerPAK 1212-8 single device package&lt;br&gt;
High-power, low thermal resistance package.</description>
</package>
<package name="FGPMMOPA6H">
</package>
<package name="DPAK">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J3" library="zortness" package="XBEE" value="XBEE"/>
<element name="J4" library="zortness" package="MICROSD" value="MICROSD"/>
<element name="U3" library="zortness" package="FGPMMOPA6H" value="FGPMMOPA6H">
<attribute name="NAME"/>
</element>
<element name="U6" library="kurt" package="LGA16-4X4" value="L3GD20TR">
<attribute name="NAME"/>
</element>
<element name="U5" library="kurt" package="LGA14" value="LSM303DLHCTR">
<attribute name="NAME"/>
</element>
<element name="U1" library="zortness" package="DPAK" value="NCP1117DT33G">
<attribute name="NAME"/>
</element>
<element name="Q3" library="kurt" package="SOT23" value="BSS138">
<attribute name="NAME"/>
</element>
<element name="Q2" library="kurt" package="SOT23" value="BSS138">
<attribute name="NAME"/>
</element>
<element name="C6" library="adafruit" package="C1210" value="100uF16V">
<attribute name="NAME"/>
</element>
<element name="C5" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="J2" library="zortness" package="ARDUINO_MEGA" value="Mega R3"/>
<element name="J1" library="SparkFun-Connectors" package="JST-2-PTH-NS" value="ExtBatt">
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="U.FL" value="U.FL"/>
<element name="C11" library="adafruit" package="C1206" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C12" library="adafruit" package="C1206" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C13" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C14" library="adafruit" package="C1206" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C10" library="adafruit" package="C1206" value="0.22uF">
<attribute name="NAME"/>
</element>
<element name="C20" library="adafruit" package="C1206" value="0.01uF">
<attribute name="NAME"/>
</element>
<element name="C15" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C16" library="adafruit" package="C1206" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C8" library="adafruit" package="C1206" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C9" library="adafruit" package="C1206" value="0.01uF">
<attribute name="NAME"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED-1206" value="Fix - blue"/>
<element name="C1" library="adafruit" package="C1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="adafruit" package="C1206" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="D6" library="SparkFun-LED" package="LED-1206" value="PWR - green"/>
<element name="D4" library="SparkFun-LED" package="LED-1206" value="RSSI - yellow"/>
<element name="S2" library="SparkFun-Electromechanical" package="AYZ0202" value="AYZ0202">
<attribute name="NAME"/>
</element>
<element name="C7" library="adafruit" package="C1206" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="D5" library="SparkFun-LED" package="LED-1206" value="SDAct - orange"/>
<element name="U2" library="SparkFun-DigitalIC" package="SO016" value="M74HC4050M">
<attribute name="NAME"/>
</element>
<element name="Q7" library="zortness" package="POWERPAK1212-8" value="SI7112DN">
<attribute name="PROD_ID" value="TRANS-11055"/>
<attribute name="NAME"/>
</element>
<element name="Q4" library="zortness" package="POWERPAK1212-8" value="SI7112DN">
<attribute name="PROD_ID" value="TRANS-11055"/>
<attribute name="NAME"/>
</element>
<element name="Q6" library="zortness" package="POWERPAK1212-8" value="SI7112DN">
<attribute name="PROD_ID" value="TRANS-11055"/>
<attribute name="NAME"/>
</element>
<element name="Q5" library="zortness" package="POWERPAK1212-8" value="SI7112DN">
<attribute name="PROD_ID" value="TRANS-11055"/>
<attribute name="NAME"/>
</element>
<element name="U7" library="zortness" package="LFCSP-16" value="ADXL377">
<attribute name="NAME"/>
</element>
<element name="C21" library="adafruit" package="C1206" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C19" library="adafruit" package="C1206" value="0.01uF">
<attribute name="NAME"/>
</element>
<element name="C17" library="adafruit" package="C1206" value="0.01uF">
<attribute name="NAME"/>
</element>
<element name="C18" library="adafruit" package="C1206" value="0.01uF">
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE_ALT" value="STTH102A"/>
<element name="C4" library="adafruit" package="C1210" value="220uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="adafruit" package="C1206" value="100uF">
<attribute name="NAME"/>
</element>
<element name="J6" library="zortness" package="1X6TERMINALBLOCK" value="1X6TERMINALBLOCK"/>
<element name="D10" library="SparkFun-LED" package="LED-1206" value="Pyro4 - red"/>
<element name="D9" library="SparkFun-LED" package="LED-1206" value="Pyro3 - red"/>
<element name="D8" library="SparkFun-LED" package="LED-1206" value="Pyro2 - red"/>
<element name="D7" library="SparkFun-LED" package="LED-1206" value="Pyro1 - red"/>
<element name="RA1" library="zortness" package="1206X4RESISTORARRAY" value="330">
<attribute name="NAME"/>
</element>
<element name="RA6" library="zortness" package="1206X4RESISTORARRAY" value="10k">
<attribute name="NAME"/>
</element>
<element name="RA4" library="zortness" package="1206X4RESISTORARRAY" value="620k">
<attribute name="NAME"/>
</element>
<element name="RA3" library="zortness" package="1206X4RESISTORARRAY" value="100k">
<attribute name="NAME"/>
</element>
<element name="RA5" library="zortness" package="1206X4RESISTORARRAY" value="330">
<attribute name="NAME"/>
</element>
<element name="RA2" library="zortness" package="1206X4RESISTORARRAY" value="10k">
<attribute name="NAME"/>
</element>
<element name="R2" library="adafruit" package="R1206" value="620k">
<attribute name="NAME"/>
</element>
<element name="R1" library="adafruit" package="R1206" value="100k">
<attribute name="NAME"/>
</element>
<element name="U4" library="zortness" package="BMP180" value="BMP180">
<attribute name="NAME"/>
</element>
<element name="S1" library="zortness" package="TACTILE_KMR2" value="KMR2"/>
<element name="R4" library="adafruit" package="R1206" value="10k">
<attribute name="NAME"/>
</element>
<element name="SG1" library="SparkFun-Electromechanical" package="BUZZER-CCV" value="CCV084"/>
<element name="D2" library="SparkFun-LED" package="LED-1206" value="13 - red"/>
<element name="R3" library="adafruit" package="R1206" value="330">
<attribute name="NAME"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="Q1" library="zortness" package="POWERPAK1212-8" value="SI7112DN">
<attribute name="PROD_ID" value="TRANS-11055"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="zortness" package="OSAEROSPACE_V" value="OSAEROSPACEVECTOR"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="J2" pad="GND@3"/>
<contactref element="J2" pad="GND@0"/>
<contactref element="J2" pad="GND@1"/>
<contactref element="J2" pad="GND@2"/>
<contactref element="J2" pad="GND@4"/>
<contactref element="J1" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="U5" pad="7"/>
<contactref element="U5" pad="11"/>
<contactref element="U5" pad="10"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="U6" pad="P$13"/>
<contactref element="U6" pad="P$8"/>
<contactref element="U6" pad="P$12"/>
<contactref element="U6" pad="P$11"/>
<contactref element="U6" pad="P$10"/>
<contactref element="U6" pad="P$9"/>
<contactref element="C20" pad="2"/>
<contactref element="J5" pad="P$1"/>
<contactref element="J5" pad="P$2"/>
<contactref element="U3" pad="P$8"/>
<contactref element="U3" pad="P$3"/>
<contactref element="C15" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U3" pad="P$19"/>
<contactref element="U3" pad="P$12"/>
<contactref element="C16" pad="2"/>
<contactref element="J3" pad="10"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="J4" pad="MT1"/>
<contactref element="J4" pad="6"/>
<contactref element="J4" pad="MT2"/>
<contactref element="C7" pad="2"/>
<contactref element="J4" pad="CD2"/>
<contactref element="J4" pad="CD1"/>
<contactref element="U2" pad="8"/>
<contactref element="U7" pad="7"/>
<contactref element="U7" pad="6"/>
<contactref element="C21" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="Q6" pad="S1"/>
<contactref element="Q6" pad="S2"/>
<contactref element="Q6" pad="S3"/>
<contactref element="Q5" pad="S1"/>
<contactref element="Q5" pad="S2"/>
<contactref element="Q5" pad="S3"/>
<contactref element="Q4" pad="S1"/>
<contactref element="Q4" pad="S2"/>
<contactref element="Q4" pad="S3"/>
<contactref element="Q7" pad="S1"/>
<contactref element="Q7" pad="S2"/>
<contactref element="Q7" pad="S3"/>
<contactref element="D6" pad="C"/>
<contactref element="D5" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="RA3" pad="1"/>
<contactref element="RA3" pad="2"/>
<contactref element="RA3" pad="3"/>
<contactref element="RA3" pad="4"/>
<contactref element="RA2" pad="8"/>
<contactref element="RA2" pad="7"/>
<contactref element="RA2" pad="6"/>
<contactref element="RA2" pad="5"/>
<contactref element="D10" pad="C"/>
<contactref element="D9" pad="C"/>
<contactref element="D8" pad="C"/>
<contactref element="D7" pad="C"/>
<contactref element="R1" pad="1"/>
<contactref element="U4" pad="7"/>
<contactref element="U4" pad="7"/>
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="R4" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="Q1" pad="S1"/>
<contactref element="Q1" pad="S2"/>
<contactref element="Q1" pad="S3"/>
</signal>
<signal name="VCC3">
<contactref element="U1" pad="4"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="14"/>
<contactref element="C13" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="U6" pad="P$1"/>
<contactref element="U6" pad="P$15"/>
<contactref element="U6" pad="P$16"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="U3" pad="P$1"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="J4" pad="4"/>
<contactref element="C7" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="U7" pad="15"/>
<contactref element="U7" pad="14"/>
<contactref element="C21" pad="1"/>
<contactref element="RA1" pad="4"/>
<contactref element="RA6" pad="3"/>
<contactref element="RA6" pad="4"/>
<contactref element="U4" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="U4" pad="3"/>
<contactref element="SG1" pad="-"/>
</signal>
<signal name="MEGASDA">
<contactref element="Q2" pad="3"/>
<contactref element="J2" pad="20"/>
<contactref element="RA6" pad="8"/>
</signal>
<signal name="MEGASCL">
<contactref element="Q3" pad="3"/>
<contactref element="J2" pad="21"/>
<contactref element="RA6" pad="7"/>
</signal>
<signal name="SDA">
<contactref element="Q2" pad="2"/>
<contactref element="U5" pad="3"/>
<contactref element="U6" pad="P$3"/>
<contactref element="RA6" pad="5"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="SCL">
<contactref element="Q3" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="U6" pad="P$2"/>
<contactref element="RA6" pad="6"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="MEGA5V">
<contactref element="J2" pad="5V@0"/>
</signal>
<signal name="MEGAA0">
<contactref element="J2" pad="A0"/>
</signal>
<signal name="MEGAA1">
<contactref element="J2" pad="A1"/>
</signal>
<signal name="MEGAA2">
<contactref element="J2" pad="A2"/>
</signal>
<signal name="N$7">
<contactref element="C12" pad="1"/>
<contactref element="U5" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="C10" pad="2"/>
<contactref element="U5" pad="12"/>
</signal>
<signal name="N$6">
<contactref element="C10" pad="1"/>
<contactref element="U5" pad="13"/>
</signal>
<signal name="N$8">
<contactref element="U6" pad="P$14"/>
<contactref element="C20" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U3" pad="P$11"/>
<contactref element="J5" pad="P$3"/>
</signal>
<signal name="MEGARX1">
<contactref element="J2" pad="19"/>
<contactref element="S2" pad="6"/>
</signal>
<signal name="MEGARX2">
<contactref element="J2" pad="17"/>
<contactref element="U3" pad="P$9"/>
</signal>
<signal name="MEGARX0">
<contactref element="J2" pad="0"/>
<contactref element="S2" pad="4"/>
</signal>
<signal name="MEGATX0">
<contactref element="J2" pad="1"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="MEGATX1">
<contactref element="J2" pad="18"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="MEGATX2">
<contactref element="J2" pad="16"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="TX0">
<contactref element="S2" pad="1"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="TX1">
<contactref element="U2" pad="4"/>
<contactref element="S2" pad="3"/>
</signal>
<signal name="XRSSI">
<contactref element="J3" pad="6"/>
<contactref element="RA1" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="S2" pad="5"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="J3" pad="3"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="SDCS">
<contactref element="J4" pad="2"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="MEGASDCS">
<contactref element="J2" pad="48"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="MEGASCLK">
<contactref element="J2" pad="52"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="MEGAMOSI">
<contactref element="J2" pad="51"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="MEGAMISO">
<contactref element="J2" pad="50"/>
<contactref element="J4" pad="7"/>
</signal>
<signal name="SCLK">
<contactref element="J4" pad="5"/>
<contactref element="U2" pad="12"/>
<contactref element="RA1" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="J4" pad="3"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="IOREF">
<contactref element="J2" pad="IOREF"/>
<contactref element="RA6" pad="1"/>
<contactref element="RA6" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="J2" pad="RESET"/>
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="J2" pad="VIN"/>
<contactref element="D1" pad="C"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="BATT+">
<contactref element="J1" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="J6" pad="2"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="Q7" pad="D1"/>
<contactref element="Q7" pad="D2"/>
<contactref element="Q7" pad="D3"/>
<contactref element="Q7" pad="D4"/>
<contactref element="Q7" pad="DPAD"/>
<contactref element="J6" pad="3"/>
<contactref element="RA4" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="Q4" pad="D1"/>
<contactref element="Q4" pad="D2"/>
<contactref element="Q4" pad="D3"/>
<contactref element="Q4" pad="D4"/>
<contactref element="Q4" pad="DPAD"/>
<contactref element="J6" pad="4"/>
<contactref element="RA4" pad="6"/>
</signal>
<signal name="N$24">
<contactref element="J6" pad="6"/>
<contactref element="Q5" pad="D1"/>
<contactref element="Q5" pad="D2"/>
<contactref element="Q5" pad="D3"/>
<contactref element="Q5" pad="D4"/>
<contactref element="Q5" pad="DPAD"/>
<contactref element="RA4" pad="8"/>
</signal>
<signal name="PYRO2">
<contactref element="J2" pad="43"/>
<contactref element="Q4" pad="G"/>
<contactref element="RA2" pad="2"/>
<contactref element="RA5" pad="2"/>
</signal>
<signal name="PYRO1">
<contactref element="J2" pad="42"/>
<contactref element="Q7" pad="G"/>
<contactref element="RA2" pad="1"/>
<contactref element="RA5" pad="1"/>
</signal>
<signal name="PYRO3">
<contactref element="J2" pad="44"/>
<contactref element="Q6" pad="G"/>
<contactref element="RA2" pad="3"/>
<contactref element="RA5" pad="3"/>
</signal>
<signal name="PYRO4">
<contactref element="J2" pad="45"/>
<contactref element="Q5" pad="G"/>
<contactref element="RA2" pad="4"/>
<contactref element="RA5" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="RA1" pad="5"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="RA1" pad="6"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="RA1" pad="7"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="RA1" pad="8"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="GPSFIX">
<contactref element="U3" pad="P$5"/>
<contactref element="RA1" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="Q6" pad="D4"/>
<contactref element="Q6" pad="D2"/>
<contactref element="Q6" pad="D1"/>
<contactref element="Q6" pad="D3"/>
<contactref element="Q6" pad="DPAD"/>
<contactref element="J6" pad="5"/>
<contactref element="RA4" pad="7"/>
</signal>
<signal name="MEGAA3">
<contactref element="J2" pad="A3"/>
</signal>
<signal name="MEGAA4">
<contactref element="J2" pad="A4"/>
<contactref element="RA4" pad="4"/>
<contactref element="RA3" pad="5"/>
</signal>
<signal name="MEGAA5">
<contactref element="J2" pad="A5"/>
<contactref element="RA4" pad="3"/>
<contactref element="RA3" pad="6"/>
</signal>
<signal name="MEGAA6">
<contactref element="J2" pad="A6"/>
<contactref element="RA4" pad="2"/>
<contactref element="RA3" pad="7"/>
</signal>
<signal name="TX2">
<contactref element="U2" pad="6"/>
<contactref element="U3" pad="P$10"/>
</signal>
<signal name="N$16">
<contactref element="RA5" pad="5"/>
<contactref element="D10" pad="A"/>
</signal>
<signal name="N$17">
<contactref element="RA5" pad="6"/>
<contactref element="D9" pad="A"/>
</signal>
<signal name="N$18">
<contactref element="RA5" pad="7"/>
<contactref element="D8" pad="A"/>
</signal>
<signal name="N$19">
<contactref element="RA5" pad="8"/>
<contactref element="D7" pad="A"/>
</signal>
<signal name="N$33">
</signal>
<signal name="N$34">
</signal>
<signal name="MEGAA7">
<contactref element="J2" pad="A7"/>
<contactref element="RA4" pad="1"/>
<contactref element="RA3" pad="8"/>
</signal>
<signal name="MEGAA8">
<contactref element="J2" pad="A8"/>
<contactref element="U7" pad="16"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="MEGAA9">
<contactref element="J2" pad="A9"/>
<contactref element="U7" pad="4"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="MEGAA10">
<contactref element="J2" pad="A10"/>
<contactref element="U7" pad="5"/>
<contactref element="C19" pad="1"/>
</signal>
<signal name="MEGAA11">
<contactref element="J2" pad="A11"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="MEGAA12">
<contactref element="J2" pad="A12"/>
</signal>
<signal name="MEGAA13">
<contactref element="J2" pad="A13"/>
</signal>
<signal name="MEGAA14">
<contactref element="J2" pad="A14"/>
</signal>
<signal name="MEGAA15">
<contactref element="J2" pad="A15"/>
</signal>
<signal name="N$13">
<contactref element="SG1" pad="+"/>
<contactref element="Q1" pad="D4"/>
<contactref element="Q1" pad="D2"/>
<contactref element="Q1" pad="D1"/>
<contactref element="Q1" pad="D3"/>
<contactref element="Q1" pad="DPAD"/>
</signal>
<signal name="MEGA8">
<contactref element="J2" pad="8"/>
<contactref element="R4" pad="1"/>
<contactref element="Q1" pad="G"/>
</signal>
<signal name="N$9">
<contactref element="J2" pad="13"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="D2" pad="A"/>
<contactref element="R3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
