<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<text>GND</text>
<text>VIN</text>
<text>SIG_GND</text>
<text>VOUT</text>
<text>VS+</text>
<text>VS-</text>
<text>SMB</text>
<text>TRIM</text>
<text>SEQ</text>
<text>CLK</text>
<text>GND1</text>
<text>DATA</text>
<text>ADDR1</text>
<text>ADDR0</text>
<text>ON/OFF</text>
<text>PGOOD</text>
<wire x1="-1.754228125" y1="18.71505625" x2="19.511196875" y2="18.7194625" width="0.4064" layer="20"/>
<wire x1="19.511196875" y1="18.7194625" x2="19.514603125" y2="-1.661928125" width="0.4064" layer="20"/>
<wire x1="19.514603125" y1="-1.661928125" x2="-1.754228125" y2="-1.644440625" width="0.4064" layer="20"/>
<wire x1="-1.754228125" y1="-1.644440625" x2="-1.754228125" y2="18.71505625" width="0.4064" layer="20"/>
<text>PDT012A0X BREAKOUT</text>
<text>C1TRUZ</text>
</plain>
<libraries>
<library name="NEWBUCK">
<packages>
<package name="GEPICO">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$1" library="NEWBUCK" package="GEPICO" value=""/>
<element name="E$2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="E$3" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="E$4" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="E$5" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VIN">
<contactref element="E$2" pad="1"/>
<contactref element="E$1" pad="VIN"/>
</signal>
<signal name="S$3">
<contactref element="E$2" pad="4"/>
<contactref element="E$1" pad="VOUT"/>
</signal>
<signal name="S$4">
<contactref element="E$5" pad="4"/>
<contactref element="E$1" pad="VS+"/>
</signal>
<signal name="S$5">
<contactref element="E$5" pad="3"/>
<contactref element="E$1" pad="VS-"/>
</signal>
<signal name="S$6">
<contactref element="E$5" pad="2"/>
<contactref element="E$1" pad="SMB"/>
</signal>
<signal name="S$7">
<contactref element="E$5" pad="1"/>
<contactref element="E$1" pad="TRIM"/>
</signal>
<signal name="S$8">
<contactref element="E$3" pad="4"/>
<contactref element="E$1" pad="DATA"/>
</signal>
<signal name="S$10">
<contactref element="E$3" pad="2"/>
<contactref element="E$1" pad="CLK"/>
</signal>
<signal name="S$11">
<contactref element="E$3" pad="1"/>
<contactref element="E$1" pad="SEA"/>
</signal>
<signal name="S$12">
<contactref element="E$4" pad="1"/>
<contactref element="E$1" pad="PGOOD"/>
</signal>
<signal name="S$13">
<contactref element="E$4" pad="2"/>
<contactref element="E$1" pad="ON"/>
</signal>
<signal name="S$14">
<contactref element="E$4" pad="3"/>
<contactref element="E$1" pad="ADDR0"/>
</signal>
<signal name="S$15">
<contactref element="E$4" pad="4"/>
<contactref element="E$1" pad="ADDR1"/>
</signal>
<signal name="S$16">
<contactref element="E$2" pad="3"/>
<contactref element="E$1" pad="SGND"/>
</signal>
<signal name="GND">
<contactref element="E$3" pad="3"/>
<contactref element="E$1" pad="GND1"/>
<contactref element="E$1" pad="SYNC"/>
<contactref element="E$2" pad="2"/>
<contactref element="E$1" pad="GND"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
