<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="-0.254" y1="-0.254" x2="29.515" y2="-0.254" width="0" layer="20"/>
<wire x1="29.515" y1="-0.254" x2="29.515" y2="18.151" width="0" layer="20"/>
<wire x1="29.515" y1="18.151" x2="-0.254" y2="18.151" width="0" layer="20"/>
<wire x1="-0.254" y1="18.151" x2="-0.254" y2="-0.254" width="0" layer="20"/>
<text>GND</text>
<text>PA0</text>
<text>PA1</text>
<text>PA2</text>
<text>PA3</text>
<text>PA4</text>
<text>PA5</text>
<text>PA6</text>
<text>PA7</text>
<text>VCC</text>
<text>VCC</text>
<text>SWCLK</text>
<text>GND</text>
<text>SWDIO</text>
<text>NRST</text>
<text>PB0</text>
<text>PWR</text>
<text>PA9</text>
<text>GND</text>
<text>PA10</text>
<text>PA15</text>
<text>PB1</text>
<text>PB3</text>
<text>PB4</text>
<text>PB5</text>
<text>PB6</text>
<text>PB7</text>
<text>STM32F0
Test Board
Chris Elwood
2013</text>
</plain>
<libraries>
<library name="chris_stuff">
<packages>
<package name="LQFP-32">
<description>&lt;b&gt;Quad Flat Package&lt;/b&gt; 32 LD LQFP&lt;p&gt;
Source: ds232b12.pdf&lt;br&gt;
http://www.ftdichip.com</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10">
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-SMD-5X3">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="chris_stuff" package="LQFP-32" value="STM32F051X">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IO1" library="SparkFun-Connectors" package="1X10" value="M10&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IO2" library="SparkFun-Connectors" package="1X10" value="M10&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SWD" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF"/>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF"/>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="LED1" library="SparkFun-LED" package="LED-0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="Y1" library="SparkFun-FreqCtrl" package="CRYSTAL-SMD-5X3" value=""/>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="4.7uF"/>
<element name="C4" library="SparkFun-Capacitors" package="0603-CAP" value="18pF"/>
<element name="C5" library="SparkFun-Capacitors" package="0603-CAP" value="18pF"/>
<element name="SJ1" library="SparkFun-Passives" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="C6" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="Y1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="Y1" pad="3"/>
<contactref element="U1" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="C3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="SWD" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="C6" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="17"/>
<contactref element="IO1" pad="10"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="31"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="SWCLK">
<contactref element="SWD" pad="2"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="SWDIO">
<contactref element="SWD" pad="4"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="NRST">
<contactref element="SWD" pad="5"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="PB7">
<contactref element="U1" pad="30"/>
<contactref element="IO2" pad="10"/>
</signal>
<signal name="PB6">
<contactref element="U1" pad="29"/>
<contactref element="IO2" pad="9"/>
</signal>
<signal name="PB5">
<contactref element="U1" pad="28"/>
<contactref element="IO2" pad="8"/>
</signal>
<signal name="PB4">
<contactref element="U1" pad="27"/>
<contactref element="IO2" pad="7"/>
</signal>
<signal name="PB3">
<contactref element="U1" pad="26"/>
<contactref element="IO2" pad="6"/>
</signal>
<signal name="PA15">
<contactref element="U1" pad="25"/>
<contactref element="IO2" pad="4"/>
</signal>
<signal name="PA10">
<contactref element="U1" pad="20"/>
<contactref element="IO2" pad="3"/>
</signal>
<signal name="PA9">
<contactref element="U1" pad="19"/>
<contactref element="IO2" pad="2"/>
</signal>
<signal name="PA0">
<contactref element="U1" pad="6"/>
<contactref element="IO1" pad="2"/>
</signal>
<signal name="PA1">
<contactref element="U1" pad="7"/>
<contactref element="IO1" pad="3"/>
</signal>
<signal name="PA2">
<contactref element="U1" pad="8"/>
<contactref element="IO1" pad="4"/>
</signal>
<signal name="PA3">
<contactref element="U1" pad="9"/>
<contactref element="IO1" pad="5"/>
</signal>
<signal name="PA4">
<contactref element="U1" pad="10"/>
<contactref element="IO1" pad="6"/>
</signal>
<signal name="PA5">
<contactref element="U1" pad="11"/>
<contactref element="IO1" pad="7"/>
</signal>
<signal name="PA6">
<contactref element="U1" pad="12"/>
<contactref element="IO1" pad="8"/>
</signal>
<signal name="PA7">
<contactref element="U1" pad="13"/>
<contactref element="IO1" pad="9"/>
</signal>
<signal name="N$23">
<contactref element="U1" pad="14"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="PB1">
<contactref element="U1" pad="15"/>
<contactref element="IO2" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="IO1" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="16"/>
<contactref element="C6" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="32"/>
<contactref element="SJ1" pad="2"/>
<contactref element="SWD" pad="3"/>
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="18"/>
<contactref element="IO2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
