<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="64.8309" y1="53.3451" x2="0.0071" y2="53.3451" width="0" layer="20"/>
<wire x1="64.8309" y1="53.3451" x2="66.5581" y2="51.6276" width="0" layer="20"/>
<wire x1="66.5581" y1="40.4821" x2="66.5581" y2="51.6276" width="0" layer="20"/>
<wire x1="66.5581" y1="40.4821" x2="69.1613" y2="37.9421" width="0" layer="20"/>
<wire x1="69.1359" y1="5.0413" x2="69.1359" y2="5.0489" width="0" layer="20"/>
<wire x1="69.1359" y1="5.0489" x2="69.1613" y2="37.9421" width="0" layer="20"/>
<wire x1="66.5581" y1="2.4943" x2="69.1359" y2="5.0489" width="0" layer="20"/>
<wire x1="66.5581" y1="2.4943" x2="66.548" y2="0" width="0" layer="20"/>
<wire x1="0.0033" y1="-0.0057" x2="0.0071" y2="53.3451" width="0" layer="20"/>
<text>RST</text>
<text>3v</text>
<text>5v</text>
<text>Gnd</text>
<text>Vin</text>
<text>Analog In</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>ARef</text>
<text>gnd</text>
<text>13</text>
<text>12</text>
<text>11</text>
<text>10</text>
<text>9</text>
<text>8</text>
<text>7</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>0</text>
<text>Digital I/O</text>
<text>Digital I/O</text>
<wire x1="0" y1="0" x2="66.548" y2="0" width="0" layer="20"/>
<text>Gnd</text>
<text>Gnd</text>
<text>+5v</text>
<text>tCs1</text>
<text>tDo</text>
<text>Gnd</text>
<text>A_Gnd</text>
<text>tClk</text>
<text>tCs0</text>
<text>dPos</text>
<text>rstr1</text>
<text>LED-</text>
<text>Ptr Tx</text>
<text>Ptr RX</text>
<text>zCrs</text>
<text>gate</text>
<text>Gnd</text>
<text>pwr</text>
<text>htr</text>
<text>rstr2</text>
<text>panel</text>
<text>+12v</text>
<text>+12V</text>
<text>fanSpd</text>
<text>drumSpd</text>
<text>Gnd</text>
<text>+5v</text>
<text>+12v</text>
<text>Gnd</text>
<text>+5v</text>
<text>usrBtn</text>
<text>i2dat</text>
<text>i2clk</text>
<text>encA</text>
<text>encB</text>
<text>select</text>
<text>RoasterShield V1.6</text>
<text>Drum Control</text>
<text>Fan Control</text>
<text>21 Sep 2014</text>
<text>LED+</text>
<text>www.roasthacker.com</text>
<text>HV Signal</text>
<text>LV Signal</text>
<text>In</text>
<text>Out</text>
<text>Gnd</text>
<text>3.3v</text>
</plain>
<libraries>
<library name="carduino">
<packages>
<package name="1X08-CLEANBIG">
</package>
<package name="1X06-CLEANBIG">
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220">
<description>&lt;b&gt;TO 220 horizontal&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="1X04_LOCK">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X16">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Evan">
<packages>
<package name="5X6BOB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP3" library="carduino" package="1X08-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="carduino" package="1X08-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="carduino" package="1X06-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JP8" library="carduino" package="1X06-CLEANBIG" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="transistor" package="TO220" value="TIP122"/>
<element name="T2" library="transistor" package="TO220" value="TIP122">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="AXIAL-0.4" value="22K"/>
<element name="D1" library="diode" package="DO41-10" value="1N4004"/>
<element name="D2" library="diode" package="DO41-10" value="1N4004"/>
<element name="R2" library="SparkFun" package="AXIAL-0.4" value="2.2K"/>
<element name="R3" library="SparkFun" package="AXIAL-0.4" value="2.2K"/>
<element name="JP12" library="pinhead" package="2X16" value=""/>
<element name="JP1" library="SparkFun" package="1X04_LOCK" value=""/>
<element name="BOB-1" library="Evan" package="5X6BOB" value="BOB-08745DEFAULT"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP3" pad="2"/>
<contactref element="JP6" pad="2"/>
<contactref element="JP6" pad="3"/>
<contactref element="JP12" pad="3"/>
<contactref element="JP12" pad="9"/>
<contactref element="JP12" pad="4"/>
<contactref element="JP12" pad="14"/>
<contactref element="BOB-1" pad="9"/>
<contactref element="JP12" pad="2"/>
<contactref element="JP12" pad="28"/>
</signal>
<signal name="+5V">
<contactref element="R1" pad="P$2"/>
<contactref element="JP6" pad="4"/>
<contactref element="JP12" pad="5"/>
<contactref element="JP12" pad="11"/>
<contactref element="JP12" pad="6"/>
<contactref element="BOB-1" pad="10"/>
<contactref element="JP12" pad="32"/>
</signal>
<signal name="+12V">
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="JP12" pad="7"/>
<contactref element="JP12" pad="25"/>
<contactref element="JP12" pad="31"/>
</signal>
<signal name="N$9">
<contactref element="JP5" pad="6"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="AGND">
<contactref element="T2" pad="3"/>
<contactref element="T1" pad="3"/>
<contactref element="JP12" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="P$1"/>
<contactref element="T2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="P$2"/>
<contactref element="JP5" pad="7"/>
</signal>
<signal name="N$13">
<contactref element="R3" pad="P$1"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="JP3" pad="4"/>
<contactref element="JP12" pad="10"/>
</signal>
<signal name="N$3">
<contactref element="JP5" pad="5"/>
<contactref element="JP12" pad="21"/>
</signal>
<signal name="N$14">
<contactref element="JP12" pad="8"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="R1" pad="P$1"/>
<contactref element="JP5" pad="3"/>
<contactref element="JP12" pad="24"/>
</signal>
<signal name="N$7">
<contactref element="JP3" pad="5"/>
<contactref element="JP12" pad="12"/>
</signal>
<signal name="N$27">
<contactref element="JP12" pad="23"/>
<contactref element="JP5" pad="4"/>
</signal>
<signal name="N$28">
<contactref element="JP12" pad="29"/>
<contactref element="T2" pad="2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$29">
<contactref element="JP12" pad="27"/>
<contactref element="T1" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="JP12" pad="16"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="JP12" pad="18"/>
<contactref element="JP5" pad="8"/>
</signal>
<signal name="N$8">
<contactref element="JP3" pad="6"/>
<contactref element="JP12" pad="13"/>
</signal>
<signal name="N$2">
<contactref element="JP3" pad="7"/>
<contactref element="JP12" pad="26"/>
</signal>
<signal name="N$10">
<contactref element="JP8" pad="1"/>
<contactref element="JP12" pad="19"/>
</signal>
<signal name="N$11">
<contactref element="JP8" pad="5"/>
<contactref element="JP12" pad="15"/>
</signal>
<signal name="N$15">
<contactref element="JP8" pad="6"/>
<contactref element="JP12" pad="17"/>
</signal>
<signal name="N$16">
<contactref element="JP8" pad="2"/>
<contactref element="JP12" pad="22"/>
</signal>
<signal name="N$17">
<contactref element="JP8" pad="3"/>
<contactref element="JP12" pad="20"/>
</signal>
<signal name="N$18">
<contactref element="JP8" pad="4"/>
<contactref element="JP12" pad="30"/>
</signal>
<signal name="HEATSINK1">
</signal>
<signal name="HEATSINK2">
</signal>
<signal name="ARD-RX">
<contactref element="JP5" pad="1"/>
<contactref element="BOB-1" pad="7"/>
</signal>
<signal name="N$20">
<contactref element="JP5" pad="2"/>
<contactref element="BOB-1" pad="8"/>
</signal>
<signal name="N$21">
<contactref element="JP1" pad="3"/>
<contactref element="BOB-1" pad="4"/>
</signal>
<signal name="N$22">
<contactref element="JP1" pad="4"/>
<contactref element="BOB-1" pad="3"/>
</signal>
<signal name="N$23">
<contactref element="JP1" pad="2"/>
<contactref element="BOB-1" pad="5"/>
</signal>
<signal name="N$24">
<contactref element="JP1" pad="1"/>
<contactref element="BOB-1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
