<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="58.09" y2="0" width="0" layer="20"/>
<wire x1="58.09" y1="0" x2="58.09" y2="48.25" width="0" layer="20"/>
<wire x1="58.09" y1="48.25" x2="0" y2="48.25" width="0" layer="20"/>
<wire x1="0" y1="48.25" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.54" y="45.72" drill="3.2"/>
<hole x="2.54" y="2.54" drill="3.2"/>
<hole x="55.88" y="2.54" drill="3.2"/>
<hole x="55.88" y="45.72" drill="3.2"/>
<text>Adafruit ST7565
Rev A
04/13/15
elb</text>
</plain>
<libraries>
<library name="40xx">
<description>&lt;b&gt;CMOS Logic Devices, 4000 Series&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola &lt;i&gt;CMOS LOGIC DATA&lt;/i&gt;; book, 02/88, DL131 REV 1
&lt;li&gt;http://www.elexp.com
&lt;li&gt;http://www.intersil.com
&lt;li&gt;http://www.ls3c.com.tw/product/1/COMOS.html
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X5-SHROUDED">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="elb">
<packages>
<package name="ROTARY_ENC_PLAIN">
<description>Simple rotary encoder, no LED, push center&lt;br&gt;
COM-09117</description>
</package>
<package name="1X11_2MM">
</package>
<package name="F/QMBIII">
<description>&lt;b&gt;BUZZER&lt;/b&gt;</description>
</package>
<package name="SD_1:1">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="v-reg-3">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;/p&gt;
&lt;p&gt;&lt;date&gt;2008-05-16&lt;/date&gt;, updates by &lt;author&gt;Eike Schmidt&lt;/author&gt;&lt;/p&gt;&lt;ul&gt;&lt;li&gt;integrated library "ltc_swr.lbr" with switching regulators from &lt;a href=http://www.linear.com&gt;Linear Technology&lt;/a&gt;, created by &lt;author&gt;Claudius Stern&lt;/author&gt;&lt;/li&gt;&lt;li&gt;added step-down switching regulator LT1767&lt;/li&gt;&lt;li&gt;combined identical symbols for positive regulators&lt;/li&gt;&lt;li&gt;added packages SO8 and SOT89 for 78Lxx and 79Lxx&lt;/li&gt;&lt;li&gt;added package SO8 for LM317L and LM337L&lt;/li&gt;&lt;li&gt;added linear regulators L4931, L4949E, LM2931&lt;/li&gt;&lt;li&gt;added micropower, ultra-low dropout family LP298x&lt;/li&gt;&lt;li&gt;added ultra-low dropout regulators IRU1205, TK112, TK113&lt;/li&gt;&lt;li&gt;added low power, low dropout regulator family S-812&lt;/li&gt;&lt;li&gt;added NPN "Simple Switcher"(c) family LM257x&lt;/li&gt;&lt;li&gt;added DMOS "Simple Switcher"(c) family LM267x&lt;/li&gt;&lt;li&gt;added NPN Darlington switching regulator MC34063A&lt;/li&gt;&lt;li&gt;added LED boost drivers PR4401, PR4402, PR4403&lt;/li&gt;&lt;/ul&gt;</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AA</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="40xx" package="SO16" value="4050D"/>
<element name="JP1" library="SparkFun-Connectors" package="2X5-SHROUDED" value="EXP1">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="2X5-SHROUDED" value="EXP2">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SW1" library="elb" package="ROTARY_ENC_PLAIN" value="ROTARTY_ENCODER">
<attribute name="NAME"/>
</element>
<element name="U$1" library="elb" package="1X11_2MM" value="1X11_2MM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="SG1" library="elb" package="F/QMBIII" value="BUZZER">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="BLUE" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK" value="Blue"/>
<element name="GREEN" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK" value="Green"/>
<element name="RED" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK" value="Red"/>
<element name="U1" library="elb" package="SD_1:1" value="SD_CARD_SOCKET">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Passives" package="1206" value="0.1uF"/>
<element name="C4" library="SparkFun-Passives" package="1206" value="2.2uF"/>
<element name="IC2" library="v-reg-3" package="SO08" value="L4931D-GNDPIN7"/>
<element name="Q3" library="SparkFun-DiscreteSemi" package="SOT23-3" value="2N7002">
<attribute name="PROD_ID" value="TRANS-08345"/>
</element>
<element name="Q4" library="SparkFun-DiscreteSemi" package="SOT23-3" value="2N7002">
<attribute name="PROD_ID" value="TRANS-08345"/>
</element>
<element name="R1" library="SparkFun-Passives" package="1206" value="4.7k"/>
<element name="R2" library="SparkFun-Passives" package="1206" value="4.7k"/>
<element name="C1" library="SparkFun-Passives" package="1206" value="1 uF"/>
</elements>
<signals>
<signal name="+5V">
<contactref element="JP1" pad="1"/>
<contactref element="SG1" pad="+"/>
<contactref element="C3" pad="1"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="D29">
<contactref element="JP1" pad="3"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="D35">
<contactref element="JP1" pad="9"/>
<contactref element="SW1" pad="B"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="SW1" pad="SW+"/>
<contactref element="S1" pad="1"/>
<contactref element="U$1" pad="7"/>
<contactref element="IC1" pad="14"/>
<contactref element="U1" pad="SH@3"/>
<contactref element="U1" pad="SH@1"/>
<contactref element="U1" pad="SH@2"/>
<contactref element="U1" pad="SH@4"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="6"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="IC2" pad="7"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="SW1" pad="C"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="D27">
<contactref element="JP1" pad="4"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="D37">
<contactref element="JP1" pad="10"/>
<contactref element="SW1" pad="A"/>
</signal>
<signal name="+3.3V">
<contactref element="IC1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="9"/>
<contactref element="U1" pad="4"/>
<contactref element="IC2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="LCD_CS">
<contactref element="IC1" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="LCD_A0">
<contactref element="IC1" pad="4"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="SG1" pad="-"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="D41">
<contactref element="S1" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="D49">
<contactref element="JP2" pad="4"/>
<contactref element="U1" pad="CD"/>
</signal>
<signal name="D31">
<contactref element="JP2" pad="8"/>
<contactref element="SW1" pad="SW-"/>
</signal>
<signal name="D51">
<contactref element="JP2" pad="5"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="6"/>
<contactref element="U$1" pad="5"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="D52">
<contactref element="JP2" pad="9"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="D53">
<contactref element="JP2" pad="7"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="SD_CS">
<contactref element="IC1" pad="10"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="SCLK">
<contactref element="IC1" pad="12"/>
<contactref element="U$1" pad="4"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="D33">
<contactref element="JP2" pad="6"/>
<contactref element="Q4" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="8"/>
<contactref element="RED" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="10"/>
<contactref element="GREEN" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="11"/>
<contactref element="BLUE" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="BLUE" pad="1"/>
<contactref element="GREEN" pad="1"/>
<contactref element="RED" pad="1"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="D23">
<contactref element="JP1" pad="6"/>
<contactref element="Q3" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="D50">
<contactref element="JP2" pad="10"/>
<contactref element="U1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
