<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.46" y2="0" width="0" layer="20"/>
<wire x1="30.46" y1="0" x2="30.46" y2="12.37" width="0" layer="20"/>
<wire x1="30.46" y1="12.37" x2="0" y2="12.37" width="0" layer="20"/>
<wire x1="0" y1="12.37" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>OUTPUT</text>
<text>INPUT+</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD4-7">
<description>&lt;b&gt;SMD 4&lt;/b&gt; Option 7&lt;p&gt;
Source:&lt;a href=" http://www.vishay.com/docs/83673/sfh618.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="OK1" library="optocoupler" package="SMD4-7" value="SFH6186-2">
<attribute name="OC_NEWARK" value="58K2210"/>
<attribute name="MPN" value="SFH6186-2"/>
<attribute name="MF" value="VISHAY/TELEFUNKEN"/>
<attribute name="OC_FARNELL" value="1469583"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="OK1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="OK1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="JP2" pad="1"/>
<contactref element="OK1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="JP2" pad="2"/>
<contactref element="OK1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
