<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="63.5" y2="0" width="0" layer="20"/>
<wire x1="63.5" y1="0" x2="63.5" y2="48.26" width="0" layer="20"/>
<wire x1="63.5" y1="48.26" x2="0" y2="48.26" width="0" layer="20"/>
<wire x1="0" y1="48.26" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.8" y="45.43" drill="2.8"/>
<hole x="59.2" y="45.33" drill="2.8"/>
<hole x="4.4" y="3.73" drill="2.8"/>
<hole x="59.7" y="3.03" drill="2.8"/>
<text>NOTE: All pads and mounting holes
offset to match drill errors on mainboard.</text>
<text>Nutube 6P1 Shield for Headphone Amp</text>
<text>ChrisU @ 2016-11-05</text>
<text>F1</text>
<text>F1</text>
<text>NC</text>
<text>G1</text>
<text>NC</text>
<text>NC</text>
<text>A1</text>
<text>GND</text>
<text>F2</text>
<text>A2</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>G2</text>
<text>NP</text>
<text>F3</text>
<text>F3</text>
<text>F1</text>
<text>F1</text>
<text>G1</text>
<text>A1</text>
<text>GND</text>
<text>F2</text>
<text>A2</text>
<text>G2</text>
<text>F3</text>
<text>F3</text>
</plain>
<libraries>
<library name="ccbtech-Noritake">
<packages>
<package name="NUTUBE_6P1">
</package>
</packages>
</library>
<library name="ccbtech-Connector">
<packages>
<package name="1X17_M2">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="ccbtech-Noritake" package="NUTUBE_6P1" value="NUTUBE_6P1">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="ccbtech-Connector" package="1X17_M2" value="1X17M02"/>
<element name="SW_IN" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW_OPT" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="P$1"/>
<contactref element="U$2" pad="P$01"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="P$7"/>
<contactref element="U$2" pad="P$07"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="P$9"/>
<contactref element="U$2" pad="P$09"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="P$10"/>
<contactref element="U$2" pad="P$10"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="P$14"/>
<contactref element="U$2" pad="P$14"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="P$17"/>
<contactref element="U$2" pad="P$17"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P$4"/>
<contactref element="U$2" pad="P$04"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="P$8"/>
<contactref element="U$2" pad="P$08"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P$2"/>
<contactref element="U$2" pad="P$02"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="P$16"/>
<contactref element="U$2" pad="P$16"/>
</signal>
<signal name="N$10">
<contactref element="SW_OPT" pad="3"/>
<contactref element="SW_IN" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="SW_OPT" pad="2"/>
<contactref element="SW_IN" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="SW_OPT" pad="1"/>
<contactref element="SW_IN" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
