<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22.78" y2="0" width="0" layer="20"/>
<wire x1="22.78" y1="0" x2="22.78" y2="75.5" width="0" layer="20"/>
<wire x1="22.78" y1="75.5" x2="0" y2="75.5" width="0" layer="20"/>
<wire x1="0" y1="75.5" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.5" y="73" drill="1"/>
<hole x="20.28" y="73" drill="1"/>
<text>CC1101</text>
<text>GDO2</text>
<text>MISO</text>
<text>SCLK</text>
<text>MOSI</text>
<text>GDO0</text>
<text>CSN</text>
<text>VCC</text>
<text>GND</text>
<text>VCC</text>
<text>GND</text>
<text>1.0</text>
<text>1.1</text>
<text>1.2</text>
<text>3.0</text>
<text>3.1</text>
<text>3.2</text>
<text>3.3</text>
<text>4.7</text>
<text>1.3</text>
<text>1.4</text>
<text>1.5</text>
<text>J0</text>
<text>J1</text>
<text>J2</text>
<text>J3</text>
<text>4.0</text>
<text>VCC</text>
<text>GND</text>
<text>4.6</text>
<text>4.5</text>
<text>4.4</text>
<text>1.7</text>
<text>1.6</text>
<text>3.7</text>
<text>3.6</text>
<text>3.5</text>
<text>3.4</text>
<text>2.2</text>
<text>2.1</text>
<text>2.0</text>
<text>RST</text>
<text>2.6</text>
<text>2.5</text>
<text>TST</text>
<text>BREAKOUT
POWER</text>
<hole x="2.5" y="2.5" drill="1"/>
<hole x="20.28" y="2.5" drill="1"/>
<text>Design by:
Jeremy Wilder</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>X</text>
<text>Rated for
5 - 12V
.5 A</text>
<text>Version 1.2</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X18">
</package>
<package name="1X03_NO_SILK">
</package>
<package name="1X04_NO_SILK_ALL_ROUND">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="msp430">
<packages>
<package name="RGZ48_4P1X4P1">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="abs05">
<packages>
<package name="ABS05">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="2.2uF">
<attribute name="PROD_ID" value="CAP-07888"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="470pF">
<attribute name="PROD_ID" value="CAP-07884"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="9pF">
<attribute name="PROD_ID" value="CAP-09341"/>
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603-CAP" value="9pF">
<attribute name="PROD_ID" value="CAP-09341"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X18" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X18" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value="470"/>
<element name="R3" library="SparkFun-Passives" package="0603-RES" value="470"/>
<element name="U1" library="msp430" package="RGZ48_4P1X4P1" value="MSP430FR5969_RGZ_48">
<attribute name="VENDOR" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="msp430fr5969_rgz_48"/>
</element>
<element name="U2" library="SparkFun-PowerIC" package="SOT23-5" value="MIC5219 3.3V">
<attribute name="PROD_ID" value="VREG-09872"/>
</element>
<element name="X1" library="abs05" package="ABS05" value="ABS05-32.768KHZ-9-T">
<attribute name="DIGIKEY" value="535-11897-1-ND"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="470"/>
<element name="LED1" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="47"/>
<contactref element="U1" pad="44"/>
<contactref element="U1" pad="36"/>
<contactref element="J2" pad="2"/>
<contactref element="U1" pad="41"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="J4" pad="1"/>
<contactref element="J4" pad="2"/>
<contactref element="J4" pad="3"/>
<contactref element="J1" pad="17"/>
<contactref element="J6" pad="1"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="37"/>
<contactref element="U1" pad="48"/>
<contactref element="U2" pad="5"/>
<contactref element="C1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="18"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="TST">
<contactref element="U1" pad="22"/>
<contactref element="J2" pad="16"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="23"/>
<contactref element="J2" pad="15"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="A">
<contactref element="X1" pad="A"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="46"/>
</signal>
<signal name="B">
<contactref element="X1" pad="B"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="45"/>
</signal>
<signal name="3.0">
<contactref element="U1" pad="4"/>
<contactref element="J1" pad="13"/>
</signal>
<signal name="3.1">
<contactref element="U1" pad="5"/>
<contactref element="J1" pad="12"/>
</signal>
<signal name="3.2">
<contactref element="U1" pad="6"/>
<contactref element="J1" pad="11"/>
</signal>
<signal name="3.3">
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="4.7">
<contactref element="U1" pad="8"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="1.3">
<contactref element="U1" pad="9"/>
<contactref element="J1" pad="8"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="1.4">
<contactref element="U1" pad="10"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="1.5">
<contactref element="U1" pad="11"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="J.0">
<contactref element="U1" pad="12"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="1.7">
<contactref element="U1" pad="32"/>
<contactref element="J2" pad="6"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="1.6">
<contactref element="U1" pad="31"/>
<contactref element="J2" pad="7"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="3.5">
<contactref element="U1" pad="28"/>
<contactref element="J2" pad="10"/>
</signal>
<signal name="3.4">
<contactref element="U1" pad="27"/>
<contactref element="J2" pad="11"/>
<contactref element="J6" pad="4"/>
</signal>
<signal name="2.2">
<contactref element="U1" pad="26"/>
<contactref element="J2" pad="12"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="2.1">
<contactref element="U1" pad="25"/>
<contactref element="J2" pad="13"/>
</signal>
<signal name="J.1">
<contactref element="U1" pad="13"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="J.2">
<contactref element="U1" pad="14"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="J.3">
<contactref element="U1" pad="15"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="4.0">
<contactref element="U1" pad="16"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="4.1">
<contactref element="U1" pad="17"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="2.5">
<contactref element="U1" pad="20"/>
<contactref element="J2" pad="18"/>
</signal>
<signal name="2.6">
<contactref element="U1" pad="21"/>
<contactref element="J2" pad="17"/>
</signal>
<signal name="2.0">
<contactref element="U1" pad="24"/>
<contactref element="J2" pad="14"/>
</signal>
<signal name="N$1">
<contactref element="LED3" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="4.3">
<contactref element="U1" pad="19"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="4.2">
<contactref element="U1" pad="18"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U2" pad="4"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="5V">
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="J3" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="3.7">
<contactref element="U1" pad="30"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="4.4">
<contactref element="U1" pad="33"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="4.5">
<contactref element="J2" pad="4"/>
<contactref element="U1" pad="34"/>
</signal>
<signal name="4.6">
<contactref element="U1" pad="35"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="1.2">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="14"/>
</signal>
<signal name="1.1">
<contactref element="U1" pad="2"/>
<contactref element="J1" pad="15"/>
</signal>
<signal name="1.0">
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="16"/>
</signal>
<signal name="3.6">
<contactref element="J5" pad="4"/>
<contactref element="J2" pad="9"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
