<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="5.715" y1="3.81" x2="30.404" y2="3.81" width="0" layer="20"/>
<wire x1="30.404" y1="3.81" x2="30.404" y2="13.96" width="0" layer="20"/>
<wire x1="30.404" y1="13.96" x2="5.715" y2="13.96" width="0" layer="20"/>
<wire x1="5.715" y1="13.96" x2="5.715" y2="3.81" width="0" layer="20"/>
<text>IN</text>
<text>OUT</text>
<text>+</text>
<text>+</text>
<text>D</text>
<text>D</text>
<text>-</text>
<text>-</text>
<text>Bill Porter</text>
<text>PixelPeater</text>
</plain>
<libraries>
<library name="74xx-little-de">
<description>&lt;b&gt;Single and Dual Gates Family, US symbols&lt;/b&gt;&lt;p&gt;
Little logic devices from Texas Instruments&lt;br&gt;
TinyLogic(R) from FAIRCHILD Semiconductor TM
&lt;p&gt;
&lt;author&gt;Created by evgeni@eniks.com&lt;/author&gt;&lt;br&gt;
&lt;author&gt;Extended by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
SOT753 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT89">
<description>&lt;b&gt;SOT98&lt;/b&gt; PK (R-PDSO-G3)&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ua78l05.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LONGPADS">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="74xx-little-de" package="SOT23-5" value="74LVC1G17DBV"/>
<element name="IC2" library="linear" package="SOT89" value="MCP170312MB"/>
<element name="J1" library="SparkFun-Connectors" package="1X03_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X03_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="33"/>
<element name="R2" library="SparkFun-Resistors" package="0805" value="33"/>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="1u"/>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="2.2u"/>
<element name="C3" library="SparkFun-Capacitors" package="0805" value=".1u"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="3"/>
<contactref element="IC2" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="4"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="3"/>
<contactref element="IC2" pad="2@1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="5V">
<contactref element="IC1" pad="5"/>
<contactref element="IC2" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
