<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.4" y2="0" width="0.4064" layer="20"/>
<wire x1="25.4" y1="0" x2="25.4" y2="33.02" width="0.4064" layer="20"/>
<wire x1="25.4" y1="33.02" x2="0" y2="33.02" width="0.4064" layer="20"/>
<wire x1="0" y1="33.02" x2="0" y2="0" width="0.4064" layer="20"/>
<text>100k</text>
<text>100k</text>
<text>10uF</text>
<text>10uF</text>
<text>220</text>
<text>220</text>
<text>LED</text>
<text>LED</text>
<text>Put solder
paste here</text>
<text>NPN</text>
<text>NPN</text>
<text>20mm</text>
<text>2017</text>
<text>Small</text>
<text>Surface Mount Solder
Practice Board</text>
<text>     Instructions:
1) Apply Solder Paste
2) Place Components
3) Put in Reflow Oven</text>
<text>Designed by William Laney</text>
<text>Need 6V</text>
<text>Hall</text>
<text>Maker</text>
<text>Space</text>
<text>G</text>
<text>G</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="BAT-HLD-001-THM">
<packages>
<package name="LINX_BAT-HLD-001-THM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="10uF"/>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="10uF"/>
<element name="LED1" library="led" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT2222A">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT2222A">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="220"/>
<element name="R2" library="SparkFun-Passives" package="0805" value="220"/>
<element name="R3" library="SparkFun-Passives" package="0805" value="100k"/>
<element name="R4" library="SparkFun-Passives" package="0805" value="100k"/>
<element name="BT1" library="BAT-HLD-001-THM" package="LINX_BAT-HLD-001-THM" value="BAT-HLD-001-THM">
<attribute name="COST1000" value="0.196"/>
<attribute name="LINK_B" value="http://www.mouser.com/ProductDetail/Panasonic-Battery/CR2016/"/>
<attribute name="LINK" value="http://www.mouser.com/ProductDetail/Linx-Technologies/BAT-HLD-001-THM/"/>
<attribute name="COST1000_B" value="0.184"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="LED1" pad="C"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="C1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="LED2" pad="A"/>
<contactref element="LED1" pad="A"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="BT1" pad="+@3"/>
<contactref element="BT1" pad="+@1"/>
<contactref element="BT1" pad="+@2"/>
<contactref element="BT1" pad="+@4"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="BT1" pad="-"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
