<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="76.2" y2="0" width="0" layer="20"/>
<wire x1="76.2" y1="0" x2="76.2" y2="33.02" width="0" layer="20"/>
<wire x1="76.2" y1="33.02" x2="0" y2="33.02" width="0" layer="20"/>
<wire x1="0" y1="33.02" x2="0" y2="0" width="0" layer="20"/>
<text>Buck_MiniMega2560</text>
<text>5 Nov 2018
Ver 10_2e</text>
<text>RESET</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>RES</text>
<text>SCK</text>
<text>MISO</text>
<text>MOSI</text>
<text>SCL</text>
<text>SDA</text>
<text>TX0</text>
<text>RX0</text>
<text>PB6</text>
<text>PB4</text>
<text>RX2</text>
<text>TX2</text>
<text>PB7</text>
<text>PC6</text>
<text>PC5</text>
<text>RX1</text>
<text>TX1</text>
<text>RX3</text>
<text>TX3</text>
<text>PG5</text>
<text>AREF</text>
<text>VBAT</text>
<text>!SS</text>
<text>PH6</text>
<text>PH5</text>
<text>PH4</text>
<text>PH3</text>
<text>PE5</text>
<text>PE4</text>
<text>PB5</text>
<text>PA0</text>
<text>PA1</text>
<text>PA2</text>
<text>PA3</text>
<text>PE3</text>
<text>21</text>
<text>20</text>
<text>19</text>
<text>18</text>
<text>12</text>
<text>11</text>
<text>10</text>
<text>50</text>
<text>51</text>
<text>52</text>
<text>15</text>
<text>14</text>
<text>5</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>53</text>
<text>8</text>
<text>7</text>
<text>6</text>
<text>16</text>
<text>17</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>0</text>
<text>9</text>
<text>13</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>A4</text>
<text>A0</text>
<text>PA4</text>
<text>A5</text>
<text>PA5</text>
<text>A9</text>
<text>A10</text>
<text>A8</text>
<text>PK0</text>
<text>Cut RTS trace
Jumper DTR</text>
<text>GND</text>
<text>To change CP2104
RTS -&gt; DTR</text>
<text>VBUS</text>
<hole x="7.62" y="30.48" drill="1.016"/>
<text>GND</text>
<text>VCC</text>
<text>RESET</text>
<text>MISO</text>
<text>MOSI</text>
<text>SCK</text>
<text>PC7</text>
<text>PC4</text>
<text>PF0</text>
<text>PF1</text>
<text>PF2</text>
<text>PF3</text>
<text>PF4</text>
<text>PF5</text>
<text>A11</text>
<text>A15</text>
<text>PK1</text>
<text>PK2</text>
<text>PK3</text>
<text>PK7</text>
<text>4</text>
<text>32</text>
<text>31</text>
<text>30</text>
<text>22</text>
<text>23</text>
<text>24</text>
<text>25</text>
<text>26</text>
<text>27</text>
<text>33</text>
<text>smallmetalworks.com</text>
<text>RTS</text>
<text>DTR</text>
<text>REG__BAT</text>
<text>22</text>
<text>13</text>
<text>+</text>
<text>BAT</text>
<text>ENA.REG</text>
<text>ENA_REG</text>
<text>VCC</text>
<text>BAT</text>
<text>REG</text>
<text>https://www.richtek.com/assets/product_file/RT6222C=RT6222D/DS6222CD-01.pdf</text>
<text>Buck Reg Info</text>
</plain>
<libraries>
<library name="smartPrj">
<packages>
<package name="TQFP100">
<description>&lt;b&gt;100-lead Thin Quad Flat Pack Package Outline&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X24">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;map name="nav_main"&gt;
&lt;area shape="rect" coords="0,1,140,23" href="../military_specs.asp" title=""&gt;
&lt;area shape="rect" coords="0,24,140,51" href="../about.asp" title=""&gt;
&lt;area shape="rect" coords="1,52,140,77" href="../rfq.asp" title=""&gt;
&lt;area shape="rect" coords="0,78,139,103" href="../products.asp" title=""&gt;
&lt;area shape="rect" coords="1,102,138,128" href="../excess_inventory.asp" title=""&gt;
&lt;area shape="rect" coords="1,129,138,150" href="../edge.asp" title=""&gt;
&lt;area shape="rect" coords="1,151,139,178" href="../industry_links.asp" title=""&gt;
&lt;area shape="rect" coords="0,179,139,201" href="../comments.asp" title=""&gt;
&lt;area shape="rect" coords="1,203,138,231" href="../directory.asp" title=""&gt;
&lt;area shape="default" nohref&gt;
&lt;/map&gt;

&lt;html&gt;

&lt;title&gt;&lt;/title&gt;

 &lt;LINK REL="StyleSheet" TYPE="text/css" HREF="style-sheet.css"&gt;

&lt;body bgcolor="#ffffff" text="#000000" marginwidth="0" marginheight="0" topmargin="0" leftmargin="0"&gt;
&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0 height="55%"&gt;
&lt;tr valign="top"&gt;

&lt;/td&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/BODY&gt;&lt;/HTML&gt;</description>
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="KMR2">
</package>
<package name="JST-PH-2-THM-RA">
<description>&lt;b&gt;S2B-PH-K-S&lt;/b&gt; 
&lt;p&gt;
JST PH 2-pin thru-home side entry</description>
</package>
</packages>
</library>
<library name="UserItems">
<packages>
<package name="CRYSTAL-6X3.6">
<description>&lt;b&gt;Crystal 6x3.6 case&lt;/b&gt;</description>
</package>
<package name="QFN-24">
<description>&lt;h3&gt;24-pin QFN with Exposed Thermal pad&lt;/h3&gt;
For: &lt;li&gt;CP2104&lt;/li&gt;</description>
</package>
<package name="USB-MICROB-PTH">
<description>MicroUSB pin</description>
</package>
<package name="SOT143">
<description>&lt;b&gt;SOT-143&lt;/b&gt;</description>
</package>
<package name="POGOPAD">
</package>
<package name="PTC1812">
<description>&lt;b&gt;PTC&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="JUMP253">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JUMPER-SMT2">
<description>Small Solder Jumper pad</description>
</package>
<package name="INDUCTOR58">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="SOT23-6L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; 6 lead</description>
</package>
<package name="1206WC">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0805">
<description>0805</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOD323-W">
<description>&lt;b&gt;SOD323 Wave soldering&lt;/b&gt; Philips SC01_Mounting_1996.pdf</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ-BACK">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJ-BACK-LINK">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ATMEGA2560" library="smartPrj" package="TQFP100" value="ATMEGA2560"/>
<element name="JP1" library="pinhead" package="1X24" value="LEFT"/>
<element name="JP2" library="pinhead" package="1X24" value="RIGHT"/>
<element name="C1" library="resistor" package="C0603" value="22pf"/>
<element name="C2" library="resistor" package="C0603" value="22pf"/>
<element name="C3" library="resistor" package="C0603" value="0.1uf"/>
<element name="C4" library="resistor" package="C0603" value="0.1uf"/>
<element name="C5" library="resistor" package="C0603" value="0.1uf"/>
<element name="LPB7" library="adafruit" package="CHIPLED_0805" value="Yellow"/>
<element name="RPB7" library="resistor" package="R0603" value="820"/>
<element name="RPWR" library="resistor" package="R0603" value="820"/>
<element name="LPWR" library="adafruit" package="CHIPLED_0805" value="Yellow"/>
<element name="C8" library="resistor" package="C0603" value="0.1uf"/>
<element name="JP6" library="pinhead" package="1X06" value=""/>
<element name="C7" library="resistor" package="C0603" value="0.1uf"/>
<element name="C6" library="resistor" package="C0603K" value=".1uf"/>
<element name="RRES" library="resistor" package="R0603" value="10K"/>
<element name="RSDA" library="resistor" package="R0603" value="10k"/>
<element name="RSCL" library="resistor" package="R0603" value="10k"/>
<element name="SW2" library="adafruit" package="KMR2" value="SPST_TACT-KMR2"/>
<element name="Q1" library="UserItems" package="CRYSTAL-6X3.6" value=""/>
<element name="RPA0" library="resistor" package="R0603" value="820"/>
<element name="LPA0" library="adafruit" package="CHIPLED_0805" value="GREEN"/>
<element name="CP2104" library="UserItems" package="QFN-24" value="CP2104"/>
<element name="USB" library="UserItems" package="USB-MICROB-PTH" value="USB">
<attribute name="PROD_ID" value="USB1"/>
</element>
<element name="LTX" library="adafruit" package="CHIPLED_0805" value="Red"/>
<element name="LRX" library="adafruit" package="CHIPLED_0805" value="Green"/>
<element name="RRX" library="resistor" package="R0603" value="820"/>
<element name="RTX" library="resistor" package="R0603" value="820"/>
<element name="CV1" library="resistor" package="C0603K" value="0.1uf"/>
<element name="F1" library="UserItems" package="PTC1812" value="PTS181216V050"/>
<element name="SP5030" library="UserItems" package="SOT143" value="SP0503BAHTG"/>
<element name="RFG" library="resistor" package="R0603" value="1Meg"/>
<element name="CV2" library="resistor" package="C0603K" value="1uf"/>
<element name="CFG" library="resistor" package="C0603K" value="100pf"/>
<element name="CVPP" library="resistor" package="C0603K" value="4.7uf"/>
<element name="RRST" library="resistor" package="R0603" value="4.7K"/>
<element name="CREG" library="resistor" package="C0603K" value="1uf"/>
<element name="CN1" library="adafruit" package="JST-PH-2-THM-RA" value=""/>
<element name="D3" library="diode" package="SOD323-W" value="SS24FA"/>
<element name="D2" library="diode" package="SOD323-W" value="SS24FA"/>
<element name="SJ2" library="jumper" package="SJ-BACK-LINK" value=""/>
<element name="RPD2" library="resistor" package="R0603" value="1Meg"/>
<element name="U$1" library="UserItems" package="POGOPAD" value="POGOPAD"/>
<element name="U$2" library="UserItems" package="POGOPAD" value="POGOPAD"/>
<element name="U$3" library="UserItems" package="POGOPAD" value="POGOPAD"/>
<element name="U$4" library="UserItems" package="POGOPAD" value="POGOPAD"/>
<element name="U$5" library="UserItems" package="POGOPAD" value="POGOPAD"/>
<element name="U$6" library="UserItems" package="POGOPAD" value="POGOPAD"/>
<element name="SJ3" library="jumper" package="SJ-BACK" value=""/>
<element name="CI2" library="UserItems" package="1206WC" value=""/>
<element name="RURX" library="resistor" package="R0603" value="680"/>
<element name="RUTX" library="resistor" package="R0603" value="680"/>
<element name="JREG" library="pinhead" package="1X02" value=""/>
<element name="JPW" library="UserItems" package="JUMPER-SMT2" value="JUMPER-SMT2"/>
<element name="JDA" library="UserItems" package="JUMPER-SMT2" value="JUMPER-SMT2"/>
<element name="JCL" library="UserItems" package="JUMPER-SMT2" value="JUMPER-SMT2"/>
<element name="CO2" library="UserItems" package="1206WC" value=""/>
<element name="BAT__REG" library="UserItems" package="JUMP253" value=""/>
<element name="L1" library="UserItems" package="INDUCTOR58" value=""/>
<element name="R2" library="resistor" package="R0603" value=""/>
<element name="R1" library="resistor" package="R0603" value=""/>
<element name="CI1" library="UserItems" package="1206WC" value=""/>
<element name="CFF" library="resistor" package="C0603K" value=""/>
<element name="CO1" library="UserItems" package="1206WC" value=""/>
<element name="BUCK" library="UserItems" package="SOT23-6L" value=""/>
<element name="D1" library="diode" package="SOD323-W" value=""/>
<element name="CSW" library="resistor" package="C0805K" value=""/>
<element name="REN" library="resistor" package="R0603" value=""/>
<element name="FB1" library="UserItems" package="0805" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="ATMEGA2560" pad="11"/>
<contactref element="ATMEGA2560" pad="32"/>
<contactref element="ATMEGA2560" pad="62"/>
<contactref element="ATMEGA2560" pad="81"/>
<contactref element="ATMEGA2560" pad="99"/>
<contactref element="JP1" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="LPB7" pad="C"/>
<contactref element="SW2" pad="1"/>
<contactref element="SW2" pad="3"/>
<contactref element="JP2" pad="1"/>
<contactref element="LPA0" pad="C"/>
<contactref element="Q1" pad="4"/>
<contactref element="Q1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="USB" pad="GND"/>
<contactref element="CFG" pad="2"/>
<contactref element="RFG" pad="2"/>
<contactref element="CP2104" pad="EP"/>
<contactref element="SP5030" pad="1"/>
<contactref element="CVPP" pad="2"/>
<contactref element="CP2104" pad="2"/>
<contactref element="CP2104" pad="18"/>
<contactref element="CN1" pad="2"/>
<contactref element="LPWR" pad="C"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="RPD2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="CI2" pad="2"/>
<contactref element="CP2104" pad="EP@1"/>
<contactref element="CP2104" pad="EP@2"/>
<contactref element="CREG" pad="2"/>
<contactref element="CV2" pad="1"/>
<contactref element="CV1" pad="1"/>
<contactref element="CI1" pad="2"/>
<contactref element="BUCK" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="CO2" pad="1"/>
<contactref element="CO1" pad="1"/>
</signal>
<signal name="XTAL2">
<contactref element="ATMEGA2560" pad="33"/>
<contactref element="Q1" pad="3"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="XLAT1">
<contactref element="ATMEGA2560" pad="34"/>
<contactref element="Q1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="RXD2">
<contactref element="ATMEGA2560" pad="12"/>
<contactref element="JP2" pad="17"/>
</signal>
<signal name="TXD2">
<contactref element="ATMEGA2560" pad="13"/>
<contactref element="JP2" pad="16"/>
</signal>
<signal name="RXD3">
<contactref element="ATMEGA2560" pad="63"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="TXD3">
<contactref element="ATMEGA2560" pad="64"/>
<contactref element="JP1" pad="13"/>
</signal>
<signal name="RXD0S">
<contactref element="CP2104" pad="21"/>
<contactref element="RURX" pad="2"/>
</signal>
<signal name="TXD0S">
<contactref element="CP2104" pad="20"/>
<contactref element="RUTX" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="ATMEGA2560" pad="43"/>
<contactref element="RSCL" pad="2"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="ATMEGA2560" pad="44"/>
<contactref element="RSDA" pad="2"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="RXD1">
<contactref element="ATMEGA2560" pad="45"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="TXD1">
<contactref element="ATMEGA2560" pad="46"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="!SS">
<contactref element="ATMEGA2560" pad="19"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="SCK">
<contactref element="ATMEGA2560" pad="20"/>
<contactref element="JP2" pad="10"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="MOSI">
<contactref element="ATMEGA2560" pad="21"/>
<contactref element="JP2" pad="9"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="MISO">
<contactref element="ATMEGA2560" pad="22"/>
<contactref element="JP2" pad="8"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="!RESET">
<contactref element="ATMEGA2560" pad="30"/>
<contactref element="RRES" pad="1"/>
<contactref element="JP2" pad="3"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="SW2" pad="2"/>
<contactref element="SW2" pad="4"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="PE4">
<contactref element="ATMEGA2560" pad="6"/>
<contactref element="JP2" pad="19"/>
</signal>
<signal name="PE5">
<contactref element="JP2" pad="18"/>
<contactref element="ATMEGA2560" pad="7"/>
</signal>
<signal name="ADC0">
<contactref element="ATMEGA2560" pad="97"/>
<contactref element="JP2" pad="24"/>
</signal>
<signal name="ADC1">
<contactref element="ATMEGA2560" pad="96"/>
<contactref element="JP1" pad="24"/>
</signal>
<signal name="ADC2">
<contactref element="ATMEGA2560" pad="95"/>
<contactref element="JP1" pad="23"/>
</signal>
<signal name="ADC3">
<contactref element="ATMEGA2560" pad="94"/>
<contactref element="JP1" pad="22"/>
</signal>
<signal name="ADC4">
<contactref element="ATMEGA2560" pad="93"/>
<contactref element="JP1" pad="21"/>
</signal>
<signal name="ADC5">
<contactref element="ATMEGA2560" pad="92"/>
<contactref element="JP1" pad="20"/>
</signal>
<signal name="AREF">
<contactref element="ATMEGA2560" pad="98"/>
<contactref element="C7" pad="1"/>
<contactref element="JP6" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="RPB7" pad="2"/>
<contactref element="LPB7" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="RPWR" pad="2"/>
<contactref element="LPWR" pad="A"/>
</signal>
<signal name="PB7">
<contactref element="ATMEGA2560" pad="26"/>
<contactref element="RPB7" pad="1"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="VBAT">
<contactref element="JP1" pad="2"/>
<contactref element="CN1" pad="1"/>
<contactref element="BAT__REG" pad="INT2"/>
<contactref element="JREG" pad="1"/>
</signal>
<signal name="PE3">
<contactref element="ATMEGA2560" pad="5"/>
<contactref element="JP2" pad="20"/>
</signal>
<signal name="PB4">
<contactref element="ATMEGA2560" pad="23"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="PB5">
<contactref element="ATMEGA2560" pad="24"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="PH5">
<contactref element="ATMEGA2560" pad="17"/>
<contactref element="JP2" pad="13"/>
</signal>
<signal name="PH6">
<contactref element="ATMEGA2560" pad="18"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="PH4">
<contactref element="ATMEGA2560" pad="16"/>
<contactref element="JP2" pad="14"/>
</signal>
<signal name="PH3">
<contactref element="ATMEGA2560" pad="15"/>
<contactref element="JP2" pad="15"/>
</signal>
<signal name="ADC8">
<contactref element="ATMEGA2560" pad="89"/>
<contactref element="JP6" pad="5"/>
</signal>
<signal name="DTR">
<contactref element="SJ2" pad="1"/>
<contactref element="SJ3" pad="1"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="PB6">
<contactref element="ATMEGA2560" pad="25"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="LPA0" pad="A"/>
<contactref element="RPA0" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="CP2104" pad="4"/>
<contactref element="USB" pad="D-"/>
<contactref element="SP5030" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="CP2104" pad="3"/>
<contactref element="USB" pad="D+"/>
<contactref element="SP5030" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="USB" pad="VBUS"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="CVPP" pad="1"/>
<contactref element="CP2104" pad="16"/>
</signal>
<signal name="+3V3">
<contactref element="CP2104" pad="6"/>
<contactref element="CP2104" pad="5"/>
<contactref element="RRST" pad="1"/>
<contactref element="LTX" pad="A"/>
<contactref element="LRX" pad="A"/>
<contactref element="CV2" pad="2"/>
<contactref element="CV1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="RRST" pad="2"/>
<contactref element="CP2104" pad="9"/>
</signal>
<signal name="GP0-TX">
<contactref element="CP2104" pad="14"/>
<contactref element="RTX" pad="2"/>
</signal>
<signal name="GTX">
<contactref element="RTX" pad="1"/>
<contactref element="LTX" pad="C"/>
</signal>
<signal name="GP1-RX">
<contactref element="CP2104" pad="13"/>
<contactref element="RRX" pad="2"/>
</signal>
<signal name="GRX">
<contactref element="RRX" pad="1"/>
<contactref element="LRX" pad="C"/>
</signal>
<signal name="VBUS">
<contactref element="CP2104" pad="8"/>
<contactref element="SP5030" pad="2"/>
<contactref element="CP2104" pad="7"/>
<contactref element="F1" pad="1"/>
<contactref element="D3" pad="A"/>
<contactref element="JP1" pad="3"/>
<contactref element="CREG" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="JP2" pad="2"/>
<contactref element="RRES" pad="2"/>
<contactref element="ATMEGA2560" pad="10"/>
<contactref element="ATMEGA2560" pad="31"/>
<contactref element="ATMEGA2560" pad="61"/>
<contactref element="ATMEGA2560" pad="80"/>
<contactref element="C8" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="JPW" pad="2"/>
<contactref element="JDA" pad="2"/>
<contactref element="JCL" pad="2"/>
<contactref element="BAT__REG" pad="OUT"/>
<contactref element="FB1" pad="1"/>
</signal>
<signal name="CDTR">
<contactref element="CP2104" pad="23"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="RTS">
<contactref element="CP2104" pad="19"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="PA2">
<contactref element="ATMEGA2560" pad="76"/>
<contactref element="JP1" pad="17"/>
</signal>
<signal name="PA3">
<contactref element="ATMEGA2560" pad="75"/>
<contactref element="JP1" pad="16"/>
</signal>
<signal name="PA4">
<contactref element="ATMEGA2560" pad="74"/>
<contactref element="JP1" pad="15"/>
</signal>
<signal name="PC5">
<contactref element="ATMEGA2560" pad="58"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="PC6">
<contactref element="ATMEGA2560" pad="59"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="PC7">
<contactref element="ATMEGA2560" pad="60"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="PA5">
<contactref element="JP1" pad="14"/>
<contactref element="ATMEGA2560" pad="73"/>
</signal>
<signal name="ADC9">
<contactref element="JP6" pad="4"/>
<contactref element="ATMEGA2560" pad="88"/>
</signal>
<signal name="ADC10">
<contactref element="JP6" pad="3"/>
<contactref element="ATMEGA2560" pad="87"/>
</signal>
<signal name="ADC11">
<contactref element="JP6" pad="2"/>
<contactref element="ATMEGA2560" pad="86"/>
</signal>
<signal name="ADC15">
<contactref element="JP6" pad="1"/>
<contactref element="ATMEGA2560" pad="82"/>
</signal>
<signal name="PG5">
<contactref element="ATMEGA2560" pad="1"/>
<contactref element="JP2" pad="23"/>
</signal>
<signal name="PA1">
<contactref element="ATMEGA2560" pad="77"/>
<contactref element="JP1" pad="18"/>
</signal>
<signal name="PA0">
<contactref element="ATMEGA2560" pad="78"/>
<contactref element="JP1" pad="19"/>
<contactref element="RPA0" pad="2"/>
</signal>
<signal name="GNDF">
<contactref element="USB" pad="V1"/>
<contactref element="USB" pad="V2"/>
<contactref element="USB" pad="V3"/>
<contactref element="USB" pad="V4"/>
<contactref element="USB" pad="P$6"/>
<contactref element="USB" pad="P$3"/>
<contactref element="USB" pad="SHIELD4"/>
<contactref element="USB" pad="P$4"/>
<contactref element="USB" pad="P$8"/>
<contactref element="USB" pad="SHEILD2"/>
<contactref element="USB" pad="P$2"/>
<contactref element="USB" pad="P$12"/>
<contactref element="USB" pad="P$10"/>
<contactref element="USB" pad="P$1"/>
<contactref element="USB" pad="SHIELD"/>
<contactref element="USB" pad="SHIELD3"/>
<contactref element="RFG" pad="1"/>
<contactref element="CFG" pad="1"/>
</signal>
<signal name="PC4">
<contactref element="ATMEGA2560" pad="57"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="TXD0">
<contactref element="RUTX" pad="1"/>
<contactref element="ATMEGA2560" pad="3"/>
<contactref element="JP2" pad="21"/>
</signal>
<signal name="RXD0">
<contactref element="RURX" pad="1"/>
<contactref element="ATMEGA2560" pad="2"/>
<contactref element="JP2" pad="22"/>
</signal>
<signal name="N$3">
<contactref element="RPWR" pad="1"/>
<contactref element="JPW" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="RSDA" pad="1"/>
<contactref element="JDA" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="RSCL" pad="1"/>
<contactref element="JCL" pad="1"/>
</signal>
<signal name="VPREREG">
<contactref element="D2" pad="A"/>
<contactref element="RPD2" pad="2"/>
<contactref element="JREG" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="CI2" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="CI1" pad="1"/>
<contactref element="BUCK" pad="5"/>
<contactref element="REN" pad="1"/>
</signal>
<signal name="PREOUT">
<contactref element="BAT__REG" pad="IN1"/>
<contactref element="L1" pad="2"/>
<contactref element="CO2" pad="2"/>
<contactref element="CO1" pad="2"/>
<contactref element="CFF" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="EN">
<contactref element="BUCK" pad="4"/>
<contactref element="REN" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="L1" pad="1"/>
<contactref element="BUCK" pad="6"/>
<contactref element="CSW" pad="2"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="SW">
<contactref element="CSW" pad="1"/>
<contactref element="BUCK" pad="1"/>
</signal>
<signal name="FB">
<contactref element="R2" pad="1"/>
<contactref element="BUCK" pad="3"/>
<contactref element="CFF" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="ATMEGA2560" pad="100"/>
<contactref element="FB1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
