<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="81.915" x2="42.545" y2="81.915" width="0.4064" layer="20"/>
<text>54Ω</text>
<wire x1="42.545" y1="1.27" x2="0" y2="1.27" width="0.4064" layer="20"/>
<wire x1="0" y1="81.915" x2="0" y2="1.27" width="0.4064" layer="20"/>
<wire x1="42.545" y1="81.915" x2="42.545" y2="1.27" width="0.4064" layer="20"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="0309/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 12.5 mm</description>
</package>
<package name="TRIM-3386">
</package>
<package name="LCD1602">
</package>
</packages>
</library>
<library name="Spark2">
<packages>
<package name="PHOTON">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Sensors&lt;/h3&gt;
This library contains sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;h3&gt;TO-92 3-Pin PTH Footprint&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Sensors/Temp/TMP35_36_37.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 3&lt;/li&gt;
&lt;li&gt;Dimensions: 3.68 x 4.83 x 4.83 mm&lt;/li&gt;
&lt;li&gt;Pitch: 2.54 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;TMP36&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-10MM">
<description>2 PTH spaced 10mm apart</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="adafruit" package="0309/12" value="54"/>
<element name="TM1" library="adafruit" package="TRIM-3386" value=""/>
<element name="U$1" library="Spark2" package="PHOTON" value="PHOTON_WITH_HEADERS"/>
<element name="X1" library="adafruit" package="LCD1602" value="HD44780LCD-1602"/>
<element name="U1" library="SparkFun-Sensors" package="TO-92" value="">
<attribute name="PROD_ID" value="IC-09880"/>
<attribute name="SF_ID" value="SEN-10988"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-10MM" value="10nF">
<attribute name="PROD_ID" value="CAP-09321"/>
</element>
</elements>
<signals>
<signal name="VBAT">
<contactref element="U$1" pad="22"/>
</signal>
<signal name="N$6">
<contactref element="X1" pad="14"/>
<contactref element="U$1" pad="20"/>
</signal>
<signal name="N$1">
<contactref element="X1" pad="13"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="18"/>
<contactref element="X1" pad="12"/>
</signal>
<signal name="N$5">
<contactref element="X1" pad="11"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="16"/>
<contactref element="X1" pad="10"/>
</signal>
<signal name="N$8">
<contactref element="X1" pad="9"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="14"/>
<contactref element="X1" pad="8"/>
</signal>
<signal name="N$10">
<contactref element="X1" pad="7"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="N$3">
<contactref element="X1" pad="6"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="11"/>
<contactref element="X1" pad="4"/>
</signal>
<signal name="VSS">
<contactref element="X1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="TM1" pad="3"/>
<contactref element="X1" pad="16"/>
<contactref element="X1" pad="5"/>
</signal>
<signal name="VDD">
<contactref element="X1" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="TM1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="TM1" pad="2"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="X1" pad="15"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="10"/>
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="1"/>
<contactref element="U$1" pad="24"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="3"/>
<contactref element="U$1" pad="21"/>
<contactref element="C1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
