<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="62.484" y1="8.382" x2="62.484" y2="26.416" width="0" layer="20"/>
<wire x1="62.484" y1="26.416" x2="9.652" y2="26.416" width="0" layer="20"/>
<wire x1="9.652" y1="26.416" x2="9.652" y2="8.382" width="0" layer="20"/>
<wire x1="9.652" y1="8.382" x2="62.484" y2="8.382" width="0" layer="20"/>
<text>8</text>
<text>LED</text>
<text>1</text>
<text>Boutons</text>
<text>GND</text>
<text>8</text>
<text>1</text>
<text>VCC</text>
<text>V1.1</text>
<text>25/02/16</text>
<text>5V</text>
<text>3.3V</text>
<text>220Ω</text>
<text>65Ω</text>
</plain>
<libraries>
<library name="Charlie-Switch">
<packages>
<package name="5.2X5.2X1.5-SMD">
</package>
</packages>
</library>
<library name="Charlie-Resistances">
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="Charlie-LED">
<packages>
<package name="0805">
</package>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_ROUND">
</package>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1" library="Charlie-Switch" package="5.2X5.2X1.5-SMD" value="SWITCH_SPSTSMD">
<attribute name="NAME"/>
</element>
<element name="R1" library="Charlie-Resistances" package="0805" value="75k"/>
<element name="D1" library="Charlie-LED" package="0805" value="Red">
<attribute name="NAME"/>
</element>
<element name="S2" library="Charlie-Switch" package="5.2X5.2X1.5-SMD" value="SWITCH_SPSTSMD">
<attribute name="NAME"/>
</element>
<element name="R2" library="Charlie-Resistances" package="0805" value="75k"/>
<element name="S3" library="Charlie-Switch" package="5.2X5.2X1.5-SMD" value="SWITCH_SPSTSMD">
<attribute name="NAME"/>
</element>
<element name="R3" library="Charlie-Resistances" package="0805" value="75k"/>
<element name="S4" library="Charlie-Switch" package="5.2X5.2X1.5-SMD" value="SWITCH_SPSTSMD">
<attribute name="NAME"/>
</element>
<element name="R4" library="Charlie-Resistances" package="0805" value="75k"/>
<element name="S5" library="Charlie-Switch" package="5.2X5.2X1.5-SMD" value="SWITCH_SPSTSMD">
<attribute name="NAME"/>
</element>
<element name="R5" library="Charlie-Resistances" package="0805" value="75k"/>
<element name="S6" library="Charlie-Switch" package="5.2X5.2X1.5-SMD" value="SWITCH_SPSTSMD">
<attribute name="NAME"/>
</element>
<element name="R6" library="Charlie-Resistances" package="0805" value="75k"/>
<element name="S7" library="Charlie-Switch" package="5.2X5.2X1.5-SMD" value="SWITCH_SPSTSMD">
<attribute name="NAME"/>
</element>
<element name="R7" library="Charlie-Resistances" package="0805" value="75k"/>
<element name="S8" library="Charlie-Switch" package="5.2X5.2X1.5-SMD" value="SWITCH_SPSTSMD">
<attribute name="NAME"/>
</element>
<element name="R8" library="Charlie-Resistances" package="0805" value="75k"/>
<element name="JP1" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="VALUE"/>
</element>
<element name="R9" library="Charlie-Resistances" package="0805" value="220"/>
<element name="D2" library="Charlie-LED" package="0805" value="Red">
<attribute name="NAME"/>
</element>
<element name="R10" library="Charlie-Resistances" package="0805" value="220"/>
<element name="D3" library="Charlie-LED" package="0805" value="Red">
<attribute name="NAME"/>
</element>
<element name="R11" library="Charlie-Resistances" package="0805" value="220"/>
<element name="D4" library="Charlie-LED" package="0805" value="Red">
<attribute name="NAME"/>
</element>
<element name="R12" library="Charlie-Resistances" package="0805" value="220"/>
<element name="D5" library="Charlie-LED" package="0805" value="Red">
<attribute name="NAME"/>
</element>
<element name="R13" library="Charlie-Resistances" package="0805" value="220"/>
<element name="D6" library="Charlie-LED" package="0805" value="Red">
<attribute name="NAME"/>
</element>
<element name="R14" library="Charlie-Resistances" package="0805" value="220"/>
<element name="D7" library="Charlie-LED" package="0805" value="Red">
<attribute name="NAME"/>
</element>
<element name="R15" library="Charlie-Resistances" package="0805" value="220"/>
<element name="D8" library="Charlie-LED" package="0805" value="Red">
<attribute name="NAME"/>
</element>
<element name="R16" library="Charlie-Resistances" package="0805" value="220"/>
<element name="JP3" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="D9" library="Charlie-LED" package="LED-0603" value="White">
<attribute name="NAME"/>
</element>
<element name="R17" library="Charlie-Resistances" package="0805" value="220"/>
</elements>
<signals>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="D8" pad="2"/>
<contactref element="D7" pad="2"/>
<contactref element="D6" pad="2"/>
<contactref element="D5" pad="2"/>
<contactref element="D4" pad="2"/>
<contactref element="D3" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="D1" pad="2"/>
<contactref element="D9" pad="C"/>
</signal>
<signal name="OUT1">
<contactref element="R1" pad="2"/>
<contactref element="S1" pad="P$3" route="any" routetag="G$1.2"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="VCC">
<contactref element="S1" pad="P$1"/>
<contactref element="S2" pad="P$1"/>
<contactref element="S3" pad="P$1"/>
<contactref element="S4" pad="P$1"/>
<contactref element="S5" pad="P$1"/>
<contactref element="S6" pad="P$1"/>
<contactref element="S7" pad="P$1"/>
<contactref element="S8" pad="P$1"/>
<contactref element="JP4" pad="1"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="OUT2">
<contactref element="R2" pad="2"/>
<contactref element="S2" pad="P$3" route="any" routetag="G$1.2"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="OUT3">
<contactref element="R3" pad="2"/>
<contactref element="S3" pad="P$3" route="any" routetag="G$1.2"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="OUT4">
<contactref element="R4" pad="2"/>
<contactref element="S4" pad="P$3" route="any" routetag="G$1.2"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="OUT5">
<contactref element="R5" pad="2"/>
<contactref element="S5" pad="P$3" route="any" routetag="G$1.2"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="OUT6">
<contactref element="R6" pad="2"/>
<contactref element="S6" pad="P$3" route="any" routetag="G$1.2"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="OUT7">
<contactref element="R7" pad="2"/>
<contactref element="S7" pad="P$3" route="any" routetag="G$1.2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="OUT8">
<contactref element="R8" pad="2"/>
<contactref element="S8" pad="P$3" route="any" routetag="G$1.2"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="+D1">
<contactref element="R9" pad="2"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="+D2">
<contactref element="R10" pad="2"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="D3" pad="1"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="+D3">
<contactref element="R11" pad="2"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="D4" pad="1"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="+D4">
<contactref element="R12" pad="2"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="D5" pad="1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="+D5">
<contactref element="R13" pad="2"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="D6" pad="1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="+D6">
<contactref element="R14" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="D7" pad="1"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="+D7">
<contactref element="R15" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="D8" pad="1"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="+D8">
<contactref element="R16" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R17" pad="1"/>
<contactref element="D9" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
