<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<text>ISP</text>
<text>JTAG (A3PN)</text>
<text>R</text>
<text>T</text>
<text>F</text>
<text>M</text>
<text>Die Datenkrake v1.0</text>
<text>http://datenkrake.org</text>
<text>CH1</text>
<text>CH2</text>
<text>CH3</text>
<text>CH4</text>
<text>CH5</text>
<text>CH6</text>
<text>CH7</text>
<text>CH8</text>
<text>B1</text>
<text>!RES!</text>
<text>A</text>
<text>B</text>
<text>C</text>
<text>D</text>
<text>(C) 2013 
D. Nedospasov &amp; Th. Schroeder</text>
<text></text>
<text>Die Datenkrake v1.0 - http://datenkrake.org</text>
<text>(C) 2013 Dmitry Nedospasov &amp; Thorsten Schroeder</text>
<text>LPC</text>
<text>A3PN</text>
<text>Dmitry Nedospasov http://nedos.net
Thorsten Schröder http://www.modzero.ch</text>
<text>1</text>
<text>1</text>
<text>GND</text>
<text>3V3</text>
<text>3V3</text>
<text>1V5</text>
<text>5V0</text>
<text>RX0</text>
<text>TX0</text>
<text>GND</text>
<text>5V</text>
<text>CLK</text>
<text>http://nedos.net</text>
<text>http://www.modzero.ch</text>
<wire x1="111.76" y1="83.82" x2="116.205" y2="79.6925" width="0" layer="20" curve="-90"/>
<wire x1="116.205" y1="79.6925" x2="116.205" y2="4.445" width="0" layer="20"/>
<wire x1="116.205" y1="4.445" x2="111.76" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="111.76" y1="0" x2="4.445" y2="0" width="0" layer="20"/>
<wire x1="4.445" y1="0" x2="0" y2="4.445" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="4.445" x2="0" y2="79.53375" width="0" layer="20"/>
<wire x1="0" y1="79.53375" x2="4.445" y2="83.82" width="0" layer="20" curve="-90"/>
<wire x1="4.445" y1="83.82" x2="111.76" y2="83.82" width="0" layer="20"/>
<text>+5V</text>
<text>K</text>
<text>K</text>
<text>K</text>
<text>K</text>
<text>K</text>
<text>JTAG</text>
</plain>
<libraries>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="CT3216">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="actel-proasic3">
<packages>
<package name="VQFP100">
<description>&lt;h1&gt;VQFP100 package for Microsemiconductor's ProASIC3 nano&lt;/h1&gt;

&lt;p&gt;
&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="lpc1xxx-v6">
<description>LPC1xxx microcontrollers NXP Semiconductors (founded by Philips)</description>
<packages>
<package name="LQFP100-14X14">
<description>&lt;b&gt;LQFP100 &lt;/b&gt;&lt;p&gt;Low profile Quad Flat Package 14x14x1.4 mm&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
</packages>
</library>
<library name="devio">
<description>&lt;b&gt;project.dev.io - eagle lib (devio.lbr)&lt;/b&gt;
&lt;p&gt;
some useful parts and logos as well as "exotic" ICs

Mostly parts of Texas Instruments, using their packages are defined within this lib if they are not yet publically available as eagle library.
&lt;/p&gt;

&lt;p&gt;
Author of this library is Thorsten Schroeder &amp;lt;ths@dev.io&amp;gt;&lt;br&gt;
The Library is released under the terms of the Beer Ware License (Revision 42).
&lt;/p&gt;

&lt;p&gt;
This Eagle library is published under &lt;strong&gt;"THE BEER-WARE LICENSE"&lt;/strong&gt; (Revision 42):&lt;br&gt;
Thorsten Schr&amp;ouml;der wrote this file.  As long as you retain this notice you can do whatever you want with this stuff. If we meet some day, and you think this stuff is worth it, you can buy me a beer in return. 
&lt;/p&gt;</description>
<packages>
<package name="B3U-1000P">
<description>Without Ground Terminal, without Boss
B3U-1000P(M)</description>
</package>
<package name="VLS_INDUCTOR">
</package>
<package name="LOGO_SMALL">
</package>
<package name="PASSER-MARK">
</package>
<package name="LOGO_SMALL_TPLACE">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="pinhead-2">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de, Modified by Cougar@CasaDelGato.Com&lt;/author&gt;</description>
<packages>
<package name="2X10SMD">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 SMD</description>
</package>
<package name="2X05SMD">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 SMD</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="ftx">
<description>Generated from &lt;b&gt;ftx.sch&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="SERIAL_QFN4X4-16">
</package>
</packages>
</library>
<library name="wuerth-elektronik">
<description>&lt;BR&gt;WE eiSos -- EMC &amp; Inductive Solutions&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-400&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com"&gt;http://www.we-online.com&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:eisos@we-online.de"&gt;eisos@we-online.de&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Version 4,   July 12th 2005
&lt;HR&gt;
Copyright: Würth Elektronik eiSos</description>
<packages>
<package name="WE-KI_0805_B">
<description>SMD Wire Wound Ceramic Inductor</description>
</package>
</packages>
</library>
<library name="Labor">
<packages>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA07-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="krake-rj45">
<packages>
<package name="95501">
</package>
<package name="TSSOP16">
</package>
</packages>
</library>
<library name="SparkFun">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP08R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,3">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.3 mm with drill center</description>
</package>
</packages>
</library>
<library name="krake-power">
<packages>
<package name="GNDPAD">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC2" library="actel-proasic3" package="VQFP100" value="PROASIC3_NANO_A3PN125"/>
<element name="IC1" library="lpc1xxx-v6" package="LQFP100-14X14" value="LPC1765"/>
<element name="Q1" library="crystal" package="CTS406" value="12MHz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="C3" library="rcl" package="C0603K" value="22p"/>
<element name="C4" library="rcl" package="C0603K" value="22p"/>
<element name="C5" library="rcl" package="C0603K" value="100n"/>
<element name="C6" library="rcl" package="C0603K" value="100n"/>
<element name="C7" library="rcl" package="C0603K" value="100n"/>
<element name="C8" library="rcl" package="C0603K" value="100n"/>
<element name="C9" library="rcl" package="C0603K" value="100n"/>
<element name="C10" library="rcl" package="C0603K" value="100n"/>
<element name="C11" library="rcl" package="C0603K" value="100n"/>
<element name="C12" library="rcl" package="C0603K" value="100n"/>
<element name="C13" library="rcl" package="C0603K" value="100n"/>
<element name="RESET" library="devio" package="B3U-1000P" value=""/>
<element name="ISP" library="devio" package="B3U-1000P" value=""/>
<element name="LED1" library="led" package="CHIP-LED0603" value="RED"/>
<element name="LED2" library="led" package="CHIP-LED0603" value="RED"/>
<element name="LED3" library="led" package="CHIP-LED0603" value="RED"/>
<element name="LED4" library="led" package="CHIP-LED0603" value="RED"/>
<element name="R4" library="rcl" package="R0603" value="270"/>
<element name="R5" library="rcl" package="R0603" value="270"/>
<element name="R6" library="rcl" package="R0603" value="270"/>
<element name="R7" library="rcl" package="R0603" value="270"/>
<element name="R8" library="rcl" package="R0603" value="47k"/>
<element name="R9" library="rcl" package="R0603" value="47k"/>
<element name="JTAG_LPC" library="pinhead-2" package="2X10SMD" value=""/>
<element name="R11" library="rcl" package="R0603" value="10k"/>
<element name="R12" library="rcl" package="R0603" value="10k"/>
<element name="R13" library="rcl" package="R0603" value="10k"/>
<element name="R14" library="rcl" package="R0603" value="10k"/>
<element name="R15" library="rcl" package="R0603" value="10k"/>
<element name="R10" library="rcl" package="R0603" value="10k"/>
<element name="PWR_UP" library="led" package="CHIPLED_0603" value="GREEN"/>
<element name="R16" library="resistor" package="R0603" value="680"/>
<element name="R17" library="resistor" package="R0603" value="27"/>
<element name="R18" library="resistor" package="R0603" value="27"/>
<element name="C14" library="rcl" package="C0603" value="47p"/>
<element name="C15" library="rcl" package="C0603" value="47p"/>
<element name="FT230X" library="ftx" package="SERIAL_QFN4X4-16" value="SERIAL_FT230XQ"/>
<element name="L1" library="wuerth-elektronik" package="WE-KI_0805_B" value="10µH"/>
<element name="C16" library="rcl" package="C0603" value="100n"/>
<element name="C17" library="rcl" package="C0603" value="10n"/>
<element name="C18" library="rcl" package="C0603" value="100n"/>
<element name="C19" library="rcl" package="CT3216" value="TA 10u"/>
<element name="JTAG_A3PN" library="pinhead-2" package="2X05SMD" value=""/>
<element name="R83" library="rcl" package="R0603" value="10k"/>
<element name="R84" library="rcl" package="R0603" value="10k"/>
<element name="C28" library="rcl" package="C0603K" value="10n"/>
<element name="C29" library="rcl" package="C0603K" value="330n"/>
<element name="LM3671" library="Labor" package="SOT23-5L" value="LM3671_1V5"/>
<element name="L2" library="devio" package="VLS_INDUCTOR" value="2.2uH"/>
<element name="C35" library="rcl" package="CT3216" value="10u"/>
<element name="C36" library="rcl" package="CT3216" value="47u"/>
<element name="C37" library="rcl" package="C0603K" value="100n"/>
<element name="C38" library="rcl" package="C0603K" value="100n"/>
<element name="C39" library="rcl" package="C0603K" value="100n"/>
<element name="C40" library="rcl" package="C0603K" value="100n"/>
<element name="C41" library="rcl" package="C0603K" value="100n"/>
<element name="C42" library="rcl" package="C0603K" value="100n"/>
<element name="C43" library="rcl" package="C0603K" value="100n"/>
<element name="C44" library="rcl" package="C0603K" value="100n"/>
<element name="C45" library="rcl" package="C0603K" value="100n"/>
<element name="C46" library="rcl" package="C0603K" value="100n"/>
<element name="C47" library="rcl" package="C0603K" value="100n"/>
<element name="C48" library="rcl" package="C0603K" value="100n"/>
<element name="C49" library="rcl" package="C0603K" value="100n"/>
<element name="C50" library="rcl" package="C0603K" value="10n"/>
<element name="HCH3" library="con-lstb" package="MA07-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="CH3" library="krake-rj45" package="95501" value="955XX-86889"/>
<element name="HCH2" library="con-lstb" package="MA07-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="CH2" library="krake-rj45" package="95501" value="955XX-86889"/>
<element name="HCH1" library="con-lstb" package="MA07-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="CH1" library="krake-rj45" package="95501" value="955XX-86889"/>
<element name="HCH8" library="con-lstb" package="MA07-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="CH8" library="krake-rj45" package="95501" value="955XX-86889"/>
<element name="HCH4" library="con-lstb" package="MA07-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="CH4" library="krake-rj45" package="95501" value="955XX-86889"/>
<element name="HCH5" library="con-lstb" package="MA07-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="CH5" library="krake-rj45" package="95501" value="955XX-86889"/>
<element name="HCH6" library="con-lstb" package="MA07-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="CH6" library="krake-rj45" package="95501" value="955XX-86889"/>
<element name="HCH7" library="con-lstb" package="MA07-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="CH7" library="krake-rj45" package="95501" value="955XX-86889"/>
<element name="LM1" library="Labor" package="SOT23-5L" value="LM3671_3V3IO"/>
<element name="L3" library="devio" package="VLS_INDUCTOR" value="2.2uH"/>
<element name="C1" library="rcl" package="CT3216" value="10u"/>
<element name="C2" library="rcl" package="CT3216" value="47u"/>
<element name="C30" library="rcl" package="C0603K" value="100n"/>
<element name="LM2" library="Labor" package="SOT23-5L" value="LM3671_3V3_LPC"/>
<element name="L4" library="devio" package="VLS_INDUCTOR" value="2.2uH"/>
<element name="C31" library="rcl" package="CT3216" value="10u"/>
<element name="C32" library="rcl" package="CT3216" value="47u"/>
<element name="C33" library="rcl" package="C0603K" value="100n"/>
<element name="X1" library="SparkFun" package="USB-MINIB" value="USBSMD"/>
<element name="TP1" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP2" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP3" library="testpad" package="TP08R" value="PTR1TP08R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP4" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP5" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP6" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP7" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP8" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP9" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP10" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="R1" library="rcl" package="R0603" value="330"/>
<element name="R2" library="rcl" package="R0603" value="330"/>
<element name="R3" library="rcl" package="R0603" value="330"/>
<element name="R19" library="rcl" package="R0603" value="330"/>
<element name="R20" library="rcl" package="R0603" value="330"/>
<element name="R21" library="rcl" package="R0603" value="330"/>
<element name="U$3" library="krake-rj45" package="TSSOP16" value="NVT2006"/>
<element name="R22" library="rcl" package="R0603" value="200k"/>
<element name="C20" library="rcl" package="C0603" value="100n"/>
<element name="R23" library="rcl" package="R0603" value="330"/>
<element name="R24" library="rcl" package="R0603" value="330"/>
<element name="R25" library="rcl" package="R0603" value="330"/>
<element name="R26" library="rcl" package="R0603" value="330"/>
<element name="R27" library="rcl" package="R0603" value="330"/>
<element name="R28" library="rcl" package="R0603" value="330"/>
<element name="R29" library="rcl" package="R0603" value="200k"/>
<element name="C21" library="rcl" package="C0603" value="100n"/>
<element name="U$4" library="krake-rj45" package="TSSOP16" value="NVT2006"/>
<element name="R30" library="rcl" package="R0603" value="330"/>
<element name="R31" library="rcl" package="R0603" value="330"/>
<element name="R32" library="rcl" package="R0603" value="330"/>
<element name="R33" library="rcl" package="R0603" value="330"/>
<element name="R34" library="rcl" package="R0603" value="330"/>
<element name="R35" library="rcl" package="R0603" value="330"/>
<element name="R36" library="rcl" package="R0603" value="200k"/>
<element name="C22" library="rcl" package="C0603" value="100n"/>
<element name="U$5" library="krake-rj45" package="TSSOP16" value="NVT2006"/>
<element name="R37" library="rcl" package="R0603" value="330"/>
<element name="R38" library="rcl" package="R0603" value="330"/>
<element name="R39" library="rcl" package="R0603" value="330"/>
<element name="R40" library="rcl" package="R0603" value="330"/>
<element name="R41" library="rcl" package="R0603" value="330"/>
<element name="R42" library="rcl" package="R0603" value="330"/>
<element name="R43" library="rcl" package="R0603" value="200k"/>
<element name="C23" library="rcl" package="C0603" value="100n"/>
<element name="U$6" library="krake-rj45" package="TSSOP16" value="NVT2006"/>
<element name="R44" library="rcl" package="R0603" value="330"/>
<element name="R45" library="rcl" package="R0603" value="330"/>
<element name="R46" library="rcl" package="R0603" value="330"/>
<element name="R47" library="rcl" package="R0603" value="330"/>
<element name="R48" library="rcl" package="R0603" value="330"/>
<element name="R49" library="rcl" package="R0603" value="330"/>
<element name="R50" library="rcl" package="R0603" value="200k"/>
<element name="C24" library="rcl" package="C0603" value="100n"/>
<element name="U$7" library="krake-rj45" package="TSSOP16" value="NVT2006"/>
<element name="R51" library="rcl" package="R0603" value="330"/>
<element name="R52" library="rcl" package="R0603" value="330"/>
<element name="R53" library="rcl" package="R0603" value="330"/>
<element name="R54" library="rcl" package="R0603" value="330"/>
<element name="R55" library="rcl" package="R0603" value="330"/>
<element name="R56" library="rcl" package="R0603" value="330"/>
<element name="R57" library="rcl" package="R0603" value="200k"/>
<element name="C25" library="rcl" package="C0603" value="100n"/>
<element name="U$8" library="krake-rj45" package="TSSOP16" value="NVT2006"/>
<element name="R58" library="rcl" package="R0603" value="330"/>
<element name="R59" library="rcl" package="R0603" value="330"/>
<element name="R60" library="rcl" package="R0603" value="330"/>
<element name="R61" library="rcl" package="R0603" value="330"/>
<element name="R62" library="rcl" package="R0603" value="330"/>
<element name="R63" library="rcl" package="R0603" value="330"/>
<element name="R64" library="rcl" package="R0603" value="200k"/>
<element name="C26" library="rcl" package="C0603" value="100n"/>
<element name="U$9" library="krake-rj45" package="TSSOP16" value="NVT2006"/>
<element name="R65" library="rcl" package="R0603" value="330"/>
<element name="R66" library="rcl" package="R0603" value="330"/>
<element name="R67" library="rcl" package="R0603" value="330"/>
<element name="R68" library="rcl" package="R0603" value="330"/>
<element name="R69" library="rcl" package="R0603" value="330"/>
<element name="R70" library="rcl" package="R0603" value="330"/>
<element name="R71" library="rcl" package="R0603" value="200k"/>
<element name="C27" library="rcl" package="C0603" value="100n"/>
<element name="U$10" library="krake-rj45" package="TSSOP16" value="NVT2006"/>
<element name="C34" library="rcl" package="CT3216" value="10u"/>
<element name="C51" library="rcl" package="CT3216" value="10u"/>
<element name="C52" library="rcl" package="CT3216" value="10u"/>
<element name="C53" library="rcl" package="CT3216" value="10u"/>
<element name="C54" library="rcl" package="CT3216" value="10u"/>
<element name="C55" library="rcl" package="CT3216" value="10u"/>
<element name="C56" library="rcl" package="CT3216" value="10u"/>
<element name="C57" library="rcl" package="CT3216" value="10u"/>
<element name="U$1" library="devio" package="LOGO_SMALL" value=""/>
<element name="H1" library="holes" package="3,3" value="MOUNT-HOLE3.3"/>
<element name="H2" library="holes" package="3,3" value="MOUNT-HOLE3.3"/>
<element name="H3" library="holes" package="3,3" value="MOUNT-HOLE3.3"/>
<element name="H4" library="holes" package="3,3" value="MOUNT-HOLE3.3"/>
<element name="U$11" library="krake-power" package="GNDPAD" value="GNDPAD_4MM"/>
<element name="U$12" library="krake-power" package="GNDPAD" value="GNDPAD_4MM"/>
<element name="U$13" library="krake-power" package="GNDPAD" value="GNDPAD_4MM"/>
<element name="U$14" library="krake-power" package="GNDPAD" value="GNDPAD_4MM"/>
<element name="JP1" library="pinhead" package="1X01" value=""/>
<element name="JP2" library="pinhead" package="1X01" value=""/>
<element name="JP3" library="pinhead" package="1X01" value=""/>
<element name="JP4" library="pinhead" package="1X01" value=""/>
<element name="U$15" library="krake-power" package="GNDPAD" value="GNDPAD_4MM"/>
<element name="U$16" library="krake-power" package="GNDPAD" value="GNDPAD_4MM"/>
<element name="U$17" library="krake-power" package="GNDPAD" value="GNDPAD_4MM"/>
<element name="U$18" library="krake-power" package="GNDPAD" value="GNDPAD_4MM"/>
<element name="TP11" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="U$20" library="devio" package="PASSER-MARK" value=""/>
<element name="U$21" library="devio" package="PASSER-MARK" value=""/>
<element name="U$22" library="devio" package="PASSER-MARK" value=""/>
<element name="U$19" library="devio" package="LOGO_SMALL_TPLACE" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="9"/>
<contactref element="IC2" pad="38"/>
<contactref element="IC2" pad="51"/>
<contactref element="IC2" pad="67"/>
<contactref element="IC2" pad="88"/>
<contactref element="IC2" pad="25"/>
<contactref element="IC2" pad="75"/>
<contactref element="IC2" pad="12"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="IC1" pad="31"/>
<contactref element="IC1" pad="83"/>
<contactref element="IC1" pad="97"/>
<contactref element="IC1" pad="72"/>
<contactref element="IC1" pad="55"/>
<contactref element="IC1" pad="41"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC1" pad="11"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="ISP" pad="P$1"/>
<contactref element="RESET" pad="P$1"/>
<contactref element="R14" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="JTAG_LPC" pad="4"/>
<contactref element="JTAG_LPC" pad="20"/>
<contactref element="JTAG_LPC" pad="18"/>
<contactref element="JTAG_LPC" pad="16"/>
<contactref element="JTAG_LPC" pad="14"/>
<contactref element="JTAG_LPC" pad="12"/>
<contactref element="JTAG_LPC" pad="10"/>
<contactref element="JTAG_LPC" pad="8"/>
<contactref element="JTAG_LPC" pad="6"/>
<contactref element="R10" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="FT230X" pad="3"/>
<contactref element="FT230X" pad="13"/>
<contactref element="FT230X" pad="C"/>
<contactref element="C17" pad="1"/>
<contactref element="C19" pad="-"/>
<contactref element="C18" pad="2"/>
<contactref element="PWR_UP" pad="C"/>
<contactref element="R83" pad="1"/>
<contactref element="R84" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="JTAG_A3PN" pad="2"/>
<contactref element="JTAG_A3PN" pad="10"/>
<contactref element="LM3671" pad="2"/>
<contactref element="C36" pad="-"/>
<contactref element="C35" pad="-"/>
<contactref element="C37" pad="2"/>
<contactref element="C38" pad="1"/>
<contactref element="C49" pad="1"/>
<contactref element="C39" pad="1"/>
<contactref element="C40" pad="1"/>
<contactref element="C41" pad="1"/>
<contactref element="C42" pad="1"/>
<contactref element="C43" pad="1"/>
<contactref element="C44" pad="1"/>
<contactref element="C45" pad="1"/>
<contactref element="C46" pad="1"/>
<contactref element="C47" pad="1"/>
<contactref element="C48" pad="1"/>
<contactref element="C50" pad="1"/>
<contactref element="CH7" pad="P1"/>
<contactref element="CH6" pad="P1"/>
<contactref element="CH5" pad="P1"/>
<contactref element="CH4" pad="P1"/>
<contactref element="CH8" pad="P1"/>
<contactref element="CH1" pad="P1"/>
<contactref element="CH2" pad="P1"/>
<contactref element="CH3" pad="P1"/>
<contactref element="LM1" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="C1" pad="-"/>
<contactref element="C30" pad="2"/>
<contactref element="LM2" pad="2"/>
<contactref element="C32" pad="-"/>
<contactref element="C31" pad="-"/>
<contactref element="C33" pad="2"/>
<contactref element="X1" pad="GND"/>
<contactref element="TP7" pad="TP"/>
<contactref element="TP8" pad="TP"/>
<contactref element="TP9" pad="TP"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="C20" pad="2"/>
<contactref element="HCH4" pad="13"/>
<contactref element="HCH5" pad="13"/>
<contactref element="HCH6" pad="13"/>
<contactref element="HCH7" pad="13"/>
<contactref element="HCH8" pad="13"/>
<contactref element="HCH1" pad="13"/>
<contactref element="HCH2" pad="13"/>
<contactref element="HCH3" pad="13"/>
<contactref element="C21" pad="2"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="C22" pad="2"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="C23" pad="2"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="U$7" pad="P$1"/>
<contactref element="C24" pad="2"/>
<contactref element="U$7" pad="P$1"/>
<contactref element="U$8" pad="P$1"/>
<contactref element="C25" pad="2"/>
<contactref element="U$8" pad="P$1"/>
<contactref element="U$9" pad="P$1"/>
<contactref element="C26" pad="2"/>
<contactref element="U$9" pad="P$1"/>
<contactref element="U$10" pad="P$1"/>
<contactref element="C27" pad="2"/>
<contactref element="U$10" pad="P$1"/>
<contactref element="C34" pad="-"/>
<contactref element="C57" pad="-"/>
<contactref element="C56" pad="-"/>
<contactref element="C55" pad="-"/>
<contactref element="C52" pad="-"/>
<contactref element="C51" pad="-"/>
<contactref element="C54" pad="-"/>
<contactref element="C53" pad="-"/>
<contactref element="U$11" pad="P$1"/>
<contactref element="U$14" pad="P$1"/>
<contactref element="U$13" pad="P$1"/>
<contactref element="U$12" pad="P$1"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="U$15" pad="P$1"/>
<contactref element="U$16" pad="P$1"/>
<contactref element="U$17" pad="P$1"/>
<contactref element="U$18" pad="P$1"/>
</signal>
<signal name="N$22">
<contactref element="C4" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="N$23">
<contactref element="C3" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="TX0">
<contactref element="IC1" pad="98"/>
<contactref element="FT230X" pad="2"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="RX0">
<contactref element="IC1" pad="99"/>
<contactref element="FT230X" pad="15"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="BUT1">
<contactref element="IC1" pad="53"/>
<contactref element="ISP" pad="P$2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="TX2">
<contactref element="IC1" pad="48"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="RX2">
<contactref element="IC1" pad="49"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="TX3">
<contactref element="IC1" pad="46"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="RX3">
<contactref element="IC1" pad="47"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="!RES!">
<contactref element="IC1" pad="17"/>
<contactref element="RESET" pad="P$2"/>
<contactref element="R8" pad="1"/>
<contactref element="JTAG_LPC" pad="15"/>
</signal>
<signal name="LED4">
<contactref element="IC1" pad="79"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="LED3">
<contactref element="IC1" pad="78"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="LED2">
<contactref element="IC1" pad="77"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="LED1">
<contactref element="IC1" pad="76"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="CH5_EN">
<contactref element="R57" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="U$8" pad="P$15"/>
<contactref element="U$8" pad="P$16"/>
<contactref element="IC1" pad="51"/>
</signal>
<signal name="CH6_EN">
<contactref element="R64" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="U$9" pad="P$15"/>
<contactref element="U$9" pad="P$16"/>
<contactref element="IC1" pad="52"/>
</signal>
<signal name="CH7_EN">
<contactref element="IC1" pad="58"/>
<contactref element="R71" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="U$10" pad="P$15"/>
<contactref element="U$10" pad="P$16"/>
</signal>
<signal name="CH8_EN">
<contactref element="IC1" pad="59"/>
<contactref element="R43" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="U$6" pad="P$15"/>
<contactref element="U$6" pad="P$16"/>
</signal>
<signal name="CH1_EN">
<contactref element="IC1" pad="6"/>
<contactref element="R36" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="U$5" pad="P$15"/>
<contactref element="U$5" pad="P$16"/>
</signal>
<signal name="CH2_EN">
<contactref element="IC1" pad="7"/>
<contactref element="R29" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="U$4" pad="P$15"/>
<contactref element="U$4" pad="P$16"/>
</signal>
<signal name="CH3_EN">
<contactref element="IC1" pad="8"/>
<contactref element="C20" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="U$3" pad="P$16"/>
<contactref element="U$3" pad="P$15"/>
</signal>
<signal name="CH4_EN">
<contactref element="IC1" pad="9"/>
<contactref element="R50" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="U$7" pad="P$15"/>
<contactref element="U$7" pad="P$16"/>
</signal>
<signal name="TDO/SWO">
<contactref element="IC1" pad="1"/>
<contactref element="JTAG_LPC" pad="13"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="TDI">
<contactref element="IC1" pad="2"/>
<contactref element="JTAG_LPC" pad="5"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="TMS/SWDIO">
<contactref element="IC1" pad="3"/>
<contactref element="JTAG_LPC" pad="7"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="TRST">
<contactref element="IC1" pad="4"/>
<contactref element="JTAG_LPC" pad="3"/>
</signal>
<signal name="TCK/SWDCLK">
<contactref element="IC1" pad="5"/>
<contactref element="JTAG_LPC" pad="9"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="RTCK">
<contactref element="JTAG_LPC" pad="11"/>
<contactref element="IC1" pad="100"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="JTAG_LPC" pad="17"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="D-">
<contactref element="R18" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="X1" pad="D+"/>
</signal>
<signal name="D+">
<contactref element="R17" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="X1" pad="D-"/>
</signal>
<signal name="N$20">
<contactref element="R18" pad="1"/>
<contactref element="FT230X" pad="6"/>
</signal>
<signal name="N$24">
<contactref element="R17" pad="1"/>
<contactref element="FT230X" pad="7"/>
</signal>
<signal name="VBUS1">
<contactref element="L1" pad="1"/>
<contactref element="FT230X" pad="10"/>
<contactref element="C19" pad="+"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="FT230X" pad="9"/>
<contactref element="FT230X" pad="8"/>
<contactref element="FT230X" pad="1"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="R16" pad="1"/>
<contactref element="PWR_UP" pad="A"/>
</signal>
<signal name="F_TCK">
<contactref element="IC2" pad="47"/>
<contactref element="JTAG_A3PN" pad="1"/>
<contactref element="R83" pad="2"/>
<contactref element="IC1" pad="95"/>
</signal>
<signal name="F_TRST">
<contactref element="R84" pad="2"/>
<contactref element="JTAG_A3PN" pad="8"/>
<contactref element="IC2" pad="55"/>
<contactref element="IC1" pad="91"/>
</signal>
<signal name="F_TDI">
<contactref element="IC2" pad="48"/>
<contactref element="JTAG_A3PN" pad="9"/>
<contactref element="IC1" pad="92"/>
</signal>
<signal name="F_TDO">
<contactref element="IC2" pad="54"/>
<contactref element="JTAG_A3PN" pad="3"/>
<contactref element="IC1" pad="94"/>
</signal>
<signal name="F_TMS">
<contactref element="IC2" pad="49"/>
<contactref element="JTAG_A3PN" pad="5"/>
<contactref element="IC1" pad="93"/>
</signal>
<signal name="DATA13">
<contactref element="IC1" pad="68"/>
<contactref element="IC2" pad="98"/>
</signal>
<signal name="DATA12">
<contactref element="IC1" pad="69"/>
<contactref element="IC2" pad="97"/>
</signal>
<signal name="DATA11">
<contactref element="IC1" pad="70"/>
<contactref element="IC2" pad="96"/>
</signal>
<signal name="DATA10">
<contactref element="IC1" pad="73"/>
<contactref element="IC2" pad="95"/>
</signal>
<signal name="DATA9">
<contactref element="IC1" pad="74"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="DATA6">
<contactref element="IC1" pad="36"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="DATA5">
<contactref element="IC1" pad="35"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="DATA4">
<contactref element="IC1" pad="34"/>
<contactref element="IC2" pad="19"/>
</signal>
<signal name="DATA3">
<contactref element="IC1" pad="33"/>
<contactref element="IC2" pad="20"/>
</signal>
<signal name="DATA2">
<contactref element="IC1" pad="32"/>
<contactref element="IC2" pad="21"/>
</signal>
<signal name="DATA1">
<contactref element="IC1" pad="86"/>
<contactref element="IC2" pad="22"/>
</signal>
<signal name="DATA0">
<contactref element="IC1" pad="87"/>
<contactref element="IC2" pad="23"/>
</signal>
<signal name="DATA7">
<contactref element="IC1" pad="37"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="+5V">
<contactref element="CH8" pad="P2"/>
<contactref element="CH1" pad="P2"/>
<contactref element="CH7" pad="P2"/>
<contactref element="CH5" pad="P2"/>
<contactref element="CH4" pad="P2"/>
<contactref element="CH3" pad="P2"/>
<contactref element="CH2" pad="P2"/>
<contactref element="CH6" pad="P2"/>
<contactref element="LM2" pad="1"/>
<contactref element="C32" pad="+"/>
<contactref element="LM2" pad="3"/>
<contactref element="LM1" pad="1"/>
<contactref element="C2" pad="+"/>
<contactref element="L1" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="X1" pad="VBUS"/>
<contactref element="TP10" pad="TP"/>
<contactref element="C34" pad="+"/>
<contactref element="C51" pad="+"/>
<contactref element="C52" pad="+"/>
<contactref element="C53" pad="+"/>
<contactref element="C54" pad="+"/>
<contactref element="C55" pad="+"/>
<contactref element="C56" pad="+"/>
<contactref element="C57" pad="+"/>
<contactref element="TP11" pad="TP"/>
</signal>
<signal name="VLPC_3V3">
<contactref element="JTAG_LPC" pad="2"/>
<contactref element="JTAG_LPC" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="IC1" pad="10"/>
<contactref element="C11" pad="2"/>
<contactref element="IC1" pad="19"/>
<contactref element="IC1" pad="84"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="IC1" pad="42"/>
<contactref element="IC1" pad="96"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="IC1" pad="71"/>
<contactref element="IC1" pad="54"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="IC1" pad="28"/>
<contactref element="C13" pad="2"/>
<contactref element="IC1" pad="12"/>
<contactref element="R9" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="LM2" pad="4"/>
<contactref element="L4" pad="P$2"/>
<contactref element="C31" pad="+"/>
<contactref element="C33" pad="1"/>
<contactref element="LM3671" pad="1"/>
<contactref element="C36" pad="+"/>
<contactref element="LED4" pad="A"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED1" pad="A"/>
<contactref element="TP6" pad="TP"/>
<contactref element="HCH5" pad="14"/>
<contactref element="HCH6" pad="14"/>
<contactref element="HCH7" pad="14"/>
<contactref element="HCH4" pad="14"/>
<contactref element="HCH3" pad="14"/>
<contactref element="HCH2" pad="14"/>
<contactref element="HCH1" pad="14"/>
<contactref element="HCH8" pad="14"/>
<contactref element="R21" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="R29" pad="2"/>
<contactref element="U$3" pad="P$2"/>
<contactref element="U$4" pad="P$2"/>
<contactref element="R35" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="R31" pad="2"/>
<contactref element="R32" pad="2"/>
<contactref element="R33" pad="2"/>
<contactref element="R34" pad="2"/>
<contactref element="R36" pad="2"/>
<contactref element="U$5" pad="P$2"/>
<contactref element="R42" pad="2"/>
<contactref element="R37" pad="2"/>
<contactref element="R38" pad="2"/>
<contactref element="R39" pad="2"/>
<contactref element="R40" pad="2"/>
<contactref element="R41" pad="2"/>
<contactref element="R43" pad="2"/>
<contactref element="U$6" pad="P$2"/>
<contactref element="R70" pad="2"/>
<contactref element="R65" pad="2"/>
<contactref element="R66" pad="2"/>
<contactref element="R67" pad="2"/>
<contactref element="R68" pad="2"/>
<contactref element="R69" pad="2"/>
<contactref element="R71" pad="2"/>
<contactref element="U$10" pad="P$2"/>
<contactref element="R63" pad="2"/>
<contactref element="R58" pad="2"/>
<contactref element="R59" pad="2"/>
<contactref element="R60" pad="2"/>
<contactref element="R61" pad="2"/>
<contactref element="R62" pad="2"/>
<contactref element="R64" pad="2"/>
<contactref element="U$9" pad="P$2"/>
<contactref element="R56" pad="2"/>
<contactref element="R51" pad="2"/>
<contactref element="R52" pad="2"/>
<contactref element="R53" pad="2"/>
<contactref element="R54" pad="2"/>
<contactref element="R55" pad="2"/>
<contactref element="R57" pad="2"/>
<contactref element="U$8" pad="P$2"/>
<contactref element="R49" pad="2"/>
<contactref element="R44" pad="2"/>
<contactref element="R45" pad="2"/>
<contactref element="R46" pad="2"/>
<contactref element="R47" pad="2"/>
<contactref element="R48" pad="2"/>
<contactref element="R50" pad="2"/>
<contactref element="U$7" pad="P$2"/>
</signal>
<signal name="VA3IO_3V3">
<contactref element="IC2" pad="18"/>
<contactref element="C42" pad="2"/>
<contactref element="IC2" pad="39"/>
<contactref element="C43" pad="2"/>
<contactref element="IC2" pad="66"/>
<contactref element="C44" pad="2"/>
<contactref element="IC2" pad="87"/>
<contactref element="C45" pad="2"/>
<contactref element="IC2" pad="74"/>
<contactref element="C47" pad="2"/>
<contactref element="IC2" pad="24"/>
<contactref element="C48" pad="2"/>
<contactref element="IC2" pad="50"/>
<contactref element="C49" pad="2"/>
<contactref element="LM1" pad="4"/>
<contactref element="L3" pad="P$2"/>
<contactref element="C1" pad="+"/>
<contactref element="C30" pad="1"/>
<contactref element="TP4" pad="TP"/>
<contactref element="IC2" pad="52"/>
<contactref element="JTAG_A3PN" pad="7"/>
<contactref element="C28" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="IC2" pad="56"/>
<contactref element="JTAG_A3PN" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="LM3671" pad="5"/>
<contactref element="L2" pad="P$1"/>
</signal>
<signal name="VA3CORE_1V5">
<contactref element="LM3671" pad="4"/>
<contactref element="L2" pad="P$2"/>
<contactref element="C35" pad="+"/>
<contactref element="C37" pad="1"/>
<contactref element="IC2" pad="14"/>
<contactref element="C46" pad="2"/>
<contactref element="IC2" pad="89"/>
<contactref element="C41" pad="2"/>
<contactref element="IC2" pad="68"/>
<contactref element="C40" pad="2"/>
<contactref element="IC2" pad="17"/>
<contactref element="C38" pad="2"/>
<contactref element="IC2" pad="37"/>
<contactref element="C39" pad="2"/>
<contactref element="C50" pad="2"/>
<contactref element="TP5" pad="TP"/>
</signal>
<signal name="CH4_OC">
<contactref element="HCH3" pad="1"/>
<contactref element="IC2" pad="46"/>
<contactref element="R21" pad="1"/>
<contactref element="U$3" pad="P$8"/>
</signal>
<signal name="CH4_IC">
<contactref element="HCH3" pad="3"/>
<contactref element="IC2" pad="45"/>
<contactref element="R20" pad="1"/>
<contactref element="U$3" pad="P$7"/>
</signal>
<signal name="CH4_OB">
<contactref element="HCH3" pad="5"/>
<contactref element="IC2" pad="44"/>
<contactref element="R19" pad="1"/>
<contactref element="U$3" pad="P$6"/>
</signal>
<signal name="CH4_IB">
<contactref element="HCH3" pad="7"/>
<contactref element="IC2" pad="43"/>
<contactref element="R3" pad="1"/>
<contactref element="U$3" pad="P$5"/>
</signal>
<signal name="CH4_OA">
<contactref element="HCH3" pad="9"/>
<contactref element="IC2" pad="42"/>
<contactref element="R2" pad="1"/>
<contactref element="U$3" pad="P$4"/>
</signal>
<signal name="CH4_IA">
<contactref element="HCH3" pad="11"/>
<contactref element="IC2" pad="41"/>
<contactref element="R1" pad="1"/>
<contactref element="U$3" pad="P$3"/>
</signal>
<signal name="CH3_OC">
<contactref element="HCH2" pad="1"/>
<contactref element="IC2" pad="40"/>
<contactref element="R23" pad="1"/>
<contactref element="U$4" pad="P$8"/>
</signal>
<signal name="CH3_IC">
<contactref element="HCH2" pad="3"/>
<contactref element="IC2" pad="36"/>
<contactref element="R24" pad="1"/>
<contactref element="U$4" pad="P$7"/>
</signal>
<signal name="CH3_OB">
<contactref element="HCH2" pad="5"/>
<contactref element="IC2" pad="35"/>
<contactref element="R25" pad="1"/>
<contactref element="U$4" pad="P$6"/>
</signal>
<signal name="CH3_IB">
<contactref element="HCH2" pad="7"/>
<contactref element="IC2" pad="34"/>
<contactref element="R26" pad="1"/>
<contactref element="U$4" pad="P$5"/>
</signal>
<signal name="CH3_OA">
<contactref element="HCH2" pad="9"/>
<contactref element="IC2" pad="33"/>
<contactref element="R27" pad="1"/>
<contactref element="U$4" pad="P$4"/>
</signal>
<signal name="CH3_IA">
<contactref element="HCH2" pad="11"/>
<contactref element="IC2" pad="32"/>
<contactref element="R28" pad="1"/>
<contactref element="U$4" pad="P$3"/>
</signal>
<signal name="CH2_OC">
<contactref element="HCH1" pad="1"/>
<contactref element="IC2" pad="31"/>
<contactref element="R30" pad="1"/>
<contactref element="U$5" pad="P$8"/>
</signal>
<signal name="CH2_IC">
<contactref element="HCH1" pad="3"/>
<contactref element="IC2" pad="30"/>
<contactref element="R31" pad="1"/>
<contactref element="U$5" pad="P$7"/>
</signal>
<signal name="CH2_OB">
<contactref element="HCH1" pad="5"/>
<contactref element="IC2" pad="29"/>
<contactref element="R32" pad="1"/>
<contactref element="U$5" pad="P$6"/>
</signal>
<signal name="CH2_IB">
<contactref element="HCH1" pad="7"/>
<contactref element="IC2" pad="28"/>
<contactref element="R33" pad="1"/>
<contactref element="U$5" pad="P$5"/>
</signal>
<signal name="CH2_OA">
<contactref element="HCH1" pad="9"/>
<contactref element="IC2" pad="27"/>
<contactref element="R34" pad="1"/>
<contactref element="U$5" pad="P$4"/>
</signal>
<signal name="CH2_IA">
<contactref element="HCH1" pad="11"/>
<contactref element="IC2" pad="26"/>
<contactref element="R35" pad="1"/>
<contactref element="U$5" pad="P$3"/>
</signal>
<signal name="CH1_OC">
<contactref element="HCH8" pad="1"/>
<contactref element="IC2" pad="94"/>
<contactref element="R37" pad="1"/>
<contactref element="U$6" pad="P$8"/>
</signal>
<signal name="CH1_IC">
<contactref element="HCH8" pad="3"/>
<contactref element="IC2" pad="93"/>
<contactref element="U$6" pad="P$7"/>
<contactref element="R38" pad="1"/>
</signal>
<signal name="CH1_OB">
<contactref element="HCH8" pad="5"/>
<contactref element="IC2" pad="92"/>
<contactref element="R39" pad="1"/>
<contactref element="U$6" pad="P$6"/>
</signal>
<signal name="CH1_IB">
<contactref element="HCH8" pad="7"/>
<contactref element="IC2" pad="91"/>
<contactref element="R40" pad="1"/>
<contactref element="U$6" pad="P$5"/>
</signal>
<signal name="CH1_OA">
<contactref element="HCH8" pad="9"/>
<contactref element="IC2" pad="90"/>
<contactref element="R41" pad="1"/>
<contactref element="U$6" pad="P$4"/>
</signal>
<signal name="CH1_IA">
<contactref element="HCH8" pad="11"/>
<contactref element="IC2" pad="86"/>
<contactref element="R42" pad="1"/>
<contactref element="U$6" pad="P$3"/>
</signal>
<signal name="CH5_OC">
<contactref element="IC2" pad="62"/>
<contactref element="HCH4" pad="1"/>
<contactref element="R44" pad="1"/>
<contactref element="U$7" pad="P$8"/>
</signal>
<signal name="CH5_IC">
<contactref element="IC2" pad="61"/>
<contactref element="HCH4" pad="3"/>
<contactref element="U$7" pad="P$7"/>
<contactref element="R45" pad="1"/>
</signal>
<signal name="CH5_OB">
<contactref element="IC2" pad="60"/>
<contactref element="HCH4" pad="5"/>
<contactref element="R46" pad="1"/>
<contactref element="U$7" pad="P$6"/>
</signal>
<signal name="CH5_IB">
<contactref element="IC2" pad="59"/>
<contactref element="HCH4" pad="7"/>
<contactref element="R47" pad="1"/>
<contactref element="U$7" pad="P$5"/>
</signal>
<signal name="CH5_OA">
<contactref element="IC2" pad="58"/>
<contactref element="HCH4" pad="9"/>
<contactref element="R48" pad="1"/>
<contactref element="U$7" pad="P$4"/>
</signal>
<signal name="CH5_IA">
<contactref element="IC2" pad="57"/>
<contactref element="HCH4" pad="11"/>
<contactref element="R49" pad="1"/>
<contactref element="U$7" pad="P$3"/>
</signal>
<signal name="CH6_OC">
<contactref element="HCH5" pad="1"/>
<contactref element="IC2" pad="71"/>
<contactref element="R51" pad="1"/>
<contactref element="U$8" pad="P$8"/>
</signal>
<signal name="CH6_IC">
<contactref element="HCH5" pad="3"/>
<contactref element="IC2" pad="70"/>
<contactref element="U$8" pad="P$7"/>
<contactref element="R52" pad="1"/>
</signal>
<signal name="CH6_OB">
<contactref element="HCH5" pad="5"/>
<contactref element="IC2" pad="69"/>
<contactref element="R53" pad="1"/>
<contactref element="U$8" pad="P$6"/>
</signal>
<signal name="CH6_IB">
<contactref element="HCH5" pad="7"/>
<contactref element="IC2" pad="65"/>
<contactref element="R54" pad="1"/>
<contactref element="U$8" pad="P$5"/>
</signal>
<signal name="CH6_OA">
<contactref element="HCH5" pad="9"/>
<contactref element="IC2" pad="64"/>
<contactref element="R55" pad="1"/>
<contactref element="U$8" pad="P$4"/>
</signal>
<signal name="CH6_IA">
<contactref element="HCH5" pad="11"/>
<contactref element="IC2" pad="63"/>
<contactref element="R56" pad="1"/>
<contactref element="U$8" pad="P$3"/>
</signal>
<signal name="CH7_OC">
<contactref element="IC2" pad="79"/>
<contactref element="HCH6" pad="1"/>
<contactref element="R58" pad="1"/>
<contactref element="U$9" pad="P$8"/>
</signal>
<signal name="CH7_IC">
<contactref element="IC2" pad="78"/>
<contactref element="HCH6" pad="3"/>
<contactref element="U$9" pad="P$7"/>
<contactref element="R59" pad="1"/>
</signal>
<signal name="CH7_OB">
<contactref element="IC2" pad="77"/>
<contactref element="HCH6" pad="5"/>
<contactref element="R60" pad="1"/>
<contactref element="U$9" pad="P$6"/>
</signal>
<signal name="CH7_IB">
<contactref element="IC2" pad="76"/>
<contactref element="HCH6" pad="7"/>
<contactref element="R61" pad="1"/>
<contactref element="U$9" pad="P$5"/>
</signal>
<signal name="CH7_OA">
<contactref element="IC2" pad="73"/>
<contactref element="HCH6" pad="9"/>
<contactref element="R62" pad="1"/>
<contactref element="U$9" pad="P$4"/>
</signal>
<signal name="CH7_IA">
<contactref element="IC2" pad="72"/>
<contactref element="HCH6" pad="11"/>
<contactref element="R63" pad="1"/>
<contactref element="U$9" pad="P$3"/>
</signal>
<signal name="CH8_OC">
<contactref element="IC2" pad="85"/>
<contactref element="HCH7" pad="1"/>
<contactref element="R65" pad="1"/>
<contactref element="U$10" pad="P$8"/>
</signal>
<signal name="CH8_IC">
<contactref element="IC2" pad="84"/>
<contactref element="HCH7" pad="3"/>
<contactref element="U$10" pad="P$7"/>
<contactref element="R66" pad="1"/>
</signal>
<signal name="CH8_OB">
<contactref element="IC2" pad="83"/>
<contactref element="HCH7" pad="5"/>
<contactref element="R67" pad="1"/>
<contactref element="U$10" pad="P$6"/>
</signal>
<signal name="CH8_IB">
<contactref element="IC2" pad="82"/>
<contactref element="HCH7" pad="7"/>
<contactref element="R68" pad="1"/>
<contactref element="U$10" pad="P$5"/>
</signal>
<signal name="CH8_OA">
<contactref element="IC2" pad="81"/>
<contactref element="HCH7" pad="9"/>
<contactref element="R69" pad="1"/>
<contactref element="U$10" pad="P$4"/>
</signal>
<signal name="CH8_IA">
<contactref element="IC2" pad="80"/>
<contactref element="HCH7" pad="11"/>
<contactref element="R70" pad="1"/>
<contactref element="U$10" pad="P$3"/>
</signal>
<signal name="CLK">
<contactref element="IC1" pad="43"/>
<contactref element="IC2" pad="11"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="CH4_TIA">
<contactref element="CH4" pad="P3"/>
<contactref element="HCH4" pad="12"/>
<contactref element="U$7" pad="P$14"/>
</signal>
<signal name="CH4_TOB">
<contactref element="HCH4" pad="6"/>
<contactref element="CH4" pad="P6"/>
<contactref element="U$7" pad="P$11"/>
</signal>
<signal name="CH4_TIB">
<contactref element="CH4" pad="P5"/>
<contactref element="HCH4" pad="8"/>
<contactref element="U$7" pad="P$12"/>
</signal>
<signal name="CH4_TOA">
<contactref element="HCH4" pad="10"/>
<contactref element="CH4" pad="P4"/>
<contactref element="U$7" pad="P$13"/>
</signal>
<signal name="CH4_TIC">
<contactref element="CH4" pad="P7"/>
<contactref element="HCH4" pad="4"/>
<contactref element="U$7" pad="P$10"/>
</signal>
<signal name="CH4_TOC">
<contactref element="CH4" pad="P8"/>
<contactref element="HCH4" pad="2"/>
<contactref element="U$7" pad="P$9"/>
</signal>
<signal name="CH3_TIA">
<contactref element="CH3" pad="P3"/>
<contactref element="HCH3" pad="12"/>
<contactref element="U$3" pad="P$14"/>
</signal>
<signal name="CH3_TOB">
<contactref element="U$3" pad="P$11"/>
<contactref element="HCH3" pad="6"/>
<contactref element="CH3" pad="P6"/>
</signal>
<signal name="CH3_TIB">
<contactref element="CH3" pad="P5"/>
<contactref element="HCH3" pad="8"/>
<contactref element="U$3" pad="P$12"/>
</signal>
<signal name="CH3_TOA">
<contactref element="U$3" pad="P$13"/>
<contactref element="HCH3" pad="10"/>
<contactref element="CH3" pad="P4"/>
</signal>
<signal name="CH3_TIC">
<contactref element="CH3" pad="P7"/>
<contactref element="HCH3" pad="4"/>
<contactref element="U$3" pad="P$10"/>
</signal>
<signal name="CH3_TOC">
<contactref element="CH3" pad="P8"/>
<contactref element="HCH3" pad="2"/>
<contactref element="U$3" pad="P$9"/>
</signal>
<signal name="CH2_TIA">
<contactref element="CH2" pad="P3"/>
<contactref element="HCH2" pad="12"/>
<contactref element="U$4" pad="P$14"/>
</signal>
<signal name="CH2_TOB">
<contactref element="HCH2" pad="6"/>
<contactref element="CH2" pad="P6"/>
<contactref element="U$4" pad="P$11"/>
</signal>
<signal name="CH2_TIB">
<contactref element="CH2" pad="P5"/>
<contactref element="HCH2" pad="8"/>
<contactref element="U$4" pad="P$12"/>
</signal>
<signal name="CH2_TOA">
<contactref element="HCH2" pad="10"/>
<contactref element="CH2" pad="P4"/>
<contactref element="U$4" pad="P$13"/>
</signal>
<signal name="CH2_TIC">
<contactref element="CH2" pad="P7"/>
<contactref element="HCH2" pad="4"/>
<contactref element="U$4" pad="P$10"/>
</signal>
<signal name="CH2_TOC">
<contactref element="CH2" pad="P8"/>
<contactref element="HCH2" pad="2"/>
<contactref element="U$4" pad="P$9"/>
</signal>
<signal name="CH1_TIA">
<contactref element="HCH1" pad="12"/>
<contactref element="CH1" pad="P3"/>
<contactref element="U$5" pad="P$14"/>
</signal>
<signal name="CH1_TOB">
<contactref element="HCH1" pad="6"/>
<contactref element="CH1" pad="P6"/>
<contactref element="U$5" pad="P$11"/>
</signal>
<signal name="CH1_TIB">
<contactref element="HCH1" pad="8"/>
<contactref element="CH1" pad="P5"/>
<contactref element="U$5" pad="P$12"/>
</signal>
<signal name="CH1_TOA">
<contactref element="HCH1" pad="10"/>
<contactref element="CH1" pad="P4"/>
<contactref element="U$5" pad="P$13"/>
</signal>
<signal name="CH1_TIC">
<contactref element="HCH1" pad="4"/>
<contactref element="CH1" pad="P7"/>
<contactref element="U$5" pad="P$10"/>
</signal>
<signal name="CH1_TOC">
<contactref element="HCH1" pad="2"/>
<contactref element="CH1" pad="P8"/>
<contactref element="U$5" pad="P$9"/>
</signal>
<signal name="CH5_TIA">
<contactref element="CH5" pad="P3"/>
<contactref element="HCH5" pad="12"/>
<contactref element="U$8" pad="P$14"/>
</signal>
<signal name="CH5_TOB">
<contactref element="HCH5" pad="6"/>
<contactref element="CH5" pad="P6"/>
<contactref element="U$8" pad="P$11"/>
</signal>
<signal name="CH5_TIB">
<contactref element="CH5" pad="P5"/>
<contactref element="HCH5" pad="8"/>
<contactref element="U$8" pad="P$12"/>
</signal>
<signal name="CH5_TOA">
<contactref element="HCH5" pad="10"/>
<contactref element="CH5" pad="P4"/>
<contactref element="U$8" pad="P$13"/>
</signal>
<signal name="CH5_TIC">
<contactref element="CH5" pad="P7"/>
<contactref element="HCH5" pad="4"/>
<contactref element="U$8" pad="P$10"/>
</signal>
<signal name="CH5_TOC">
<contactref element="CH5" pad="P8"/>
<contactref element="HCH5" pad="2"/>
<contactref element="U$8" pad="P$9"/>
</signal>
<signal name="CH6_TIA">
<contactref element="CH6" pad="P3"/>
<contactref element="HCH6" pad="12"/>
<contactref element="U$9" pad="P$14"/>
</signal>
<signal name="CH6_TOB">
<contactref element="HCH6" pad="6"/>
<contactref element="CH6" pad="P6"/>
<contactref element="U$9" pad="P$11"/>
</signal>
<signal name="CH6_TIB">
<contactref element="CH6" pad="P5"/>
<contactref element="HCH6" pad="8"/>
<contactref element="U$9" pad="P$12"/>
</signal>
<signal name="CH6_TOA">
<contactref element="HCH6" pad="10"/>
<contactref element="CH6" pad="P4"/>
<contactref element="U$9" pad="P$13"/>
</signal>
<signal name="CH6_TIC">
<contactref element="CH6" pad="P7"/>
<contactref element="HCH6" pad="4"/>
<contactref element="U$9" pad="P$10"/>
</signal>
<signal name="CH6_TOC">
<contactref element="CH6" pad="P8"/>
<contactref element="HCH6" pad="2"/>
<contactref element="U$9" pad="P$9"/>
</signal>
<signal name="CH7_TIA">
<contactref element="CH7" pad="P3"/>
<contactref element="HCH7" pad="12"/>
<contactref element="U$10" pad="P$14"/>
</signal>
<signal name="CH7_TOB">
<contactref element="HCH7" pad="6"/>
<contactref element="CH7" pad="P6"/>
<contactref element="U$10" pad="P$11"/>
</signal>
<signal name="CH7_TIB">
<contactref element="CH7" pad="P5"/>
<contactref element="HCH7" pad="8"/>
<contactref element="U$10" pad="P$12"/>
</signal>
<signal name="CH7_TOA">
<contactref element="HCH7" pad="10"/>
<contactref element="CH7" pad="P4"/>
<contactref element="U$10" pad="P$13"/>
</signal>
<signal name="CH7_TIC">
<contactref element="CH7" pad="P7"/>
<contactref element="HCH7" pad="4"/>
<contactref element="U$10" pad="P$10"/>
</signal>
<signal name="CH7_TOC">
<contactref element="CH7" pad="P8"/>
<contactref element="HCH7" pad="2"/>
<contactref element="U$10" pad="P$9"/>
</signal>
<signal name="CH8_TIA">
<contactref element="HCH8" pad="12"/>
<contactref element="CH8" pad="P3"/>
<contactref element="U$6" pad="P$14"/>
</signal>
<signal name="CH8_TOB">
<contactref element="HCH8" pad="6"/>
<contactref element="CH8" pad="P6"/>
<contactref element="U$6" pad="P$11"/>
</signal>
<signal name="CH8_TIB">
<contactref element="HCH8" pad="8"/>
<contactref element="CH8" pad="P5"/>
<contactref element="U$6" pad="P$12"/>
</signal>
<signal name="CH8_TOA">
<contactref element="HCH8" pad="10"/>
<contactref element="CH8" pad="P4"/>
<contactref element="U$6" pad="P$13"/>
</signal>
<signal name="CH8_TIC">
<contactref element="HCH8" pad="4"/>
<contactref element="CH8" pad="P7"/>
<contactref element="U$6" pad="P$10"/>
</signal>
<signal name="CH8_TOC">
<contactref element="HCH8" pad="2"/>
<contactref element="CH8" pad="P8"/>
<contactref element="U$6" pad="P$9"/>
</signal>
<signal name="EN_IO">
<contactref element="LM1" pad="3"/>
<contactref element="IC1" pad="61"/>
</signal>
<signal name="N$85">
<contactref element="LM1" pad="5"/>
<contactref element="L3" pad="P$1"/>
</signal>
<signal name="N$86">
<contactref element="LM2" pad="5"/>
<contactref element="L4" pad="P$1"/>
</signal>
<signal name="EN_CORE">
<contactref element="LM3671" pad="3"/>
<contactref element="IC1" pad="60"/>
</signal>
<signal name="TX1">
<contactref element="IC1" pad="62"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="RX1">
<contactref element="IC1" pad="63"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="DATA8">
<contactref element="IC1" pad="75"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="DATA14">
<contactref element="IC1" pad="67"/>
<contactref element="IC2" pad="99"/>
</signal>
<signal name="DATA15">
<contactref element="IC1" pad="66"/>
<contactref element="IC2" pad="100"/>
</signal>
<signal name="N$25">
<contactref element="LED4" pad="C"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="LED3" pad="C"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="LED2" pad="C"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="LED1" pad="C"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="N$2">
</signal>
</signals>
</board>
</drawing>
</eagle>
