<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="58.4" y2="0" width="0" layer="20"/>
<wire x1="58.4" y1="0" x2="58.42" y2="45.72" width="0" layer="20"/>
<wire x1="58.42" y1="45.72" x2="0" y2="45.72" width="0" layer="20"/>
<wire x1="0" y1="45.72" x2="0" y2="0" width="0" layer="20"/>
<text>VCC</text>
<text>GND</text>
<text>RST</text>
<text>SWCLK</text>
<text>SWDIO</text>
<text>TRG</text>
<text>GPO</text>
<text>RST</text>
<text>GPI</text>
<text>VCC</text>
<text>RXD</text>
<text>TXD</text>
<text>SIGI</text>
<text>SIGO</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>SCL</text>
<text>GND</text>
<text>PSU</text>
<text>GND</text>
<text>GND</text>
<text>CLK</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>SDA</text>
<text>http://www.github.com/danpage/scale</text>
<text>SCALE
target board
rev. C.1
(lpc812m101jdh16)
</text>
<text>CLK</text>
<text>XTAL</text>
<text>CLK</text>
<text>XTAL</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>RXD</text>
<text>TXD</text>
<text>RXD</text>
<text>TXD</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X16">
<description>&lt;h3&gt;Plated Through Hole -16 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:16&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_16&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
</package>
<package name="2X10">
<description>&lt;h3&gt;Plated Through Hole - 2x10&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="board">
<packages>
<package name="TSSOP16">
<description>TSSOP16</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="T.J6" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T.J5" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T.J1R" library="SparkFun-Connectors" package="1X16" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T.J1L" library="SparkFun-Connectors" package="1X16" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T.XTAL" library="SparkFun-FreqCtrl" package="HC49US" value="16 Mhz">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="T.C2" library="SparkFun-Capacitors" package="0603-CAP" value="0.018 nF = 18 pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T.C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.018 nF = 18 pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T.C4" library="SparkFun-Capacitors" package="0603-CAP" value="0.1 nF = 100 pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T.J3" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T.J4" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T.C3" library="SparkFun-Capacitors" package="0603-CAP" value="0.3 nF = 300 pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T.J2" library="SparkFun-Connectors" package="2X10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T.DUT" library="board" package="TSSOP16" value="LPC812M101JDH16">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="T.J1L" pad="11"/>
<contactref element="T.J1L" pad="10"/>
<contactref element="T.J1L" pad="8"/>
<contactref element="T.J1L" pad="7"/>
<contactref element="T.J1L" pad="16"/>
<contactref element="T.J1R" pad="13"/>
<contactref element="T.J1R" pad="12"/>
<contactref element="T.J1R" pad="11"/>
<contactref element="T.J1R" pad="10"/>
<contactref element="T.J1R" pad="4"/>
<contactref element="T.J1R" pad="3"/>
<contactref element="T.J1R" pad="1"/>
<contactref element="T.J1R" pad="5"/>
<contactref element="T.C1" pad="1"/>
<contactref element="T.C2" pad="1"/>
<contactref element="T.C3" pad="1"/>
<contactref element="T.J1L" pad="6"/>
<contactref element="T.J1L" pad="4"/>
<contactref element="T.J1R" pad="16"/>
<contactref element="T.J1L" pad="3"/>
<contactref element="T.J1L" pad="1"/>
<contactref element="T.J1L" pad="14"/>
<contactref element="T.J2" pad="20"/>
<contactref element="T.J2" pad="18"/>
<contactref element="T.J2" pad="16"/>
<contactref element="T.J2" pad="14"/>
<contactref element="T.J2" pad="12"/>
<contactref element="T.J2" pad="10"/>
<contactref element="T.J2" pad="8"/>
<contactref element="T.J2" pad="6"/>
<contactref element="T.J2" pad="4"/>
<contactref element="T.DUT" pad="13"/>
</signal>
<signal name="DUT_RST">
<contactref element="T.J1R" pad="7"/>
<contactref element="T.J2" pad="15"/>
<contactref element="T.DUT" pad="3"/>
</signal>
<signal name="DUT_TRG">
<contactref element="T.J1R" pad="9"/>
<contactref element="T.DUT" pad="15"/>
</signal>
<signal name="DUT_SIGO">
<contactref element="T.J1R" pad="2"/>
</signal>
<signal name="DUT_RXD">
<contactref element="T.J6" pad="1"/>
<contactref element="T.J1L" pad="12"/>
</signal>
<signal name="DUT_TXD">
<contactref element="T.J5" pad="1"/>
<contactref element="T.J1L" pad="13"/>
</signal>
<signal name="DUT_CLK">
<contactref element="T.C4" pad="2"/>
<contactref element="T.J1L" pad="9"/>
</signal>
<signal name="DUT_SIGI">
<contactref element="T.J1L" pad="2"/>
</signal>
<signal name="DUT_VCC">
<contactref element="T.J1L" pad="5"/>
<contactref element="T.J2" pad="1"/>
<contactref element="T.DUT" pad="12"/>
</signal>
<signal name="N$28">
<contactref element="T.J6" pad="2"/>
<contactref element="T.DUT" pad="16"/>
</signal>
<signal name="N$27">
<contactref element="T.J5" pad="2"/>
<contactref element="T.DUT" pad="4"/>
</signal>
<signal name="DUT_XTAL2">
<contactref element="T.J4" pad="2"/>
<contactref element="T.DUT" pad="10"/>
</signal>
<signal name="DUT_XTAL1">
<contactref element="T.J3" pad="2"/>
<contactref element="T.DUT" pad="11"/>
</signal>
<signal name="N$20">
<contactref element="T.C4" pad="1"/>
<contactref element="T.J3" pad="3"/>
<contactref element="T.C3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="T.J3" pad="1"/>
<contactref element="T.C1" pad="2"/>
<contactref element="T.XTAL" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="T.J4" pad="1"/>
<contactref element="T.C2" pad="2"/>
<contactref element="T.XTAL" pad="1"/>
</signal>
<signal name="DUT_GPO">
<contactref element="T.J1R" pad="8"/>
<contactref element="T.DUT" pad="14"/>
</signal>
<signal name="DUT_GPI">
<contactref element="T.J1R" pad="6"/>
<contactref element="T.DUT" pad="2"/>
</signal>
<signal name="DUT_SDA">
<contactref element="T.J1R" pad="14"/>
<contactref element="T.DUT" pad="8"/>
</signal>
<signal name="DUT_SCL">
<contactref element="T.J1R" pad="15"/>
<contactref element="T.DUT" pad="7"/>
</signal>
<signal name="PSU">
<contactref element="T.J1L" pad="15"/>
</signal>
<signal name="DUT_SWDIO">
<contactref element="T.J2" pad="7"/>
<contactref element="T.DUT" pad="6"/>
</signal>
<signal name="DUT_SWCLK">
<contactref element="T.J2" pad="9"/>
<contactref element="T.DUT" pad="5"/>
</signal>
<signal name="DUT_SWO">
<contactref element="T.J2" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
