<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="21.59" y2="0" width="0" layer="20"/>
<wire x1="21.59" y1="0" x2="21.59" y2="10.16" width="0" layer="20"/>
<wire x1="21.59" y1="10.16" x2="0" y2="10.16" width="0" layer="20"/>
<wire x1="0" y1="10.16" x2="0" y2="0" width="0" layer="20"/>
<text>PWM</text>
<text>GND</text>
<text>+5V</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-3-PTH">
<description>&lt;h3&gt;JST 3 Pin Right Angle Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LFPAK33">
<description>&lt;b&gt; LFPAK33 using NextPower Technology&lt;/b&gt; SOT1210&lt;p&gt;
PSMN013-30MLC  N-channel 30 V 13.6 mΩ logic level MOSFET&lt;p&gt;
Source: &lt;a href="http://www.nxp.com/documents/data_sheet/PSMN013-30MLC.pdf"&gt; Data sheet &lt;/a&gt;&lt;br&gt;
PSMN013-30MLC © NXP B.V. 2012. All rights reserved.</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0805-THM">
</package>
</packages>
</library>
<library name="we-con">
<description>Connectors, Sockets...</description>
<packages>
<package name="JST_S2B-PH-K">
<description>S2B-PH-K - normal insertion force&lt;br&gt;
S2B-PH-KL - low insertion force</description>
</package>
</packages>
</library>
<library name="we-rcl">
<description>R, C, L, Diodes, Crystals, Pot, Jumper...</description>
<packages>
<package name="SMA_DO214AC">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="SparkFun-Connectors" package="JST-3-PTH" value="">
<attribute name="PROD_ID" value="WIRE-10037"/>
<attribute name="SF_ID" value="PRT-09915"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="transistor-power" package="LFPAK33" value="PSMN013">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PSMN013-30MLC"/>
<attribute name="OC_FARNELL" value="2115260"/>
<attribute name="OC_NEWARK" value="05W5709"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0805-THM" value="470R">
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0805-THM" value="4k7">
<attribute name="VALUE"/>
</element>
<element name="J1" library="we-con" package="JST_S2B-PH-K" value="JST2-S2B-PH-K">
<attribute name="NAME"/>
</element>
<element name="D1" library="we-rcl" package="SMA_DO214AC" value="1N4007">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J2" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="5V">
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="PWM_IN">
<contactref element="J2" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="Q1" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="2"/>
<contactref element="Q1" pad="MB"/>
<contactref element="D1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
