<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="11.41" y2="0" width="0" layer="20"/>
<wire x1="11.41" y1="0" x2="11.41" y2="17.45" width="0" layer="20"/>
<wire x1="11.41" y1="17.45" x2="0" y2="17.45" width="0" layer="20"/>
<wire x1="0" y1="17.45" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="PAM2804AAB010">
<packages>
<package name="SOT95P280X100-5N">
</package>
</packages>
</library>
<library name="LMK212AB7106MG-T">
<packages>
<package name="CAPC2013X140N">
</package>
</packages>
</library>
<library name="ERJ-8BWFR100V">
<packages>
<package name="RESC3216X75N">
</package>
</packages>
</library>
<library name="NRS4010T4R7MDGG">
<packages>
<package name="IND_TAIYO_NRS4010">
</package>
</packages>
</library>
<library name="WL-TMRW">
<packages>
<package name="LED-3MM-ROUND">
<description>WL-TMRC THT LED mono-color round color
lens,Size: 3 mm,</description>
</package>
</packages>
</library>
<library name="PiB_batteries">
<packages>
<package name="DUAL_PTH_PADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="PAM2804AAB010" package="SOT95P280X100-5N" value="PAM2804AAB010">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Cap Aluminum 3300uF 63V 20% _30 X 25mm_ Snap-In Aluminum Cylindrical Can 2330mA 3000 hr 105°C Bulk "/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="PAM2804AAB010"/>
<attribute name="PACKAGE" value="SOT-23-5 Diodes Inc."/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="LMK212AB7106MG-T" package="CAPC2013X140N" value="LMK212AB7106MG-T">
<attribute name="DESCRIPTION" value=" LMK212AB7106MG-T "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="587-3417-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/taiyo-yuden/LMK212AB7106MG-T/587-3417-1-ND/4157381?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MP" value="LMK212AB7106MG-T"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="2012 Taiyo Yuden"/>
</element>
<element name="C2" library="LMK212AB7106MG-T" package="CAPC2013X140N" value="LMK212AB7106MG-T">
<attribute name="DESCRIPTION" value=" LMK212AB7106MG-T "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="587-3417-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/taiyo-yuden/LMK212AB7106MG-T/587-3417-1-ND/4157381?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MP" value="LMK212AB7106MG-T"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="2012 Taiyo Yuden"/>
</element>
<element name="R1" library="ERJ-8BWFR100V" package="RESC3216X75N" value="ERJ-8BWFR100V">
<attribute name="DESCRIPTION" value=" Res Thick Film 1206 0.1 Ohm 1% 1W ±100ppm/°C Molded SMD Automotive Punched T/R "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="P.10AUCT-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/panasonic-electronic-components/ERJ-8BWFR100V/P.10AUCT-ND/1711706?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Panasonic Electronic"/>
<attribute name="MP" value="ERJ-8BWFR100V"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="3216 Panasonic Electronic Components"/>
</element>
<element name="L1" library="NRS4010T4R7MDGG" package="IND_TAIYO_NRS4010" value="NRS4010T4R7MDGG">
<attribute name="MANUFACTURER_PART_NUMBER" value="NRS4010T4R7MDGG"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="TAIYO YUDEN"/>
</element>
<element name="LIPO1" library="PiB_batteries" package="DUAL_PTH_PADS" value="BATTERY_LIPO_2S"/>
<element name="D2" library="WL-TMRW" package="LED-3MM-ROUND" value="WL-TMRW151033BS03000-B">
<attribute name="DESCRIPTION" value=" LED [Würth Elektronik] 151054RS03000 LED "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="732-11408-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/wurth-electronics-inc/151054RS03000/732-11408-ND/7315780?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Wurth Electronics"/>
<attribute name="MP" value="151054RS03000"/>
<attribute name="PACKAGE" value="Radial Würth Elektronik"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="LIPO1" pad="-"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="3"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="L1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="D2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="LIPO1" pad="+"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="PWM-P">
<contactref element="U1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
