<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="-0.5842" y1="22.7076" x2="5.6388" y2="22.7076" width="0.1524" layer="20"/>
<wire x1="5.6388" y1="22.7076" x2="5.6388" y2="7.8486" width="0.1524" layer="20"/>
<wire x1="5.6388" y1="7.8486" x2="-0.5842" y2="7.8486" width="0.1524" layer="20"/>
<wire x1="-0.5842" y1="7.8486" x2="-0.5842" y2="22.7076" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="BNO055">
<packages>
<package name="BNO055">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BNO055" library="BNO055" package="BNO055" value="BNO055A"/>
<element name="_" library="SparkFun-Capacitors" package="1206" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="__" library="SparkFun-Capacitors" package="1206" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VDD" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="GND" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SDA" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SCL" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="_" pad="1"/>
<contactref element="BNO055" pad="9"/>
</signal>
<signal name="GND">
<contactref element="BNO055" pad="6"/>
<contactref element="_" pad="2"/>
<contactref element="BNO055" pad="8"/>
<contactref element="BNO055" pad="7"/>
<contactref element="BNO055" pad="10"/>
<contactref element="BNO055" pad="15"/>
<contactref element="BNO055" pad="16"/>
<contactref element="BNO055" pad="18"/>
<contactref element="BNO055" pad="5"/>
<contactref element="BNO055" pad="2"/>
<contactref element="BNO055" pad="17"/>
<contactref element="BNO055" pad="25"/>
<contactref element="__" pad="2"/>
<contactref element="GND" pad="1"/>
</signal>
<signal name="VDD">
<contactref element="BNO055" pad="28"/>
<contactref element="BNO055" pad="3"/>
<contactref element="__" pad="1"/>
<contactref element="VDD" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="BNO055" pad="20"/>
<contactref element="SDA" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="BNO055" pad="19"/>
<contactref element="SCL" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
