<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="27.432" y1="0" x2="27.432" y2="31.75" width="0" layer="20"/>
<wire x1="27.432" y1="31.75" x2="0" y2="31.75" width="0" layer="20"/>
<wire x1="0" y1="31.75" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="27.432" y2="0" width="0" layer="20"/>
<text>ESP-07/12</text>
<text>RX  TX</text>
<text>CuriousTech.net
</text>
<text>WiFi Garage Door</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="1X02">
</package>
<package name="PIC-ICSP-MINI">
</package>
<package name="USB-MICROB">
<description>Micro USB Package</description>
</package>
<package name="MOLEX-1X3">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805-CAP">
</package>
</packages>
</library>
<library name="CuriousTech">
<description>CuriousTech custom misc parts</description>
<packages>
<package name="SMD-PAD1">
<description>SMD pad 0.2x0.1</description>
</package>
<package name="SIDE-TACT">
</package>
</packages>
</library>
<library name="ESP-07_12">
<packages>
<package name="ESP-07/12">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="Microchip_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 11:22:31</description>
<packages>
<package name="SOT95P270X145-6N">
</package>
<package name="SOT230P700X180-4N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R2" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="R3" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="U$1" library="ESP-07_12" package="ESP-07/12" value="ESP-07/12"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="OLED" library="SparkFun-Connectors" package="1X04" value=""/>
<element name="." library="SparkFun-Connectors" package="1X02" value=""/>
<element name="C1" library="SparkFun-Capacitors" package="0805-CAP" value="0.1uF"/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="P-FET"/>
<element name="U$3" library="CuriousTech" package="SMD-PAD1" value="SMD-PAD1"/>
<element name="10F320" library="Microchip_By_element14_Batch_1" package="SOT95P270X145-6N" value="PIC10F320T-I/OT">
<attribute name="MPN" value="PIC10F220T-I/OT"/>
<attribute name="OC_NEWARK" value="31K4981"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="OC_FARNELL" value="1332175"/>
<attribute name="PACKAGE" value="SOT-6"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="330"/>
<element name="U$9" library="SparkFun-Connectors" package="PIC-ICSP-MINI" value="PIC-ICSP-MINI"/>
<element name="C2" library="SparkFun-Capacitors" package="0805-CAP" value="0.1uF"/>
<element name="JP1" library="SparkFun-Connectors" package="USB-MICROB" value="USB-MICROB">
<attribute name="PROD_ID" value="CONN-09505"/>
</element>
<element name="3V3R" library="Microchip_By_element14_Batch_1" package="SOT230P700X180-4N" value="MCP1824ST-3302E/DB">
<attribute name="MPN" value="MCP1824ST-3302E/DB"/>
<attribute name="PACKAGE" value="SOT-223-3"/>
<attribute name="OC_FARNELL" value="1578379"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="OC_NEWARK" value="05N1293"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="MOLEX-1X3" value=""/>
<element name="JP3" library="SparkFun-Connectors" package="MOLEX-1X3" value=""/>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="SOT23-3" value="">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805-CAP" value="1uF"/>
<element name="JP4" library="SparkFun-Connectors" package="MOLEX-1X3" value=""/>
<element name="R4" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="C3" library="SparkFun-Capacitors" package="0805-CAP" value="0.1uF"/>
<element name="R5" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="R6" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="JP5" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="JP6" library="SparkFun-Connectors" package="MOLEX-1X3" value=""/>
<element name="R8" library="SparkFun-Resistors" package="0805" value="330"/>
<element name="U$2" library="CuriousTech" package="SIDE-TACT" value="SIDE-TACT"/>
<element name="3V3" library="SparkFun-Connectors" package="1X01" value=""/>
</elements>
<signals>
<signal name="IO15">
<contactref element="U$1" pad="GPIO15"/>
<contactref element="R1" pad="2"/>
<contactref element="10F320" pad="6"/>
<contactref element="U$9" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="CH_PD"/>
</signal>
<signal name="3V3">
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="VCC"/>
<contactref element="C1" pad="1"/>
<contactref element="10F320" pad="5"/>
<contactref element="C2" pad="1"/>
<contactref element="3V3R" pad="3"/>
<contactref element="OLED" pad="2"/>
<contactref element="3V3" pad="1"/>
</signal>
<signal name="N$25">
</signal>
<signal name="N$24">
</signal>
<signal name="N$27">
</signal>
<signal name="N$29">
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="10F320" pad="2"/>
<contactref element="U$9" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="3V3R" pad="4"/>
<contactref element="3V3R" pad="2"/>
<contactref element="JP1" pad="GND"/>
<contactref element="JP1" pad="MT1"/>
<contactref element="JP1" pad="MT2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="OLED" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="TXD">
<contactref element="U$1" pad="TXD"/>
<contactref element="." pad="1"/>
</signal>
<signal name="RXD">
<contactref element="U$1" pad="RXD"/>
<contactref element="." pad="2"/>
</signal>
<signal name="ADC">
<contactref element="U$1" pad="ADC"/>
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="IO2">
<contactref element="U$1" pad="GPIO2"/>
<contactref element="10F320" pad="4"/>
</signal>
<signal name="IO12">
<contactref element="U$1" pad="GPIO12"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="IO14">
<contactref element="U$1" pad="GPIO14"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="IO13">
<contactref element="U$1" pad="GPIO13"/>
<contactref element="R8" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="IO16">
<contactref element="U$1" pad="GPIO16"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="IO0">
<contactref element="U$1" pad="GPIO0"/>
<contactref element="JP6" pad="3"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="ICSPCLK">
<contactref element="10F320" pad="3"/>
<contactref element="U$9" pad="5"/>
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="REST"/>
</signal>
<signal name="N$2">
<contactref element="JP2" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="JP3" pad="1"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="2"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="ICSPDAT">
<contactref element="10F320" pad="1"/>
<contactref element="U$9" pad="4"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="GPIO4"/>
<contactref element="OLED" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="OLED" pad="3"/>
<contactref element="U$1" pad="GPIO5"/>
</signal>
<signal name="N$8">
<contactref element="Q1" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="ANA">
<contactref element="R5" pad="2"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="JP1" pad="VBUS"/>
<contactref element="3V3R" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U$3" pad="&gt;NAME"/>
<contactref element="C3" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R7" pad="2"/>
<contactref element="JP5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
