<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="19.5" y2="0" width="0" layer="20"/>
<wire x1="19.5" y1="0" x2="19.5" y2="19" width="0" layer="20"/>
<wire x1="19.5" y1="19" x2="0" y2="19" width="0" layer="20"/>
<wire x1="0" y1="19" x2="0" y2="0" width="0" layer="20"/>
<text>Ghetto PoE</text>
<text>(c) packom.net
2016</text>
<text>5V</text>
<text>v0.1</text>
</plain>
<libraries>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-B-MICRO-SMD_V03">
</package>
</packages>
</library>
<library name="Piers's library">
<packages>
<package name="RJ45_AMPHENOL">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="1.5K">
<attribute name="NAME"/>
</element>
<element name="U$1" library="SparkFun-Connectors" package="USB-B-MICRO-SMD_V03" value="USB-MICROB&quot;">
<attribute name="PROD_ID" value="CONN-11752"/>
</element>
<element name="U$2" library="Piers's library" package="RJ45_AMPHENOL" value="RJ45_AMPHENOL"/>
<element name="F1" library="adafruit" package="R1206" value="0.5A Hold, 1.0A Trip">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="SHIELD1"/>
<contactref element="U$1" pad="SHIELD2"/>
<contactref element="U$1" pad="SHIELD3"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$2" pad="P1"/>
<contactref element="U$2" pad="P3"/>
<contactref element="U$2" pad="P5"/>
<contactref element="U$2" pad="P7"/>
<contactref element="U$2" pad="P9"/>
<contactref element="U$2" pad="P12"/>
<contactref element="U$2" pad="P11"/>
</signal>
<signal name="G_LED">
<contactref element="U$2" pad="P10"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="VBUS"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="P2"/>
<contactref element="U$2" pad="P8"/>
<contactref element="U$2" pad="P6"/>
<contactref element="U$2" pad="P4"/>
<contactref element="R1" pad="2"/>
<contactref element="F1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
