<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="24.1175" y2="0" width="0" layer="20"/>
<wire x1="24.1175" y1="0" x2="24.1175" y2="24.4375" width="0" layer="20"/>
<wire x1="24.1175" y1="24.4375" x2="0" y2="24.4375" width="0" layer="20"/>
<wire x1="0" y1="24.4375" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>VCC</text>
<text>LM555</text>
<text>Rev. A, 2015/09/12
D. Fisher</text>
<text>electronicfish.wordpress.com</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="0207/9">
</package>
<package name="TAP5-50">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5.0 mm, grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="ic-package" package="DIL08" value="LM555">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0207/9" value=""/>
<element name="R2" library="adafruit" package="0207/9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0207/9" value=""/>
<element name="R4" library="adafruit" package="0207/9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="TAP5-50" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="-"/>
</signal>
<signal name="VCC">
<contactref element="JP1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="K"/>
<contactref element="LED2" pad="A"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="LED2" pad="K"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="2"/>
<contactref element="C1" pad="+"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
