<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>Ultra-Sound Array Breakout Board</text>
<text>Thayer School at Dartmouth</text>
<text>Drawn by</text>
<text>Joe Skinner March 2017</text>
<text>1</text>
<text>34</text>
<wire x1="0" y1="3.6576" x2="0" y2="0" width="0.1524" layer="20"/>
<wire x1="0" y1="0" x2="46.0248" y2="0" width="0.1524" layer="20"/>
<wire x1="32.3088" y1="76.5048" x2="13.716" y2="76.5048" width="0.1524" layer="20"/>
<wire x1="13.716" y1="76.5048" x2="13.716" y2="73.6092" width="0.1524" layer="20"/>
<wire x1="13.716" y1="71.7804" x2="13.716" y2="70.866" width="0.1524" layer="20"/>
<wire x1="46.0248" y1="0" x2="46.0248" y2="3.6576" width="0.1524" layer="20"/>
<wire x1="46.0248" y1="3.6576" x2="46.0248" y2="5.7912" width="0.1524" layer="20"/>
<wire x1="46.0248" y1="5.7912" x2="46.0248" y2="7.62" width="0.1524" layer="20"/>
<wire x1="0" y1="7.62" x2="0" y2="3.6576" width="0.1524" layer="20"/>
<wire x1="32.3088" y1="76.5048" x2="32.3088" y2="74.5236" width="0.1524" layer="20"/>
<wire x1="32.3088" y1="74.5236" x2="32.3088" y2="72.0852" width="0.1524" layer="20"/>
<wire x1="13.716" y1="70.866" x2="13.716" y2="21.336" width="0.1524" layer="20"/>
<wire x1="32.3088" y1="21.336" x2="32.3088" y2="72.0852" width="0.1524" layer="20"/>
<wire x1="13.716" y1="73.6092" x2="13.716" y2="71.7804" width="0.1524" layer="20"/>
<wire x1="0" y1="7.62" x2="10.8204" y2="18.4404" width="0.1524" layer="20"/>
<wire x1="46.0248" y1="7.62" x2="35.2044" y2="18.4404" width="0.1524" layer="20"/>
<wire x1="10.8204" y1="18.4404" x2="13.716" y2="21.336" width="0.1524" layer="20"/>
<wire x1="35.2044" y1="18.4404" x2="32.3088" y2="21.336" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="con-hirose">
<packages>
<package name="FH19C-30S-0.5SH(05)">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X17">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="P1" library="con-hirose" package="FH19C-30S-0.5SH(05)" value="FC19C-30S-0.5SH(05)"/>
<element name="JP1" library="pinhead" package="2X17" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="P1" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="P1" pad="3"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="P1" pad="4"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="P1" pad="5"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="P1" pad="7"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="P1" pad="8"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="P1" pad="9"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="N$12">
<contactref element="P1" pad="12"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="N$13">
<contactref element="P1" pad="13"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="N$14">
<contactref element="P1" pad="14"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="N$17">
<contactref element="P1" pad="17"/>
<contactref element="JP1" pad="17"/>
</signal>
<signal name="N$18">
<contactref element="P1" pad="18"/>
<contactref element="JP1" pad="18"/>
</signal>
<signal name="N$19">
<contactref element="P1" pad="19"/>
<contactref element="JP1" pad="19"/>
</signal>
<signal name="N$22">
<contactref element="P1" pad="22"/>
<contactref element="JP1" pad="20"/>
</signal>
<signal name="N$23">
<contactref element="P1" pad="23"/>
<contactref element="JP1" pad="21"/>
</signal>
<signal name="N$24">
<contactref element="P1" pad="24"/>
<contactref element="JP1" pad="22"/>
</signal>
<signal name="N$26">
<contactref element="P1" pad="26"/>
<contactref element="JP1" pad="23"/>
</signal>
<signal name="N$27">
<contactref element="P1" pad="27"/>
<contactref element="JP1" pad="24"/>
</signal>
<signal name="N$28">
<contactref element="P1" pad="28"/>
<contactref element="JP1" pad="25"/>
</signal>
<signal name="N$29">
<contactref element="P1" pad="29"/>
<contactref element="JP1" pad="26"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
