<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>160921</text>
<wire x1="0.635" y1="16.129" x2="0.635" y2="8.255" width="0.127" layer="20"/>
<wire x1="0.635" y1="8.255" x2="4.572" y2="8.255" width="0.127" layer="20"/>
<wire x1="0.635" y1="16.129" x2="4.572" y2="16.129" width="0.127" layer="20"/>
<wire x1="30.353" y1="16.129" x2="30.353" y2="8.255" width="0.127" layer="20"/>
<wire x1="30.353" y1="8.255" x2="26.289" y2="8.255" width="0.127" layer="20"/>
<wire x1="30.353" y1="16.129" x2="26.289" y2="16.129" width="0.127" layer="20"/>
<wire x1="23.368" y1="20.701" x2="7.493" y2="20.701" width="0.127" layer="20"/>
<wire x1="7.493" y1="3.683" x2="23.368" y2="3.683" width="0.127" layer="20"/>
<wire x1="7.493" y1="3.683" x2="4.572" y2="8.255" width="0.127" layer="20" curve="-30"/>
<wire x1="4.572" y1="16.129" x2="7.493" y2="20.701" width="0.127" layer="20" curve="-30"/>
<wire x1="23.368" y1="20.701" x2="26.289" y2="16.129" width="0.127" layer="20" curve="-30"/>
<wire x1="26.289" y1="8.255" x2="23.368" y2="3.683" width="0.127" layer="20" curve="-30"/>
<text>SPRINGSWITCHBLINK</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="my library">
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
<package name="PLCC4">
</package>
<package name="NOSS_AVR-ISP-6">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 6 Pin, 0.1" Straight</description>
</package>
</packages>
</library>
<library name="Pinoccio">
<description>Pinoccio Board Devices</description>
<packages>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="spring_switch">
<packages>
<package name="SW-18020P-RA">
</package>
</packages>
</library>
<library name="battery_holders">
<packages>
<package name="BU2032-1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CB1" library="SparkFun-Capacitors" package="0603-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RST" library="Pinoccio" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="my library" package="SO08-EIAJ" value="ATTINY85">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="BATT1" library="battery_holders" package="BU2032-1" value="20MM_HOLDERBU2032-1"/>
<element name="S1" library="spring_switch" package="SW-18020P-RA" value="SPRING_SWITCH">
<attribute name="NAME"/>
</element>
<element name="RB" library="SparkFun-Resistors" package="0603-RES" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RG" library="SparkFun-Resistors" package="0603-RES" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RR" library="SparkFun-Resistors" package="0603-RES" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="my library" package="PLCC4" value="LED-RGBPLCC4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISP" library="my library" package="NOSS_AVR-ISP-6" value="MYISP-AVR-ISP-6VERT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="RST" pad="1"/>
<contactref element="CB1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="BATT1" pad="-"/>
<contactref element="ISP" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="8"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="CB1" pad="1"/>
<contactref element="BATT1" pad="+@1"/>
<contactref element="BATT1" pad="+@2"/>
<contactref element="ISP" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="R3" pad="2"/>
<contactref element="RST" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="ISP" pad="5"/>
</signal>
<signal name="MOSI/LED_B">
<contactref element="U1" pad="5"/>
<contactref element="RB" pad="2"/>
<contactref element="ISP" pad="4"/>
</signal>
<signal name="MISO/LED_G">
<contactref element="U1" pad="6"/>
<contactref element="RG" pad="2"/>
<contactref element="ISP" pad="1"/>
</signal>
<signal name="SCK/SWITCH">
<contactref element="U1" pad="7"/>
<contactref element="R1" pad="2"/>
<contactref element="S1" pad="P$2"/>
<contactref element="ISP" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="S1" pad="P$1"/>
</signal>
<signal name="LED_R">
<contactref element="U1" pad="3"/>
<contactref element="RR" pad="2"/>
</signal>
<signal name="LED_RETURN">
<contactref element="U1" pad="2"/>
<contactref element="D1" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="RR" pad="1"/>
<contactref element="D1" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="RG" pad="1"/>
<contactref element="D1" pad="P$4"/>
</signal>
<signal name="N$5">
<contactref element="RB" pad="1"/>
<contactref element="D1" pad="P$3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
