<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="44.45" y2="0" width="0" layer="20"/>
<wire x1="44.45" y1="0" x2="44.45" y2="17.78" width="0" layer="20"/>
<wire x1="44.45" y1="17.78" x2="0" y2="17.77" width="0" layer="20"/>
<wire x1="0" y1="17.77" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_MINI">
</package>
</packages>
</library>
<library name="stepOSP">
<packages>
<package name="STEPS_CRYSTAL">
</package>
<package name="QFN28-ML_6X6MM">
<description>&lt;b&gt;QFN28-ML_6X6MM&lt;/b&gt;&lt;p&gt;
Source: http://www.microchip.com .. 39637a.pdf</description>
</package>
<package name="TC2030-IDC-NL-TOP">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="PAD-JUMPER-2-NO_YES_SILK">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="FIDUCIAL-1X2">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_12MM_PTH">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="stepOSP" package="STEPS_CRYSTAL" value="STEPS_BACKUP_XTAL">
<attribute name="NAME"/>
</element>
<element name="U$9" library="SparkFun-Boards" package="ARDUINO_MINI" value="ARDUINO_MINI"/>
<element name="U2" library="stepOSP" package="QFN28-ML_6X6MM" value="PIC24FJ64GA002">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Passives" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Passives" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FID1" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FID2" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="J1" library="stepOSP" package="TC2030-IDC-NL-TOP" value="TC2030-MCP-NL-TOP">
<attribute name="NAME"/>
</element>
<element name="U1" library="stepOSP" package="SOT23-5" value="TPS709XX">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Passives" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BAT1" library="SparkFun-Electromechanical" package="BATTCON_12MM_PTH" value="">
<attribute name="VALUE"/>
</element>
<element name="FID3" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="J2" library="SparkFun-Connectors" package="JST-2-SMD" value="">
<attribute name="PROD_ID" value="CONN-08352"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_YES_SILK" value="JUMPER-PAD-2-NOYES_SILK"/>
<element name="SJ2" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK" value="JUMPER-PAD-2-NC_BY_TRACE"/>
<element name="R5" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="MCLR">
<contactref element="U2" pad="26"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="RB0">
<contactref element="U$9" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="RB1">
<contactref element="U$9" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="RB2">
<contactref element="U$9" pad="5"/>
<contactref element="U2" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="RB3">
<contactref element="U$9" pad="6"/>
<contactref element="U2" pad="4"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="RB15">
<contactref element="U$9" pad="18"/>
<contactref element="U2" pad="23"/>
</signal>
<signal name="RB14">
<contactref element="U$9" pad="17"/>
<contactref element="U2" pad="22"/>
</signal>
<signal name="RB13">
<contactref element="U$9" pad="16"/>
<contactref element="U2" pad="21"/>
</signal>
<signal name="RB11">
<contactref element="U$9" pad="15"/>
<contactref element="U2" pad="19"/>
</signal>
<signal name="RB10">
<contactref element="U$9" pad="14"/>
<contactref element="U2" pad="18"/>
</signal>
<signal name="RA2">
<contactref element="U$9" pad="7"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="RA3">
<contactref element="U$9" pad="8"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="RB5">
<contactref element="U$9" pad="9"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="RB6">
<contactref element="U$9" pad="10"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="RB7">
<contactref element="U$9" pad="11"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="RB8">
<contactref element="U$9" pad="12"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="RB9">
<contactref element="U$9" pad="13"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="RA1">
<contactref element="U$9" pad="20"/>
<contactref element="U2" pad="28"/>
</signal>
<signal name="RA0">
<contactref element="U$9" pad="19"/>
<contactref element="U2" pad="27"/>
</signal>
<signal name="RB12">
<contactref element="U2" pad="20"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$5">
<contactref element="U2" pad="17"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="RST">
<contactref element="U$9" pad="22"/>
<contactref element="C8" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="U$9" pad="24"/>
<contactref element="U1" pad="1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="J1" pad="3"/>
<contactref element="C5" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U$9" pad="4"/>
<contactref element="U1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U2" pad="24"/>
<contactref element="U2" pad="5"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U$9" pad="23"/>
<contactref element="BAT1" pad="GND"/>
<contactref element="J2" pad="1"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="2.5V">
<contactref element="U$9" pad="21"/>
<contactref element="R2" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="U2" pad="25"/>
<contactref element="C4" pad="1"/>
<contactref element="U2" pad="10"/>
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="SOSCI">
<contactref element="U2" pad="8"/>
<contactref element="X1" pad="P$2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="SOSCO">
<contactref element="U2" pad="9"/>
<contactref element="X1" pad="P$1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="16"/>
<contactref element="BAT1" pad="VCC@1"/>
<contactref element="SJ1" pad="2"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="2"/>
<contactref element="SJ2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
