<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="59.69" x2="0" y2="0" width="0.4064" layer="20"/>
<wire x1="0" y1="0" x2="38.1" y2="0" width="0.4064" layer="20"/>
<wire x1="38.1" y1="0" x2="38.1" y2="59.69" width="0.4064" layer="20"/>
<wire x1="38.1" y1="59.69" x2="0" y2="59.69" width="0.4064" layer="20"/>
<hole x="36.068" y="43.18" drill="2.8"/>
<hole x="20.32" y="43.18" drill="2.8"/>
<hole x="36.068" y="57.15" drill="2.8"/>
<hole x="20.32" y="57.15" drill="2.8"/>
<hole x="2.54" y="57.15" drill="2.8"/>
<hole x="2.54" y="2.54" drill="2.8"/>
<hole x="35.56" y="2.54" drill="2.8"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
</package>
<package name="1X04_NO_SILK">
</package>
<package name="1X03_NO_SILK">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="JST-PH-2-THM">
<description>4UCon #01528
http://www.4uconnector.com/online/object/4udrawing/01528.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="MoteinoR4Mod">
<packages>
<package name="MOTEINTO_R4_SQ">
<description>&lt;b&gt;Footprint for Moteino R4 Module using 0.025" Square Post Pins&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LCK" library="adafruit" package="JST-PH-2-THM" value=""/>
<element name="BUTTON" library="adafruit" package="JST-PH-2-THM" value=""/>
<element name="SPKR" library="adafruit" package="JST-PH-2-THM" value=""/>
<element name="PWRSW" library="adafruit" package="JST-PH-2-THM" value=""/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.4" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.4" value="3.3K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="MoteinoR4Mod" package="MOTEINTO_R4_SQ" value="MOTEINO_R4_MODULEUSING_SQ_POST_PINS"/>
<element name="OLED" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CHRGR" library="SparkFun-Connectors" package="1X04_NO_SILK" value=""/>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.4" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POT" library="SparkFun-Connectors" package="1X03_NO_SILK" value=""/>
<element name="SDAPULLUP" library="SparkFun-Resistors" package="AXIAL-0.4" value="3.3K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SCLPULLUP" library="SparkFun-Resistors" package="AXIAL-0.4" value="3.3K"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="G2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="LCK" pad="1"/>
<contactref element="SPKR" pad="1"/>
<contactref element="BUTTON" pad="1"/>
<contactref element="CHRGR" pad="2"/>
<contactref element="OLED" pad="4"/>
</signal>
<signal name="PWR">
<contactref element="R1" pad="P$1"/>
<contactref element="PWRSW" pad="2"/>
<contactref element="OLED" pad="6"/>
<contactref element="U$1" pad="PWR"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="P$1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="U$1" pad="A0"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="D4"/>
<contactref element="BUTTON" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="LCK" pad="2"/>
<contactref element="U$1" pad="D3"/>
</signal>
<signal name="BATT_+">
<contactref element="PWRSW" pad="1"/>
<contactref element="CHRGR" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="OLED" pad="1"/>
<contactref element="U$1" pad="A4"/>
<contactref element="SDAPULLUP" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="OLED" pad="2"/>
<contactref element="U$1" pad="A5"/>
<contactref element="SCLPULLUP" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="D5"/>
<contactref element="POT" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="POT" pad="2"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="P$2"/>
<contactref element="SPKR" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="SCLPULLUP" pad="P$2"/>
<contactref element="U$1" pad="3.3V"/>
<contactref element="SDAPULLUP" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="OLED" pad="3"/>
<contactref element="U$1" pad="D6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
