<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="60.96" x2="31.75" y2="60.96" width="0" layer="20"/>
<wire x1="31.75" y1="60.96" x2="31.75" y2="80" width="0" layer="20"/>
<wire x1="31.75" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="60.96" width="0" layer="20"/>
<hole x="27.94" y="64.76" drill="3.2"/>
<text>Pentawatt IC
Audio Amplifier</text>
<text>TEST BOARD</text>
<text>TJP 6/2014</text>
</plain>
<libraries>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="L200S">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="SCREWTERMINAL-5MM-3">
</package>
</packages>
</library>
<library name="solpad">
<description>&lt;b&gt;Solder Pads/Test Points&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LSP11">
<description>&lt;b&gt;SOLDER PAD&lt;/b&gt;&lt;p&gt;
drill 1.1 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PENTAWATT" library="v-reg" package="L200S" value="">
<attribute name="VALUE"/>
</element>
<element name="VCC" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="M025MM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AUDIO" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AUD+" library="solpad" package="LSP11" value="LSP11">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AUD-" library="solpad" package="LSP11" value="LSP11">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VCC-" library="solpad" package="LSP11" value="LSP11">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT" library="solpad" package="LSP11" value="LSP11">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VCC+" library="solpad" package="LSP11" value="LSP11">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="PENTAWATT" pad="5"/>
<contactref element="VCC+" pad="MP"/>
<contactref element="VCC" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="PENTAWATT" pad="3"/>
<contactref element="VCC-" pad="MP"/>
<contactref element="VCC" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="PENTAWATT" pad="1"/>
<contactref element="AUD+" pad="MP"/>
<contactref element="AUDIO" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="PENTAWATT" pad="2"/>
<contactref element="AUD-" pad="MP"/>
<contactref element="AUDIO" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="PENTAWATT" pad="4"/>
<contactref element="OUT" pad="MP"/>
<contactref element="AUDIO" pad="3"/>
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$14">
</signal>
<signal name="N$13">
</signal>
<signal name="N$15">
</signal>
<signal name="N$16">
</signal>
</signals>
</board>
</drawing>
</eagle>
