<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<board>
<plain>
<wire x1="0.9525" y1="0" x2="40.945" y2="0" width="0" layer="20"/>
<wire x1="40.945" y1="0" x2="40.945" y2="34.915" width="0" layer="20"/>
<wire x1="40.945" y1="34.915" x2="0.9525" y2="34.915" width="0" layer="20"/>
<wire x1="0.9525" y1="34.915" x2="0.9525" y2="0" width="0" layer="20"/>
<text>Watchia v1.1</text>
<text>Designed by</text>
<text>Andrew Cassidy</text>
<text>MicroSD Card 
    Slot</text>
<text>BTLE</text>
<text>Buttons</text>
<text>Batt</text>
<text>+</text>
<text>-</text>
<text>ML414 
batt</text>
<text>Watchia</text>
<text>Micro
 USB</text>
<text>Atmega
328p</text>
<text>programmer</text>
<text>GND</text>
<text>FT231X</text>
<text>Prog. Status</text>
<text>ON</text>
<text>OFF</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MICROB">
<description>Micro USB Package</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT143">
<description>&lt;h3&gt;SOT143&lt;/h3&gt;
Package is used for the STM811 (also APX811)&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Proven&lt;/b&gt;</description>
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="SSOP20_L">
<description>Longer version of SSOP-20 Package</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-32KHZ-SMD">
</package>
</packages>
</library>
<library name="Texas Instruments_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:45:58</description>
<packages>
<package name="SOT95P280X145-5N">
</package>
<package name="SOIC127P600X175-8N">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="lph-7366">
<description>&lt;b&gt;LPH-7366: PCD8544-based Nokia 5110 monochrome LCD display&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="LPH-7366">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH-SPST-SMD-A">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="con-jst2">
<description>&lt;b&gt;J.S.T. Connectors&lt;/b&gt;&lt;p&gt;
J.S.T Mfg Co.,Ltd.&lt;p&gt;
http://www.jst-mfg.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SM02B-SRSS-TB">
<description>&lt;b&gt;Shrouded Header, side entry type&lt;/b&gt;</description>
</package>
<package name="SM06B-SRSS-TB">
<description>&lt;b&gt;Shrouded Header, side entry type&lt;/b&gt;</description>
</package>
<package name="SM05B-SRSS-TB">
<description>&lt;b&gt;Shrouded Header, side entry type&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ML414">
<packages>
<package name="BK-414-TR">
</package>
</packages>
</library>
<library name="NXP_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 14:27:46</description>
<packages>
<package name="SOT65P210X110-6N">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-L">
</package>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
<library name="hrs_DM3D-SF">
<packages>
<package name="DM3D">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP2" library="SparkFun-Connectors" package="USB-MICROB" value="USB-MICROB">
<attribute name="PROD_ID" value="CONN-09505"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="CRYSTAL-32KHZ-SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PROD_ID" value="XTAL-07894"/>
</element>
<element name="U1" library="Texas Instruments_By_element14_Batch_1" package="SOT95P280X145-5N" value="LP2985A-10DBVR">
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="OC_NEWARK" value="24R9590"/>
<attribute name="MPN" value="LP2985A-10DBVR"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="OC_FARNELL" value="-"/>
</element>
<element name="U2" library="SparkFun-DigitalIC" package="SOT143" value="STM811">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="30V, 2.5A">
<attribute name="PROD_ID" value="TRANS-11308"/>
<attribute name="VALUE" value="30V, 2.5A"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P">
<attribute name="PROD_ID" value="IC-09069"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="47kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LCD1" library="lph-7366" package="LPH-7366" value="LPH-7366">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="Texas Instruments_By_element14_Batch_1" package="SOIC127P600X175-8N" value="BQ32000DR">
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="OC_NEWARK" value="24R9067"/>
<attribute name="MPN" value="BQ32000DR"/>
<attribute name="SUPPLIER" value="TEXAS INSTRUMENTS"/>
<attribute name="OC_FARNELL" value="1754773"/>
</element>
<element name="U5" library="SparkFun-PowerIC" package="SOT23-5" value="MAX1555">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="SWITCH-SPST-SMD-A" value=""/>
<element name="C1" library="SparkFun-Passives" package="0603-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="SparkFun-DigitalIC" package="SSOP20_L" value="FTS31XS-U">
<attribute name="PROD_ID" value="IC-11524"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Passives" package="0603-CAP" value="47pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Passives" package="0603-CAP" value="47pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun-LED" package="LED-0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="LED3" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="LED4" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="R5" library="SparkFun-Passives" package="0603-RES" value="47kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="0603-RES" value="47kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Passives" package="0603-CAP" value="1µF"/>
<element name="C9" library="SparkFun-Passives" package="0603-CAP" value="1µF"/>
<element name="LED5" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="R7" library="SparkFun-Passives" package="0603-RES" value="330Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-jst2" package="SM02B-SRSS-TB" value="SM02B-SRSS-TB"/>
<element name="X4" library="con-jst2" package="SM06B-SRSS-TB" value="SM06B-SRSS-TB"/>
<element name="U$1" library="ML414" package="BK-414-TR" value="ML414"/>
<element name="X2" library="con-jst2" package="SM05B-SRSS-TB" value="SM05B-SRSS-TB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U8" library="NXP_By_element14_Batch_1" package="SOT65P210X110-6N" value="BSS84AKS">
<attribute name="PACKAGE" value="SOT-363-6"/>
<attribute name="OC_NEWARK" value="58T9005"/>
<attribute name="MPN" value="BSS84AKS"/>
<attribute name="SUPPLIER" value="NXP"/>
<attribute name="OC_FARNELL" value="1972665"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-L" value="OSHW-LOGOL"/>
<element name="LOGO2" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="U$2" library="hrs_DM3D-SF" package="DM3D" value="MICROSD-HRS_DM3D">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="5"/>
<contactref element="JP2" pad="MT2"/>
<contactref element="JP2" pad="GND"/>
<contactref element="JP2" pad="MT1"/>
<contactref element="U4" pad="4"/>
<contactref element="U5" pad="2"/>
<contactref element="LCD1" pad="7"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="LED5" pad="C"/>
<contactref element="X1" pad="2"/>
<contactref element="X4" pad="1"/>
<contactref element="U3" pad="21"/>
<contactref element="U$1" pad="GND"/>
<contactref element="X2" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="C6" pad="2"/>
<contactref element="U6" pad="6"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U8" pad="5"/>
<contactref element="U8" pad="2"/>
<contactref element="U$2" pad="GND1"/>
<contactref element="U$2" pad="GND2"/>
<contactref element="U$2" pad="GND3"/>
<contactref element="U$2" pad="GND4"/>
<contactref element="U$2" pad="VSS"/>
</signal>
<signal name="N$2">
<contactref element="U4" pad="1"/>
<contactref element="Y1" pad="X2"/>
</signal>
<signal name="5V">
<contactref element="C1" pad="1"/>
<contactref element="U6" pad="15"/>
<contactref element="U5" pad="1"/>
<contactref element="JP2" pad="VBUS"/>
<contactref element="U8" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="5"/>
<contactref element="U3" pad="4"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="18"/>
<contactref element="U3" pad="20"/>
<contactref element="R1" pad="2"/>
<contactref element="U4" pad="8"/>
<contactref element="LCD1" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="U6" pad="3"/>
<contactref element="X2" pad="1"/>
<contactref element="U$2" pad="VDD"/>
</signal>
<signal name="N$13">
<contactref element="U2" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="V_BATT">
<contactref element="U2" pad="4"/>
<contactref element="Q2" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="U5" pad="5"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U4" pad="3"/>
<contactref element="U$1" pad="+@2"/>
<contactref element="U$1" pad="+"/>
</signal>
<signal name="N$5">
<contactref element="Y1" pad="X1"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="JP2" pad="D-"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="C4" pad="1"/>
<contactref element="U6" pad="13"/>
<contactref element="U6" pad="14"/>
</signal>
<signal name="N$1">
<contactref element="JP2" pad="D+"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R2" pad="1"/>
<contactref element="U6" pad="11"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U6" pad="12"/>
<contactref element="R4" pad="1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="RX">
<contactref element="U3" pad="30"/>
<contactref element="U6" pad="20"/>
</signal>
<signal name="TX">
<contactref element="U3" pad="31"/>
<contactref element="U6" pad="4"/>
</signal>
<signal name="RST">
<contactref element="U6" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U3" pad="29"/>
</signal>
<signal name="SCLK">
<contactref element="U3" pad="17"/>
<contactref element="LCD1" pad="2"/>
<contactref element="U$2" pad="CLK"/>
</signal>
<signal name="MOSI">
<contactref element="U3" pad="15"/>
<contactref element="LCD1" pad="3"/>
<contactref element="U$2" pad="CMD"/>
</signal>
<signal name="D/C">
<contactref element="LCD1" pad="4"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="RES">
<contactref element="LCD1" pad="9"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="SCE">
<contactref element="LCD1" pad="5"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="N$14">
<contactref element="Q2" pad="3"/>
<contactref element="U8" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="U3" pad="16"/>
<contactref element="U$2" pad="DAT0"/>
</signal>
<signal name="CS">
<contactref element="U3" pad="14"/>
<contactref element="U$2" pad="CD/DAT3"/>
</signal>
<signal name="SDA">
<contactref element="U4" pad="5"/>
<contactref element="U3" pad="27"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U4" pad="6"/>
<contactref element="U3" pad="28"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="LED5" pad="A"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R7" pad="2"/>
<contactref element="U6" pad="18"/>
</signal>
<signal name="B_UP">
<contactref element="X4" pad="2"/>
<contactref element="U3" pad="12"/>
</signal>
<signal name="B_DOWN">
<contactref element="X4" pad="3"/>
<contactref element="U3" pad="13"/>
</signal>
<signal name="B_LEFT">
<contactref element="X4" pad="4"/>
<contactref element="U3" pad="23"/>
</signal>
<signal name="B_RIGHT">
<contactref element="X4" pad="5"/>
<contactref element="U3" pad="24"/>
</signal>
<signal name="B_SELECT">
<contactref element="X4" pad="6"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="IRQ">
<contactref element="U4" pad="7"/>
<contactref element="U3" pad="32"/>
</signal>
<signal name="KEY">
<contactref element="U3" pad="7"/>
<contactref element="X2" pad="5"/>
</signal>
<signal name="LED">
<contactref element="LED1" pad="A"/>
<contactref element="LED4" pad="A"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="U3" pad="19"/>
</signal>
<signal name="BT_TX">
<contactref element="U3" pad="10"/>
<contactref element="X2" pad="4"/>
</signal>
<signal name="BT_RX">
<contactref element="U3" pad="11"/>
<contactref element="X2" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="S1" pad="2"/>
<contactref element="U8" pad="4"/>
<contactref element="U8" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
