<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="9.365" x2="0" y2="0.635" width="0" layer="20"/>
<wire x1="0" y1="0.635" x2="0.635" y2="0" width="0" layer="20" curve="90"/>
<wire x1="0.635" y1="0" x2="27.865" y2="0" width="0" layer="20"/>
<wire x1="27.865" y1="0" x2="28.5" y2="0.635" width="0" layer="20" curve="90"/>
<wire x1="28.5" y1="0.635" x2="28.5" y2="9.365" width="0" layer="20"/>
<wire x1="28.5" y1="9.365" x2="27.865" y2="10" width="0" layer="20" curve="90"/>
<wire x1="27.865" y1="10" x2="0.635" y2="10" width="0" layer="20"/>
<wire x1="0.635" y1="10" x2="0" y2="9.365" width="0" layer="20" curve="90"/>
<text>G</text>
<text>+</text>
<text>S</text>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_LOCK">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="00_PERSONAL">
<packages>
<package name="3X1.75">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="adafruit" package="M0805" value=""/>
<element name="U$1" library="SparkFun" package="SO08-EIAJ" value="ATTINY85">
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0805K" value=""/>
<element name="J1" library="SparkFun-Connectors" package="2X3_LOCK" value="AVR_SPI_PRG_62X3_LOCK"/>
<element name="U$2" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$3" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$4" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$5" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$6" library="00_PERSONAL" package="3X1.75" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="U$6" pad="P$1"/>
</signal>
<signal name="+5V">
<contactref element="U$1" pad="8"/>
<contactref element="R1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="WS2812">
<contactref element="U$1" pad="2"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="RST">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="3R">
<contactref element="U$1" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="7"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="6"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="5"/>
<contactref element="J1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
