<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="-1.27" x2="27.4755" y2="-1.27" width="0.254" layer="20"/>
<wire x1="27.4755" y1="-1.27" x2="27.4755" y2="30.0865" width="0.254" layer="20"/>
<wire x1="27.4755" y1="30.0865" x2="0" y2="30.0865" width="0.254" layer="20"/>
<wire x1="0" y1="30.0865" x2="0" y2="-1.27" width="0.254" layer="20"/>
<text>#cougballoon</text>
<text>HackHD Interface 
Board v1.5</text>
<text>becca was here! :)</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ45-8">
</package>
<package name="RCA">
</package>
<package name="1X09_LOCK">
</package>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALLEZ">
<description>This is the "EZ" version of the .1" spaced ceramic thru-hole cap.&lt;br&gt;
It has reduced top mask to make it harder to put the component on the wrong side of the board.</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="COMM" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="VIDEO_OUT" library="SparkFun-Connectors" package="RCA" value="RCA">
<attribute name="OC_NEWARK" value="65K7770"/>
<attribute name="MF" value="SWITCHCRAFT"/>
<attribute name="MPN" value="PJRAN1X1U01X"/>
</element>
<element name="HACKHD" library="SparkFun-Connectors" package="1X09_LOCK" value="M09LOCK">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="BATT" library="SparkFun-Connectors" package="JST-2-SMD" value="">
<attribute name="PROD_ID" value="CONN-08352"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="OC_NEWARK" value="38K0328"/>
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="MCF 0.25W 10K"/>
</element>
<element name="U1" library="SparkFun-PowerIC" package="SOT23-5" value="MCP73831">
<attribute name="PROD_ID" value="IC-09995"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="84R6271"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCP73831T-2DCI/OT"/>
</element>
<element name="C1" library="SparkFun-Passives" package="CAP-PTH-SMALLEZ" value="4.7uF">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="C2" library="SparkFun-Passives" package="CAP-PTH-SMALLEZ" value="4.7uF">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="38K0363"/>
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="MCF 0.25W 330R"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="2k">
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="58K3823"/>
<attribute name="MF" value="Multicomp Passives"/>
<attribute name="MPN" value="MCMF0W4FF2001A50"/>
</element>
<element name="CHARGE" library="adafruit" package="LED3MM" value="YELLOW">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="06F6576"/>
<attribute name="MF" value="AGILENT TECHNOLOGIES"/>
<attribute name="MPN" value="HLMP-1401"/>
</element>
<element name="RECORD" library="adafruit" package="LED3MM" value="RED">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="16M1519"/>
<attribute name="MF" value="SLI (CML/IDI)"/>
<attribute name="MPN" value="4303F1"/>
</element>
</elements>
<signals>
<signal name="SIGNAL">
<contactref element="COMM" pad="2"/>
<contactref element="HACKHD" pad="7"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="VIDEO_OUT">
<contactref element="HACKHD" pad="6"/>
<contactref element="VIDEO_OUT" pad="PIN"/>
<contactref element="COMM" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="2"/>
<contactref element="CHARGE" pad="A"/>
</signal>
<signal name="VIN">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="R3" pad="1"/>
<contactref element="COMM" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="CHARGE" pad="K"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="5"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="HACKHD" pad="2"/>
<contactref element="BATT" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="HACKHD" pad="5"/>
<contactref element="HACKHD" pad="9"/>
<contactref element="BATT" pad="1"/>
<contactref element="HACKHD" pad="1"/>
<contactref element="COMM" pad="8"/>
<contactref element="RECORD" pad="K"/>
<contactref element="VIDEO_OUT" pad="SHELL"/>
</signal>
<signal name="N$12">
<contactref element="RECORD" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="CONTROL">
<contactref element="HACKHD" pad="3"/>
<contactref element="COMM" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
