<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<circle x="2.75" y="33.25" radius="1.5" width="0.1" layer="20"/>
<wire x1="0" y1="33.87868125" x2="0" y2="2.12131875" width="0.1" layer="20"/>
<wire x1="0" y1="2.12131875" x2="2.12131875" y2="0" width="0.1" layer="20" curve="90"/>
<wire x1="2.12131875" y1="0" x2="33.87868125" y2="0" width="0.1" layer="20"/>
<wire x1="33.87868125" y1="0" x2="36" y2="2.12131875" width="0.1" layer="20" curve="90"/>
<wire x1="36" y1="2.12131875" x2="36" y2="33.763934375" width="0.1" layer="20"/>
<wire x1="36" y1="33.763934375" x2="33.763934375" y2="36" width="0.1" layer="20" curve="90"/>
<wire x1="33.763934375" y1="36" x2="2.12131875" y2="36" width="0.1" layer="20"/>
<wire x1="2.12131875" y1="36" x2="0" y2="33.87868125" width="0.1" layer="20" curve="90"/>
<circle x="2.75" y="2.75" radius="1.5" width="0.1" layer="20"/>
<circle x="33.25" y="2.75" radius="1.5" width="0.1" layer="20"/>
<circle x="28.97" y="33.035" radius="0.75" width="0.1" layer="20"/>
<circle x="5.97" y="33.035" radius="0.75" width="0.1" layer="20"/>
<text>3.3V</text>
<text>5V in</text>
<text>GND</text>
<text>PWM</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>PPM In</text>
<text>Ed Lafargue 2015
CC-BY-SA</text>
<text>TX1</text>
<text>RX1</text>
<text>Ch1</text>
<text>Ch5</text>
<circle x="33.25" y="33.25" radius="1.5" width="0.1" layer="20"/>
<text>www.aerodynes.org</text>
<text>Gemini Adapter v1.0</text>
</plain>
<libraries>
<library name="con-amp-micromatch">
<description>AMP Connectors, Type  MicroMatch</description>
<packages>
<package name="MICROMATCH-16">
<description>&lt;b&gt;MicroMaTch 16 &lt;/b&gt; 8-215464-6 / 1-215464-6&lt;p&gt;
Drawing Number C-215464&lt;br&gt;
DDEController.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
</package>
<package name="1X03">
</package>
<package name="1X02">
</package>
<package name="1X05">
</package>
</packages>
</library>
<library name="aerodynes">
<description>My own parts list for Aerodynes projects.</description>
<packages>
<package name="LOGO-AERODYNES-S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="con-amp-micromatch" package="MICROMATCH-16" value="MICROMATCH-16">
<attribute name="OC_NEWARK" value="26H3309"/>
<attribute name="MPN" value="8-215464-6"/>
<attribute name="MF" value="FARNELL"/>
<attribute name="OC_FARNELL" value="3784680"/>
</element>
<element name="X2" library="con-amp-micromatch" package="MICROMATCH-16" value="MICROMATCH-16">
<attribute name="OC_NEWARK" value="26H3309"/>
<attribute name="MPN" value="8-215464-6"/>
<attribute name="MF" value="FARNELL"/>
<attribute name="OC_FARNELL" value="3784680"/>
</element>
<element name="JP1" library="SparkFun" package="1X06" value=""/>
<element name="JP2" library="SparkFun" package="1X03" value=""/>
<element name="JP3" library="SparkFun" package="1X02" value=""/>
<element name="JP4" library="SparkFun" package="1X03" value=""/>
<element name="U$1" library="aerodynes" package="LOGO-AERODYNES-S" value="LOGO-AERODYNESSMALL"/>
<element name="JP5" library="SparkFun" package="1X02" value=""/>
<element name="JP6" library="SparkFun" package="1X05" value=""/>
</elements>
<signals>
<signal name="PWMIN1">
<contactref element="X1" pad="1"/>
<contactref element="JP6" pad="5"/>
</signal>
<signal name="PWMIN2">
<contactref element="X1" pad="2"/>
<contactref element="JP6" pad="4"/>
</signal>
<signal name="PWMIN3">
<contactref element="X1" pad="3"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="PWMIN4">
<contactref element="X1" pad="4"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="PWMIN5">
<contactref element="X1" pad="5"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="PWMIN6">
<contactref element="X1" pad="6"/>
</signal>
<signal name="PWMIN7">
<contactref element="X1" pad="7"/>
</signal>
<signal name="PWMIN8">
<contactref element="X1" pad="8"/>
</signal>
<signal name="TX1">
<contactref element="X1" pad="9"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="RX1">
<contactref element="X1" pad="10"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="SWDIO">
<contactref element="X1" pad="11"/>
</signal>
<signal name="SWCLK">
<contactref element="X1" pad="12"/>
</signal>
<signal name="VCCEXT">
<contactref element="X1" pad="13"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="X1" pad="14"/>
</signal>
<signal name="GND">
<contactref element="X1" pad="15"/>
<contactref element="X2" pad="16"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="+VB">
<contactref element="X1" pad="16"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="PWM1">
<contactref element="X2" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="PWM2">
<contactref element="X2" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="PWM3">
<contactref element="X2" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="PWM4">
<contactref element="X2" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="PWM5">
<contactref element="X2" pad="5"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="PWM6">
<contactref element="X2" pad="6"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="PWM7">
<contactref element="X2" pad="7"/>
</signal>
<signal name="PWM8">
<contactref element="X2" pad="8"/>
</signal>
<signal name="TX2">
<contactref element="X2" pad="9"/>
</signal>
<signal name="RX2_S.BUS">
<contactref element="X2" pad="10"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="TX3">
<contactref element="X2" pad="11"/>
</signal>
<signal name="RX3">
<contactref element="X2" pad="12"/>
</signal>
<signal name="+5V_USB">
<contactref element="X2" pad="13"/>
</signal>
<signal name="D+">
<contactref element="X2" pad="14"/>
</signal>
<signal name="D-">
<contactref element="X2" pad="15"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
